{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":17,"n_cols":13,"rows_kept":17,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["陕西长青能源化工有限公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","无税单价（元）","总价（元）","品牌","备注"]
["1","TM202112181059565366593","便携式气体分析仪（HCL）","内置泵吸式测量，显示方式，2.5 寸 320*240 高清彩屏显示 典型精度：≤±2% FS12.线性度，≤±1% 13.重复性？≤±1% 报警方式，声光+振动+视觉报警15. 工作电源，充电式锂电池，电池容量;3.6VDC，5500mA大容量可充电电池 使用环境，温度-40℃~+70℃； 相对湿度≤0-99%RH 数据存储量：10万条数据容量存储时间间隔设置 防爆等级？Exia II CT4 防护等级 IP66 执行标准：GB 15322.3-2019","附参数表","块","1.00","","","","","","气化应急照明改造"]
["2","TM20211218105956537b4ba","便携式气体分析仪（N2H4）","内置泵吸式测量，显示方式，2.5 寸 320*240 高清彩屏显示 典型精度：≤±2% FS12.线性度，≤±1% 13.重复性？≤±1% 报警方式，声光+振动+视觉报警15. 工作电源，充电式锂电池，电池容量;3.6VDC，5500mA大容量可充电电池 使用环境，温度-40℃~+70℃； 相对湿度≤0-99%RH 数据存储量：10万条数据容量存储时间间隔设置 防爆等级？Exia II CT4 防护等级 IP66 执行标准：GB 15322.3-2019","附参数表","块","1.00","","","","","","一级安全标准化整改"]
["3","TM20211218105956538cf36","便携式气体分析仪（SF6）","内置泵吸式测量，显示方式，2.5 寸 320*240 高清彩屏显示 典型精度：≤±2% FS12.线性度，≤±1% 13.重复性？≤±1% 报警方式，声光+振动+视觉报警15. 工作电源，充电式锂电池，电池容量;3.6VDC，5500mA大容量可充电电池 使用环境，温度-40℃~+70℃； 相对湿度≤0-99%RH 数据存储量：10万条数据容量存储时间间隔设置 防爆等级？Exia II CT4 防护等级 IP66 执行标准：GB 15322.3-2019","附参数表","块","1.00","","","","","","一级安全标准化整改"]
["4","TM202112181059565380d92","CO检测报警仪","MIC-500-CO；线制：两线制；量程：0-500ppm； 电压：24VDC 配：防水密封接头：EXdII CT6；防护等级：IP65；防爆连接螺纹3/4'NPT","MSA，深圳逸云天，英思科","台","4.00","","","","","",""]
["5","TM20211218105956538c0f6","CO检测报警仪","量程：0-100ppm；三线制；输出4-20mA；电压24VDC；精度：＜±5%F.S；工作温度：-40℃-70℃；防护等级IP66；防爆等级ExdII CT6，带声光报警；带遥控器，带HART协议；","MSA，深圳逸云天，英思科","台","6.00","","","","","",""]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]