{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":16,"n_cols":13,"rows_kept":16,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["陕西长青能源化工有限公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","TM20211224155713480ff1b","防爆轴流风机","BT35-11-315# 风量2300m3/h，风压80Pa，转速1450rpm，电压380V，功率0.12KW，防爆标志ExdⅡCT4Gb，玻璃钢材质，壁式安装，风叶前后加防护罩及百叶，WF2，要求0.18KW。","","台","2.00","","","","","","一级安全生产标准问题整改：原水消防泵房轴流风机更换。玻璃钢材质，壁式安装，风叶前后加防护罩及百叶，WF2，要求0.18KW。"]
["2","TM20211224155713481719b","轴流风机","FBT35-11-3.15/220 0.37KW 电压AC220V 安装方式：壁式（I）转速1450r/min 风量3810m3/h 风机前后加防护罩、网格 防爆等级：ExdIIBT4 防腐等级WF2  壳体材质：玻璃钢风筒及风叶","","台","4.00","","","","","","动力脱硫综合楼腐蚀轴流风机更换"]
["3","TM20211224155713481fb76","变频器风机","NMB-MAT 3615KL-05W-B50 DC24V 0.32A","","件","2.00","","","","","","捞渣机变频器柜风扇"]
["4","TM2021122415571348160f7","离心式通风机","9-26 5A 风量：4293-6762m3/h全压：6033-6180pa电机功率：15kw，风机进口尺寸：170*270mm 出口尺寸：φ273mm 电机地脚螺栓：M10 孔距：210mm \n风机方向顺时针逆时针各一个，","","台","2.00","","","","","","风机进口尺寸：170*270mm 出口尺寸：φ273mm 电机地脚螺栓：M10 孔距：210mm 风机方向顺时针逆时针各一个，C4301A/B挡板门密封风机更换"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]