{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":26,"n_cols":13,"rows_kept":26,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["陕西长青能源化工有限公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","TM2021112211522926083cd","安全阀","A27W-10T   DN15mm","","只","6.00","","","","","","皮带除尘器；工作压力0.7-1.0Mpa;整定压力0.7Mpa，T≤200℃。"]
["2","TM20211122115229261a108","安全阀","A14H-10 公称通径：DN8；连接尺寸：M20*1.5；整定压力：0.88MPa；回座压力：0.79MPa；排放压力：0.906MPa；工作温度:≤200℃。材质304","","台","5.00","","","","","","净化储气罐安全阀"]
["3","TM20211122115229262cc3a","安全阀","A14H-10 公称通径：DN8；连接尺寸：M20*1.5；整定压力：0.88MPa；回座压力：0.79MPa；排放压力：0.906MPa；工作温度:≤200℃。材质304","","台","18.00","","","","","","气化储气罐增加安全阀"]
["4","TM2021112211522926245a3","安全阀","A14H-10 公称通径：DN15；连接尺寸：M30*2；整定压力：0.88MPa；回座压力：0.79MPa；排放压力：0.906MPa；工作温度:≤200℃。材质304","","台","9.00","","","","","","气化储气罐增加安全阀"]
["5","TM2021112211522926292cd","安全阀","A14H-10 公称通径：DN15；连接尺寸：M30*2；整定压力：0.88MPa；回座压力：0.79MPa；排放压力：0.906MPa；工作温度:≤200℃。材质304","","台","1.00","","","","","","净化储气罐安全阀"]
["6","TM20211122115229263330d","安全阀","A14H-10 公称通径：DN20；连接尺寸：M36*2；整定压力：0.88MPa；回座压力：0.79MPa；排放压力：0.906MPa；工作温度:≤200℃。材质304","","台","6.00","","","","","","气化储气罐增加安全阀"]
["7","TM2021112211522926334bd","安全阀","A14H-10 公称通径：DN25；连接尺寸：M42*2；整定压力：0.88MPa；回座压力：0.79MPa；排放压力：0.906MPa；工作温度:≤200℃。材质304","","台","15.00","","","","","","气化储气罐增加安全阀"]
["8","TM202111221152292645b4d","安全阀","A21W-16P  DN15 压力等级:0.7-1.0MPa 整定压力:0.8MPa","","台","1.00","","","","","","合成储气罐增加安全阀"]
["9","TM20211122115229264adf5","安全阀","A21W-16P，DN40（11/2\")，压力等级:0.7-1.0MPa 整定压力:0.8MPa  介质：空气  材质：304","","台","4.00","","","","","","仪表空气储罐用"]
["10","TM20211122115229264f962","安全阀","A21W-16P，DN50（2\")，压力等级:0.7-1.0MPa 整定压力:0.8MPa  介质：空气  材质：304","","台","3.00","","","","","","压缩空气储罐用"]
["11","TM202111221152292655682","安全阀","A27Y-16P DN50 1.6MPa  整定压力1.05MPa    温度110℃ CF8/STL","","台","1.00","","","","","","回用水储气罐"]
["12","TM20211122115229265ff38","安全阀","A27Y-16P DN65 1.6MPa  整定压力1.05MPa    温度110℃ CF8/STL","","台","1.00","","","","","","回用水储气罐"]
["13","TM20211122115229265d4aa","安全阀","A42Y-16P DN32  1.6MPa  RF 整定压力0.8MPa  温度50℃ CF8/STL","","台","2.00","","","","","","脱盐水储气罐"]
["14","TM202111221152292668a09","安全阀","A42Y-16P DN32 1.6MPa  RF 整定压力1.05MPa 温度150℃    CF8/STL","","台","1.00","","","","","","污水储气罐"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]