{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":15,"n_cols":13,"rows_kept":15,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["陕西长青能源化工有限公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","TM202111011522278434adb","气动调节阀","口径1\"公称压力ANSI150   额定CV13 阀前压力：0.5MPa，工作温度：150℃ 流量特性EQ%   行程20mm   阀体A216-WCB   阀芯/阀板SUS316/SS 阀座SUS316/SS 工作温度-5~+230℃   驱动源340KPa G 动作DA 4-20mA   介质：液化气 FC 结构长度：185mm","TV101温度调节阀更换","台","1.00","","","","","","吴忠仪表、北京艾坦姆、无锡智能自控"]
["2","TM202111011522278448e78","调节阀","DN100 150LB 温度：40℃ 阀前压力：0.5MPa 阀后压力：0.015MPa 正常流量:250Nm/h 最大流量：300Nm3/h 事故位：FO 介质：氮气 密封面：RF 阀体材质：ASTM A216 WCB 阀芯材质：316 阀座/密封环：316 轴承/导向套：316/HCr 阀杆材质：316/HCr 电气接口：1/2 NPT 电源接口：1/4 NPT 泄漏等级：Ⅴ级","T3701B罐氮气管线阀门新增","台","1.00","","","","","","吴忠仪表、北京艾坦姆、无锡智能自控"]
["3","TM20211101152227844a0e7","调节阀","DN50 600LB 工作压力：-5-230℃ 形成：25mm FC 阀体材质：A216-WCC 阀芯材质：SUS410\\HT 阀座材质：SUS410\\HT 范围：4-20mA 额定CV：9.8 流量特性：LIN结构长度：290mm 介质：循环气 阀前：5MPa 阀后常温 温度：70℃ 附阀门规格书","PV33205阀门更换","台","1.00","","","","","","吴忠仪表、北京艾坦姆、无锡智能自控"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]