{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":29,"n_cols":13,"rows_kept":29,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["陕西长青能源化工有限公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","TM2021121811135860371ed","不锈钢耐震压力表","YN-100BT -0.1-0.15MPa，径向带后边  \"螺纹安装M20*1.5 外壳材质：304；精度 ：1.6级","","只","3.00","","","","","","径向带后边"]
["2","TM202112181113586034568","不锈钢耐震压力表","YN-100B    1.6MPa，量程：0-1.6MPa；结构形式：径向无边；精度1.6；螺纹连接：M20*1.5；表盘直径：100mm","","只","10.00","","","","","","量程：0-1.6MPa；结构形式：径向无边；精度1.6；螺纹连接：M20*1.5；表盘直径：100mm"]
["3","TM20211218111358604a56a","磁翻板液位计","温度：45℃额定压力：常压 测量范围：1000mm 连接法兰：DN25 150LB RF 侧安装 精度±10mm 防护等级：IP65 介质密度：1000KG/m3 带排污阀（材质304）本体材质304 浮子材质：316L","LG-22521 E2217罐","个","1.00","","","","","","罐区T3601AB增加水洗塔液位计用"]
["4","TM20211218111358604bf23","电动球阀","工作电压AC/DC24V， 功率 4W ，开关时间 5S， 防护等级 IP67， 最大扭力 2N.m  ，带继电器输出型反馈功能， 阀体材质316L ，接口尺寸  1”/2，内螺纹。","参考：BD3S；DC24 POWER 4W TORQUE 2Nm Acttime 5-7s     S&amp;S Miniature Electric Ball Valve","台","6.00","","","","","","全厂脱销CEMS用"]
["5","TM2021121811135860509c8","取样泵","型号：N86KNE ；电源：220-230VAC 50HZ；工作压力：Pmax：2.4 bar；功率：60W；安装方式：带泵体、带终端接头Φ6","脱硝氮氧化物取样","台","2.00","","","","","","全厂脱销CEMS用"]
["6","TM202112181113586055a91","差压变送器","型号：430A，模式：S1，-EBS4A-92DB/NS11，电源：10.5-30V DC,输出：4-20mA,最大工作压力：14MPa，出厂量程：-5～20KPa，带三阀组","动力驰放气总管流量计","台","1.00","","","","","","动力驰放气总管流量计"]
["7","TM20211218111358606c308","压力开关","压力范围：0-60KPa，出厂设定压力：50KPa，电压：DC 24V，防护等级：IP65，防爆等级：Exd IIC T6，连接形式：螺纹M20×1.5","","台","3.00","","","","","","动力A/B/C炉驰放气系统压力开关"]
["8","TM2021121811135860607d8","压力开关","压力范围：0-60KPa，出厂设定压力：5KPa，电压：DC 24V，防护等级：IP65，防爆等级：Exd IIC T6，连接形式：螺纹M20×1.5","","台","3.00","","","","","","动力A/B/C炉驰放气系统压力开关"]
["9","TM2021121811135860633b2","转速探头","Bi5-M18-AN6X 电压10-30VDC  200mA","","件","2.00","","","","","","畅卫兴计划；气化煤称重给料机转速探头"]
["10","TM20211218111358607104c","电磁阀","V5222-08,压力：0.15-0.8MPa，电压：220V，防爆线圈：Exd IIC T4","","个","1.00","","","","","","动力甲醇点火系统检修"]
["11","TM20211218111358607fa38","取样针型阀","材质：316  压力：60MPa 耐温：≥300℃ 连接方式：双卡套 连接尺寸：φ10  ( 参考型号：SS-1RS10MM )","","个","6.00","","","","","","全厂取样根部阀"]
["12","TM2021121811135860835c8","蓄电池","TYSONIC TY-6-4.5 带四头端子线","","块","2.00","","","","","","设备后续维修用零部件，其他厂家无法加工替代"]
["13","TM202112181113586081bba","VENTIS MX4 外置泵","部件号：VTSP-0011   美国英思科，MX4四合一便携式气体检测仪","","个","5.00","","","","","","设备后续维修用零部件，其他厂家无法加工替代"]
["14","TM202112181113586082fb6","氧传感器","部件号：17134461   美国英思科MX4复合式气体检测仪","","个","5.00","","","","","","设备后续维修用零部件，其他厂家无法加工替代"]
["15","TM20211218111358609b0a8","显示屏","XP-3110可燃气体测爆仪用","日本新宇宙XP-3110测爆仪","件","2.00","","","","","","设备后续维修用零部件，其他厂家无法加工替代"]
["16","TM202112181113586091c29","IR光源","订货号：C79451-A3468-B206，西门子","ULTRAMAT 23气体分析仪用","个","1.00","","","","","","设备后续维修备件，其他品牌无法代替"]
["17","TM202112181113586107e18","ARM驱动板","CA8JYPJ005ML  艾默生","污水调节池艾默生COD表用","个","1.00","","","","","","设备后续维修用零部件，其他厂家无法加工替代，必须从原供应商处采购"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]