{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":21,"n_cols":13,"rows_kept":21,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["陕西长青能源化工有限公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","TM202509091041571949f99","防爆电缆夹紧密封接头","防爆等级：Exd IICT4；防护等级：IP65；螺纹尺寸：M60*1.5(M)；材质：黄铜镀镍；温度范围：-40℃-120℃；3C认证 过线范围：30-36mm，非铠装电缆","华荣科技股份有限公司/中国创正防爆电气有限公司、英国GMP公司","个","11.00","","","","","","气化、罐区气体报警器中间接线箱更换，螺纹需具体测量，华荣科技股份有限公司/中国创正防爆电气有限公司、英国GMP公司"]
["2","TM202509091041571968f45","防爆电缆夹紧密封接头","防爆等级：Exd IICT4；防护等级：IP65；螺纹尺寸：G1-1/2\"(M)；材质：黄铜镀镍；温度范围：-40℃-120℃；3C认证，线缆线径：26mm-36mm，非铠装电缆","华荣科技股份有限公司/中国创正防爆电气有限公司、英国GMP公司","个","12.00","","","","","","低甲、压缩机气体报警器中间接线箱更换，华荣科技股份有限公司/中国创正防爆电气有限公司、英国GMP公司"]
["3","TM20250909104157196be5e","防爆铠装电缆密封接头","防爆等级：Exd IICT4；防护等级：IP65；螺纹尺寸：M25*1.5(M)；材质：黄铜镀镍；温度范围：-40℃-120℃；3C认证","华荣科技股份有限公司/中国创正防爆电气有限公司、英国GMP公司","个","18.00","","","","","","安可信气体报警器胶泥整改用，华荣科技股份有限公司/中国创正防爆电气有限公司、英国GMP公司"]
["4","TM202509091041571971073","防爆铠装电缆密封接头","防爆等级：Exd IICT4；防护等级：IP65；螺纹尺寸：G1-1/2\"(M)；材质：黄铜镀镍；温度范围：-40℃-120℃；3C认证，通径，线径20mm","","个","22.00","","","","","","气化装置分析仪表接线箱防爆密封格兰头检修更换，"]
["5","TM202509091041571982cbc","防爆铠装电缆密封接头","防爆等级：Exd IICT4；防护等级：IP65；螺纹尺寸：M32*2(M)；材质：黄铜镀镍；温度范围：-40℃-120℃；3C认证.通径，线径17mm","","个","25.00","","","","","","气化装置分析仪表接线箱防爆密封格兰头检修更换，"]
["6","TM202509091041571990f89","防爆铠装电缆密封接头","防爆等级：Exd IICT4；防护等级：IP65；螺纹尺寸：M25*2(M)；材质：黄铜镀镍；温度范围：-40℃-120℃；3C认证。通径。线径14mm","","个","3.00","","","","","","气化装置分析仪表接线箱防爆密封格兰头检修更换，"]
["7","TM20250909104157200661c","防爆电缆密封接头","黄铜镀镍 M16*1.5（M） EXdII CT5","-长青","个","6.00","","","","","","气化装置分析仪表接线箱防爆密封格兰头检修更换，"]
["8","TM202509091041572017efc","防溢流防静电控制器","ET-DLC-B  防爆等级EXDIIBT4GB","-长青","台","1.00","","","","","","甲醇装车栈台使用"]
["9","TM20250909104157202c998","防爆接线箱","BXJ53-20/60，箱体材质为不锈钢316L，箱体尺寸：400*300*150（宽*高*深）；内置60节魏德米勒或菲尼克斯品牌端子，分成2排布局；下进线，1个M32*1.5黄铜镀镍防爆格兰，下出线，14个M20*1.5黄铜镀镍防爆格兰；防爆标志：ExebⅡCT6 Gb / ExtbIIIC T80℃？Db，防护等级：IP66，防腐等级：WF2，3C认证，防爆合格证。","","套","2.00","","","","","","渣水气体报警器中间接线箱腐蚀更换，需提供图纸，华荣科技股份有限公司/中国创正防爆电气有限公司、英国GMP公司"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]