{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":25,"n_cols":13,"rows_kept":25,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["江苏徐矿能源股份有限公司物资供销分公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","TM20250612151133282f001","PH计","E+H 变送器：CPM223-MR005 线缆：CYK10-E051 电极：CPS11E-BA7BAA2 配套仪表箱及流通池","","套","1.00","","","","","","配套仪表箱、控制箱IP66 支架：D-CYA112支架（PVC）+D-CYH112支架，热控：合理化建议#2沉淀池进口加装PH计使用"]
["2","TM202506121511332831674","聚氯乙烯护套软线","RVV 4*6.0mm2","","m","300.00","","","","","","#0皮带通风廊风机断路器安装"]
["3","TM20250612151133284917a","家用电线","BVR软线，4平方，红色","","m","200.00","","","","","","输煤楼宿舍安全整改/"]
["4","TM202506121511332869e03","家用电线","BVR软线，5平方，蓝色","","m","200.00","","","","","","输煤楼宿舍安全整改/"]
["5","TM202506121511332901404","家用电线","BVR软线，6平方，地线","","m","200.00","","","","","","输煤楼宿舍安全整改/"]
["6","TM20250612151133293e75d","热继电器","LED3357C 37-50A","","个","3.00","","","","","","电气：中央空调控制柜更换/"]
["7","TM202506121511332940d0f","气密式组合开关","HZ10M-10/3 380V 10A 双管式 安装孔距：上下中心孔距60mm 左右中心孔距78mm","","个","8.00","","","","","","电气：轴流风机墙壁开关/"]
["8","TM202506121511332945610","差压开关","SOR BH-001008-001 0-3kPa 最大静压70kPa","","块","4.00","","","","","","热控：#1炉B修膛负压主保护开关需更换4块/"]
["9","TM202506121511332952f8f","铝合金防爆断路器","3P 10A","","套","2.00","","","","","","#0皮带通风廊风机断路器安装/"]
["10","TM202506121511332964d37","时间控制配电箱","380V 延时停止 启停按钮","","套","1.00","","","","","","密封制粉机开关安装/"]
["11","TM20250612151133297088d","压力变送器","EJA530A -DAS4N-02DE 0-25KPa S2 M20*1.5 Hart协议 耐压0.2MPa","","台","3.00","","","","","","热控：合理化建议#1炉磨煤机动态分离器密封风风压使用/"]
["12","TM20250612151133298e152","压力变送器","EJA530A -DCS4N-02DE 0-2.5MPa S2 M20*1.5 Hart协议 耐压10MPa 带计量所检定报告","","台","1.00","","","","","","热控：工业抽汽压力变送器使用1台/"]
["13","TM2025061215113329926f8","差压变送器","0-4kPa EJA110A-DMS5A-62DC S1带配套固定底座 最大静压16MPa φ10mm宝塔嘴接口","","块","3.00","","","","","","热控：#1炉密封风机入口差压改造使用2个、同类型磨煤机风压变送器20个以上备用1个/"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]