{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":13,"n_cols":13,"rows_kept":13,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["江苏徐矿能源股份有限公司物资供销分公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","8275160013","PH分析仪","包含PH电极、控制器、仪表箱及安装支架。测量介质：硫铵浆液，有腐蚀性，测量范围：（0-14）PH；工作压力：0.5MPa，工作温度：85℃，PH电极采用插入式安装，尺寸为1”，长度457mm，电极选用抗腐蚀钛材护套，电极电缆5米。控制器：电源24V，4-20mA输出带现场温度及PH显示。电极及控制器防爆等级EXiaIIC T4。控制器需安装在不锈钢保温仪表箱内。","硫回收脱硫二级循环泵P23A02A/B出口管线增加PH计","台","1.00","","","","","","产品符合规格型号参数，严格执行化工标准等国家、行业强制认证规定，直发长青能源化工有限公司，货到需包含卸车，物流快递需送货上门，交货期为订单下达后45天内送达。报价备注申请付款方式。建议品牌：E+H、罗斯蒙特、ABB"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]