{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":41,"n_cols":13,"rows_kept":41,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["陕西长青能源化工有限公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","TM202506040932218838240","接触器","LC1D18M7C-AC220V","","件","3.00","","","","","","气化P1302A/B/C高压煤浆泵控制柜更换"]
["2","TM20250604093221885c9cf","交流接触器","LC1D25M7C  220V","","只","2.00","","","","","","气化P1302A/B/C高压煤浆泵控制柜更换"]
["3","TM20250604093221886e1f4","跑偏开关","两级跑偏开关-12-30EX-KPT1 380V","沈阳东鹰实业有限公司","个","2.00","","","","","","煤运皮带使用，满足煤粉尘防爆环境"]
["4","TM202506040932218878848","阻旋式堵煤开关","XLLV-Z-250？？防爆等级：Ex tb IIIC T130℃？Db","","个","4.00","","","","","","煤运装置4#、9#皮带堵煤开关更换"]
["5","TM202506040932218877bd0","压力开关","\"ZSE30A-01-N；Sup：12-24VDC  \nCLASS2  40mA MAX\nOP.PRESS  0--101kpa     SMC               \nOUT1  NPN\"","SMC","个","1.00","","","","","","关键备件补库，动力硫酸铵包装机检修"]
["6","TM20250604093221888a81a","按钮开关","XB2-EA135，AC/DC 220/380,自复位，一开一闭，红色","上海天逸电气有限公司/正泰/思楷楷（上海）开关有限公司/施耐德","只","5.00","","","","","","动力A/C炉炉膛火焰电视就地控制柜检修"]
["7","TM20250604093221889da05","按钮开关","XB2-EA135，AC/DC 220/380,自复位，一开一闭，绿色","上海天逸电气有限公司/正泰/思楷楷（上海）开关有限公司/施耐德","只","5.00","","","","","","动力A/C炉炉膛火焰电视就地控制柜检修"]
["8","TM20250604093221890807a","指示灯","AD22-22D/S  220VAC红色","上海天逸电气有限公司/正泰/思楷楷（上海）开关有限公司/施耐德","只","12.00","","","","","","动力A/C炉炉膛火焰电视就地控制柜检修"]
["9","TM20250604093221891b864","指示灯","AD22-22D/S  220VAC绿色","上海天逸电气有限公司/正泰/思楷楷（上海）开关有限公司/施耐德","只","12.00","","","","","","动力A/C炉炉膛火焰电视就地控制柜检修"]
["10","TM202506040932218927549","瓷保险管","R015 ，φ10*36/4A  500V","上海沪工/德力西电气/正泰","个","8.00","","","","","","动力A/C炉炉膛火焰电视就地控制柜检修"]
["11","TM2025060409322189304bc","打滑检测器","EXDH-III  220VAC  3A  防爆等级：ExtD A21 IP66，皮带速度范围:0.3-5.0m/s","-长青","个","4.00","","","","","","1#、2#皮带速度开关更换"]
["12","TM202506040932218942fcf","键盘","MatePad Pro13.2 宣白 智能磁吸","","只","1.00","","","","","","办公室1"]
["13","TM20250604093221895594d","UPS电源","C1KS(G7) 额定容量：1KVA/1KW","","台","1.00","","","","","","厂前区办公楼209室食堂充卡器不间断电源使用"]
["14","TM20250604093221895231f","加热盘","直径180mm,220V/2kw FL-2Y封闭电热板用","","个","5.00","","","","","","封闭电热板备件"]
["15","TM202506040932218962aa2","照明开关","双开双控，AC220V，10A，86型，白色 明装","","个","4.00","","","","","","动力高低压室照明改造"]
["16","TM20250604093221897c647","照明开关","86型？ 暗装 三联？ 白色","","只","4.00","","","","","","厂前区食堂二楼大包间使用和驿站楼一楼大厅使用，要求未启用时是整个平面"]
["17","TM20250604093221898f6a1","LED应急装置","型号：SS-SLZD-E18W-261C,额定电压：AC220V 50Hz，应急时间：90分钟，保护等级：IP30，配接光源：LED 18W(主电功耗18W），光通量：50lm","","套","2.00","","","","","","厂前区食堂2楼招待餐厅使用"]
["18","TM20250604093221899a2a1","300型红绿交通信号灯","规格型号：电压：220V  功率：24W  尺寸：754mm*360mm*120mm  灯珠：LED  灯杆：2m","","套","1.00","","","","","","汽车洗车台用"]
["19","TM20250604093221899a97f","防爆接线盒","G型二吊BHD51-G3/4G ExdIICT6 Gb/ExtdIIIC T80℃CDb AC220/380V 20A 铝合金外壳 镀镍紧固件及压紧螺母","","只","100.00","","","","","","防爆区域现场照明接线盒整改使用"]
["20","TM20250604093221900baf6","防爆接线盒","D型四平BHD51-G3/4G ExdIICT6 Gb/ExtdIIIC T80℃CDb AC220/380V 20A 铝合金外壳  镀镍紧固件及压紧螺母","","只","100.00","","","","","","防爆区域现场照明接线盒整改使用"]
["21","TM20250604093221901e93a","电动葫芦吊钩","2T  360°旋转式","","件","2.00","","","","","","供水班组用，双挂绳"]
["22","TM2025060409322190217fc","电机接线盒","型号：Y2-160-180 功率：22kW 安装孔距：102×102mm 固定孔距：138*145mm 高度：74mm 材质：加厚铁皮 带胶垫","","件","3.00","","","","","","P409D系列电机"]
["23","TM20250604093221902f765","电机接线盒","型号：Y2-200-225 功率：37kW 安装孔距：132×132mm 固定孔距：192*175mm 高度：97mm 材质：加厚铁皮 带胶垫","","件","2.00","","","","","","P409C系列电机"]
["24","TM202506040932219034b8a","饮水机","美的 YR1002S-X，尺寸：920MM*310MM*305MM，上置，立式，冷热款","","台","1.00","","","","","","生产1"]
["25","TM202506040932219049078","电梯通话主机","型号：ZDH01-020-GG","办公楼电梯使用","个","1.00","","","","","","办公楼电梯使用"]
["26","TM202506040932219047575","魔管制冷器","型号：FTV-M 动力火焰电视摄像机用","铁岭铁光/铁岭诚信","个","1.00","","","","","","动力A/C炉火焰电视就地控制柜检修"]
["27","TM202506040932219050a75","滑块","孔径：4mm，孔中心距（长）：40mm，孔中心距（宽）：35mm，槽宽：25mm，材质：316L，滚轮固定螺栓为沉头型","","个","2.00","","","","","","动力硫酸铵包装机滑块检修"]
["28","TM20250604093221906aa54","黄油嘴（带防尘帽）","PT1/8 铜镀镍  1/8转10*1接头","","个","20.00","","","","","","气化现场电机加油嘴更换"]
["29","TM20250604093221907f491","槽式直通电缆桥架","宽200mm*高100mm*厚2.0mm（附盖板及其连接件、螺丝），材质：铝合金，附件材质：304","","m","10.00","","","","","","动力1#脱硫CEMSS旁仪表桥架腐蚀更换"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]