{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":17,"n_cols":13,"rows_kept":17,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["苏能（锡林郭勒）发电有限公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","TM2025102713555345093f7","快速门门板","铝片厚度0.7mm，中间聚氨酯发泡，门板总厚度为45mm，宽不低于200mm、防夹手门帘","","套","2.00","","","","","","约24平方，保障质量，安装及使用能够满足现场使用需求。"]
["2","TM20251027135553452f999","伺服门控系统","人机对话界面；多圈绝对值编码器多功能端口；开、关、停、安保、感应外、手自动切换、一键启停、互锁输入、外部故障输入；输出端口具有：互锁输出、故障输出等；电机堵转和过载保护。","","套","2.00","","","","","","速度每秒0.8-1.3米，保障质量，安装及使用能够满足现场使用需求。"]
["3","TM20251027135553453c85c","伺服电机","1.5KW","","套","2.00","","","","","","建议品牌：宝久、格兰德。保障质量，安装及使用能够满足现场使用需求。"]
["4","TM20251027135553454de1c","五金框架部件、钢结构等","专用镀锌基板2.0mm烤漆","","套","2.00","","","","","","含钢结构、封板、五金件等。保障质量，安装及使用能够满足现场使用需求。"]
["5","TM20251027135553455a335","安全保护","","","套","2.00","","","","","","光电保护装置对射型红外、无线全气囊保护装置、手动开关（三孔）、双面地磁开启装置、遇阻反弹装置。保障质量，安装及使用能够满足现场使用需求。"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]