{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":28,"n_cols":13,"rows_kept":28,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["陕西长青能源化工有限公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","TM20250909105514609f3e5","双卡套直通终端接头","？6-？6   材质：塑料","","个","10.00","","","","","","煤质仪器管路用"]
["2","TM2025090910551461031a5","单卡套式直通终端接头","1/4NPT外丝-？6.316L卡套  材质：不锈钢","","只","10.00","","","","","","区域报警仪修用备件"]
["3","TM202509091055146117458","浆轮流量探头","P51530-P2；管道尺寸DN300  管道压力等级PN16；   流量计螺纹连接","美国GF","只","1.00","","","","","","回用水反渗透进水总管，美国GF"]
["4","TM20250909105514612187c","针型阀","YW-VKV，3000PSI,1/2-1/4   316L  附图","","个","10.00","","","","","","密闭取样器用"]
["5","TM202509091055146139fa1","压力开关","SOR 6B3-EE2-M3-C2A-C1 7-30PSI 防爆等级：EXdIICT6 防护等级：IP64","P2205B泵缓冲罐压力开关更换","台","2.00","","","","","","P2205B泵缓冲罐压力开关更换"]
["6","TM20250909105514614d3b2","电动葫芦吊钩","2T  360°旋转式","","件","4.00","","","","","","供水班组用"]
["7","TM20250909105514614247e","铜开口接线鼻","100A","","件","20.00","","","","","","现场接地线整改"]
["8","TM20250909105514615a6db","铜开口接线鼻","150A","","件","20.00","","","","","","现场接地线整改"]
["9","TM20250909105514616d734","充电LED防爆照明灯","12V 400W ExeII CT6 IP6","","只","2.00","","","","","","动力、气化、净化现场受限空间应急使用"]
["10","TM20250909105514617402d","碳钢标准腐蚀挂片","I型 50mm*25mm*2mm","","片","70.00","","","","","","循环水腐蚀速率监测"]
["11","TM20250909105514618f1d7","13X分子筛填充气相色谱柱","长度6ft,1/8\",内径2mm,60/80目，部件号G3591-81035","美国安捷伦，7820A气相色谱","根","4.00","","","","","","美国安捷伦，7820A气相色谱用"]
["12","TM2025090910551461880a3","磁性开关","XQJHUHZ-68;带1组常开常闭触点，触点容量：24VDC 0.5A，220VAC 0.3A;防护等级：IP65.","","个","4.00","","","","","","脱盐水酸碱间计量箱液位计"]
["13","TM20250909105514619f074","防爆行程开关","BZX51-6 防爆行程开关 ExdeⅡCT6 AC220V /380V 6A","","只","2.00","","","","","","2#合成压缩机防爆行车行程开关"]
["14","TM20250909105514620cabb","智能温度报警器","DM-1079，DELIXI","","套","2.00","","","","","","脱盐水变频室，煤浆制备变电所用，德力西"]
["15","TM20250909105514620709e","防爆执法记录仪","DSJ-T3,防爆标志：Ex ib ⅡC T4 Gb;Ex ib ⅢC T130℃ Db。录像分辨率：1440p，显示屏：2.0英寸，电池：内置3000mAh，内存：128G,传输接口3.0.F2.2大光圈，高清红外夜视，IP6级防水。","","台","15.00","","","","","","生产部现场受限空间及特级动火作业视频记录用"]
["16","TM202509091055146218e76","电子式执行机构","型号：361LXB-50，电源：220V AC，50HZ,150VA，行程：60mm,输出力矩：5000N，4～20mA，防爆等级：Exd IIC T4，防护等级：IP66，执行机构连接尺寸与原阀门匹配。","动力厂前区采暖系统蒸汽调节阀检修","台","1.00","","","","","","动力厂前区采暖系统蒸汽调节阀检修，鞍山工装自控仪表有限公司/江苏贝尔阀门控制有限公司"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]