{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":18,"n_cols":13,"rows_kept":18,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["江苏徐矿能源股份有限公司物资供销分公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","8260139915","超高效三相异步电动机","YE3-225M-10-W 15KW电压：380V、电流：36.1A安装方式：立式安装，绝缘等级：F级，△ ,3C，转速584r/min，？ 防护等级：IP68，防腐等级：WF2，带加油嘴","动力汽轮机蒸发冷风机电机更换 ，带不锈钢防雨罩，因前轴特殊，需现场测绘","台","2.00","","","","","","以下产品符合规格型号参数，严格执行化工标准等国家、行业强制认证规定，直发长青能源化工有限公司，货到需包含卸车，物流快递需送货上门，交货期为订单下达后30天内送达；备注申请付款方式，不备注默认按集团月度排款。建议厂家：卧龙电气南阳防爆、佳木斯电机股份、 兰州电机股份，带不锈钢防雨罩，因前轴特殊，需现场测绘。"]
["2","8260186211","电机","YBX3-160M1-2-WF2  11KW，电压：380V、电流：20.6/11.9A 安装方式：卧式安装，绝缘等级：F级，△/Y ，转速2927r/min，防爆标志 ExdIICT4 Gb，EX 3C  防护等级：IP55，防腐等级：WF2，带加油嘴","","台","1.00","","","","","","需现场测绘。"]
["3","8260193475","隔爆型三相异步电动机","YBX4-132M-4，7.5KW，电压380V， 电流15.4A，△接法，转速1440r/min， 防爆标志 ExdIICT4 Gb，EX 3C，卧式安装，F级，IP55，带加油嘴","","台","1.00","","","","","","建议厂家：卧龙电气南阳防爆集团股份有限公司、佳木斯电机股份有限公司"]
["4","8260193476","隔爆型三相异步电动机","YBX4-132M-4，7.5KW，电压380V，电流27/15.6A，Y/△接法，转速1440r/min，防爆标志 ExdIICT4 Gb，EX 3C，立式安装，F级，IP55,带加油嘴。","","台","1.00","","","","","","建议厂家：卧龙电气南阳防爆集团股份有限公司、佳木斯电机股份有限公司，原型号为BN 132MA4-U2，防腐等级：WF2，带不锈钢防雨罩，需供应商现场测绘确认，附原电机铭牌照片"]
["5","8260784275","高效率复合防爆型三相异步电动机","YBFBX-132S-2，7.5KW，电压：380V、电流：14.8/8.6A 接法：△， 转速：2900r/min，防爆标志 ExdIIC T4Gb/ExtD A21 IP66 T135°C 安装方式：立式安装，气体粉尘双认证 绝缘等级：F级,防腐等级：WF2","","台","2.00","","","","","","建议厂家：卧龙电气南阳防爆集团股份有限公司、佳木斯电机股份有限公司，特殊电机需现场测绘"]
["6","1465060011","超高效三相异步电动机","YE3-90L-6  1.1KW","","台","2.00","","","","","","立式"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]