{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":18,"n_cols":13,"rows_kept":18,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["江苏徐矿综合利用发电有限公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","无税单价（元）","总价（元）","品牌","备注"]
["1","6002030006","电动截止阀","J961Y-32 DN50 21V 12Crlmov","","只","4.00","","","","","","阀杆与阀瓣配合至少有两重保护，防止阀瓣脱落，阀瓣、阀座设计耐磨损、耐冲刷，推荐：南通电站，上海电修，中核苏阀.连接盘尺寸：145/120，三爪连接，阀体长度不低于260mm.温度545℃，不含电动头"]
["2","1134465532","气动球阀","Q661H-64C  32mm","","只","1.00","","","","","","热再供热减温器后疏水气动门，阀体铸钢材质，介质蒸汽，压力3.6MPa，温度≤425℃。执行器为气动AT型，全开全关，单进汽形式，气开门，配气管连接件"]
["3","2522840032","气动阀","DN80","","个","4.00","","","","","","气动金属旋转阀，型号：LM641Y-10Q-80，阀体要求整体铸造，厂家：江苏龙迈环保，无锡宝丰电力，山东丰晖环保，纽普兰能源环境科技。除尘器灰斗平衡阀用。已核实库存，无需核减。"]
["4","1005161049","不锈钢截止阀","J41W-25P  50mm","","只","4.00","","","","","","304不锈钢材质，规格型号符合国标要求，不得使用翻新阀门，提供质检报告，水压试验报告"]
["5","1135224066","蝶阀","D371J-16C   65mm","","只","5.00","","","","","","铸钢阀门，全衬胶，配蜗杆传动机构，用于除盐水制水系统。"]
["6","1135224081","蝶阀","D371J-16C   80mm","","只","5.00","","","","","","铸钢阀门，全衬胶，配蜗杆传动机构，用于除盐水制水系统。"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]