{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":17,"n_cols":13,"rows_kept":17,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["陕西长青能源化工有限公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","TM202510101018031704dc0","防爆接线箱","\"型号规格：  BXJ53—20/50\n\n主要技术参数：\n1、箱体为不锈钢316L材质  ，箱体尺寸 400*400*250 ；\n2、内置50节魏德米勒 、或菲尼克斯品牌端子  ；\n\n3、下进线 1个M40*1.5  黄铜镀镍铠装双密封防爆格兰  ，下出线 10个 M20*1.5 黄铜镀镍铠装双密封防爆格兰；\n4、防爆标志：Ex db ⅡC T6 Gb /  Ex tb IIIC T80℃ Db ， \n5、防护等级： IP66   ，防腐等级：WF2；产品带防爆合格证 、国家强制性3C认证书 、型式报告书\"","华荣科技股份有限公司、中国创正防爆电气有限公司、英国CMP公司","台","3.00","","","","","","氢回收仪表接线箱整改，华荣科技股份有限公司、中国创正防爆电气有限公司、英国CMP公司"]
["2","TM20251010101803172ddc9","防爆接线箱","\"型号规格：  BXK\n\n主要技术参数：\n1、壳体为 铝合金材质  ， 箱内装2个 消防模板 、接线端子 、固定安装板 ；\n2、下进线  6个 M20*1.5 黄铜镀镍 ，铠装双密封防爆格兰 ；\n3、防爆标志：Ex db ⅡB T6 Gb /  Ex tb IIIC T80℃ Db ; \n4、防护等级：IP66  ， 防腐等级：WF2；产品带防爆合格证 、国家强制性3C认证书 、型式报告书\"","华荣科技股份有限公司、中国创正防爆电气有限公司、英国CMP公司","台","10.00","","","","","","煤储运消防接线箱整改，华荣科技股份有限公司、中国创正防爆电气有限公司、英国CMP公司"]
["3","TM202510101018031734f4d","防爆接线箱","BHD-22/2.AD 30*23*16（cm） 进线线径：40mm 出线线径 （5-15）mm 出线口数量：16个（带防爆堵头） 额定电压：380/220V 额定电流：20A  防爆等级：EXdbIICT4 EXtbIIIC Db 防护等级：IP66/IP67（铭牌带EX标识）,带3C认证","飞策防爆电气股份有限公司/华荣科技股份有限公司/新黎明防爆电器","个","2.00","","","","","","硫磺造粒机防爆接线箱更换（现场测量），飞策防爆电气股份有限公司/华荣科技股份有限公司/新黎明防爆电器"]
["4","TM20251010101803174b625","防爆接线箱","BHD-22/2.AD 长19.5cm 宽13cm 高：6cm  进线数量：1 出线口数量：4个（带防爆堵头） 额定电压：380/220V 额定电流：6A  防爆等级：EXdbIICT4 EXtbIIIC Db 防护等级：IP66/IP68（铭牌带EX标识）,带3C认证","飞策防爆电气股份有限公司/华荣科技股份有限公司/新黎明防爆电器","个","1.00","","","","","","硫磺造粒机防爆接线箱更换（现场测量），飞策防爆电气股份有限公司/华荣科技股份有限公司/新黎明防爆电器"]
["5","TM202510101018031758979","防爆控制按钮","YH8030 两组常开触点","硫磺包装机用","个","3.00","","","","","","气化捞渣机现场控制柜用"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]