{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":31,"n_cols":13,"rows_kept":31,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["陕西长青能源化工有限公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","TM2025100916430622647b3","止回阀","ZHF-40\t镀锌","锅炉仓泵（无锡中冶环保科技有限公司）","件","6.00","","","","","","锅炉仓泵用"]
["2","TM202510091643062281056","波纹管安全阀","PSV2302AB 整定压力0.3MPa 进口DN40 150LB 出口DN80 150LB 进出口尺寸 面心距依照安全阀数据表1 工艺参数详见数据表2","WCB/304+Ste","台","2.00","","","","","","PSV2302AB"]
["3","TM202510091643062293af5","安全阀","PSV2309B  整定压力：1.0Mpa；其他详见数据表","WCB 北京航天 V2304闪蒸罐顶","台","1.00","","","","","","PSV2309B更新"]
["4","TM20251009164306229f90a","安全阀","PSV3505 型号0.75DIHTXYL-01C 介质循环水 DN20 工作压力0.4MPa 常温 整定压力0.6MPa 进口法兰DN20 150Lb RF 出口法兰DN25 150Lb RF","","台","1.00","","","","","","E-3507冷却水出口"]
["5","TM20251009164306230ba84","气动插板阀","DN300,管道介质：锅炉炉渣，阀体/阀板材质：WCB/304，阀板厚度：10mm，法兰孔径：22mm，孔中心距：397mm，阀门档距：155mm，气缸电磁阀供电：220VAC，气缸及电磁阀带φ10快插接头，气缸活塞杆带橡胶护套。","","台","2.00","","","","","","动力C炉渣仓放渣阀检修/整阀品牌：上海巨良集团/双恒阀门集团/雷力（上海）阀门，气缸及电磁阀品牌：SMC、亚德客"]
["6","TM20251009164306231844f","减压阀","Y42X-16P DN50 介质常温水，进口压力0.8-0.9MPa，出口压力0.2-0.3MPa  阀体材质：不锈钢","回用水配药管线专用","台","1.00","","","","","","回用水配药管线"]
["7","TM2025100916430623115b2","闸阀","Z41H-16C DN150 RF  WCB/13Cr，介质：污水；适用温度≤425℃。","","台","1.00","","","","","","回用水浓水池管线（结构长度275mm）"]
["8","TM20251009164306232f119","闸阀","Z41H-25C  RF  DN200  WCB/13Cr","--煤化工专用","台","1.00","","","","","","B组一级高加蒸汽调节阀后手阀/中核苏阀/哈尔滨电站阀门/青岛电站阀门/上海电站阀门/华夏阀门"]
["9","TM20251009164306233f7a5","气动陶瓷双闸板阀","Z644TC-16C，DN50，PN1.6，阀体材质：WCB+内衬陶瓷；阀芯::WCB+内衬陶瓷，，档距：200mm，法兰孔径：16mm，孔中心距：125mm。气缸工作压力：0.4-0.6MPa，使用压力：0.2-0.6MPa，工作温度：≤220℃，配3/8NPT转φ8卡套式终端接头。","","个","3.00","","","","","","动力3台锅炉仓泵气动排气阀检修/无锡中冶/青岛山野/金泰美林"]
["10","TM202510091643062341265","球阀","Q41F-16C PN16 DN20  RF A105/橡胶","","台","2.00","","","","","","污水PAC补水管线"]
["11","TM20251009164306234add0","球阀","Q41F46-10C  DN25  RF WCB/F46","全衬氟（包含阀芯）","台","1.00","","","","","","P23A02AB导淋用"]
["12","TM202510091643062353fec","球阀","Q41F46-16P  DN40 PN1.6Mpa  RF   316L/F46，介质：硫酸铵溶液 温度：70度。","","台","3.00","","","","","","P23A06出口"]
["13","TM202510091643062362b99","蝶阀","D341F46-16C DN125 RF  WCB/全衬氟（包含阀芯衬氟），介质：硫酸铵浆液，适用温度≤200℃。","","台","1.00","","","","","","P23A04入口"]
["14","TM202510091643062362090","内螺纹截止阀","J11W-16  DN20  PN1.6Mpa  304，阀体长度55mm","","个","2.00","","","","","","P2101AB循环水管线"]
["15","TM2025100916430623725e4","内螺纹截止阀","J11W-16 DN25 PN1.6Mpa 304","","个","4.00","","","","","","P4003AB循环水管线"]
["16","TM20251009164306237bde2","法兰截止阀","J41H-16C DN15    PN1.6MPa,  RF   A105/13Cr  ,制造标准GB/T12238,压力试验标准GB/T13927,","","只","1.00","","","","","","/"]
["17","TM2025100916430623810eb","法兰旋启式止回阀","H44H-16C  DN150  RF WCB/STL","汽机凝结水泵出口","台","2.00","","","","","","汽机凝结水泵出口止回阀更换/中核苏阀/哈尔滨电站阀门/青岛电站阀门/上海电站阀门/华夏阀门"]
["18","TM20251009164306239d605","法兰旋启式止回阀","H44W-16P DN80 RF    304/304","","台","1.00","","","","","","2#汽轮机高压油泵出口止回阀更换/中核苏阀/哈尔滨电站阀门/青岛电站阀门/上海电站阀门/华夏阀门"]
["19","TM20251009164306239c109","疏水阀","TB11F-16C,DN15,PN1.6Mpa,RF,A105/13Cr","","台","5.00","","","","","","净化伴热站疏水阀维护"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]