{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":29,"n_cols":13,"rows_kept":29,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["江苏徐矿能源股份有限公司物资供销分公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","TM20250527143302599b9e2","O型圈","φ187*4.5、氟橡胶（温度：≥250°，压力：10Mpa，介质：水）","/阿克苏电厂","个","9.00","","","","","","机务：#1、2、3热网循环泵机封端盖使用（留一套备用）/"]
["2","TM20250527143302601ddfe","O型圈","φ170*3.5、氟橡胶（温度：≥250°，压力：10Mpa，介质：水）","/阿克苏电厂","个","12.00","","","","","","机务：#1、2、3热网循环泵轴承室使用（留一套备用）/"]
["3","TM202505271433026025717","O型圈","φ200*4.5、氟橡胶（温度：≥250°，压力：10Mpa，介质：水）","/阿克苏电厂","个","9.00","","","","","","机务：#1、2、3热网循环泵骨架油封端盖使用（留一套备用）/"]
["4","TM20250527143302603a650","开关电源","NDR-240-24（220VAC输入24VDC10A输出）导轨安装","/阿克苏电厂","块","10.00","","","","","","磨煤机控制柜及其他控制柜更换10个/B修"]
["5","TM2025052714330260461a9","轴套","泵型号DG450-60*3；转速：1480r/min；扬程160m；流量340m3/h；汽蚀余量4.9m；配套功率250kw；效率79%；原厂家：湖南利欧泵业有限公司","/阿克苏电厂","个","6.00","","","","","","机务：#1、2、3热网疏水泵使用/"]
["6","TM20250527143302605f5cc","双筒油滤器","型号：GYZ2-25（带切换阀）；材质：#45钢。配滤芯2个、尺寸：滤芯总长85mm、滤芯直径φ47mm、滤芯口内径22mm、滤芯口外径31.5mm、滤芯口高5.5mm；原厂家：北京电力设备总厂","/阿克苏电厂","套","2.00","","","","","","机务：2-1、2-2引风机油站使用/"]
["7","TM20250527143302605dfb9","轴套","泵型号600S 100G；扬程115m；流量3200m3/h；允许汽蚀余量6.6m；轴功率1179kw；转速1450r/min；配用功率1400kw；效率85%；重量4030kg；原厂家：新疆兰泵节能科技有限公司","/阿克苏电厂","个","6.00","","","","","","机务：#1、2、3热网循环泵使用/"]
["8","TM20250527143302606ac5e","填料套","泵型号600S 100G；杨程115m；流量3200m3/h；允许汽蚀余量6.6m；轴功率1179kw；转速1450r/min；配用功率1400kw；效率85%；重量4030kg；原厂家：新疆兰泵节能科技有限公司","/阿克苏电厂","个","6.00","","","","","","机务：#1、2、3热网循环泵使用/"]
["9","TM20250527143302607c56e","双吸环","泵型号600S 100G；杨程115m；流量3200m3/h；允许汽蚀余量6.6m；轴功率1179kw；转速1450r/min；配用功率1400kw；效率85%；重量4030kg；原厂家：新疆兰泵节能科技有限公司","/阿克苏电厂","个","6.00","","","","","","机务：#1、2、3热网循环泵使用/"]
["10","TM20250527143302607e1c0","正压式组合密封体","GMF-18-BR1/00.00","/阿克苏电厂","个","4.00","","","","","","碎煤机前后轴密封用/"]
["11","TM20250527143302608253a","方形带衬板双法兰S型管","700*700mm L=1300mm材质：本体：8mmQ235 衬板：8mmQ235+6mm厚的高铬合金耐磨材料，含碳量≥3.8%，含铬量≥32%","/阿克苏电厂","套","2.00","","","","","","滚轴筛至#5皮带落煤管/"]
["12","TM20250527143302609eaf1","方形带衬板双法兰S型管","700*700mm L=1000mm材质：本体：8mmQ235 衬板：8mmQ235+6mm厚的高铬合金耐磨材料，含碳量≥3.8%，含铬量≥32%","/阿克苏电厂","套","2.00","","","","","","碎煤机至#5皮带落煤管/"]
["13","TM202505271433026096e9c","机械密封","泵型号OS125-290I；杨程：106m；流量：580m3/h；转速：2980r/min；效率：83%；必须汽蚀余量8m；配用功率280KW；原厂家：山东硕泵泵业科技有限公司","/阿克苏电厂","套","2.00","","","","","","机务：中水泵备用（一台泵两套机封）/"]
["14","TM202505271433026105e8e","机械密封","泵型号TJ100-80-160；Q=85m3/H；H=30m；U=380V；N=15KW；转速2900r/min；原厂家：江苏通用机械设备有限公司","/阿克苏电厂","套","3.00","","","","","","机务：化水#1中间水泵机封更换（7台泵通用）/"]
["15","TM202505271433026113193","GR对轮","对轮材质：42CrMo；电机侧：轴径φ75mm、长140mm、键槽宽20mm；泵侧：轴径φ45mm、长110mm、键槽宽14mm；对轮总长250mm（配套GR缓冲垫、材质：聚氨酯）","/阿克苏电厂","套","3.00","","","","","","机务：#1、2、3中水泵对轮更换/"]
["16","TM202505271433026128a58","电话","CORD 118","/阿克苏电厂","个","5.00","","","","","","电气：办公室更换/"]
["17","TM20250527143302612fad2","止回阀","H44H-25C DN125 温度≤425℃ 介质：水","/阿克苏电厂","个","1.00","","","","","","机务：#2热网补水泵出口逆止门更换/"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]