{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":26,"n_cols":13,"rows_kept":26,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["陕西长青能源化工有限公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","TM20250508151413642dc37","涡轮法兰式蝶阀","D341X-16 DN125,RF,介质：蒸汽，温度150℃，DN125，档距约135mm（不含凸面）","226A换热站","台","4.00","","","","","","介质：蒸汽，温度150℃，DN125，档距约135mm（不含凸面），226A换热站/ 中国上正阀门/精工阀门/五洲阀门/良工阀门/立信阀门/无锡美瑞克"]
["2","TM2025050815141364421c0","内螺纹球阀","Q11F-16P DN15 (1/2″)   304/F46","","个","3.00","","","","","","离心机冲洗水用/中国上正阀门/精工阀门/五洲阀门/良工阀门/立信阀门/无锡美瑞克"]
["3","TM20250508151413644d3e3","蝶阀","D41X-16C DN100 RF   WCB/橡胶","","台","1.00","","","","","","介质：蒸汽，温度150℃，档距约120mm（不含凸面），226A换热站/中国上正阀门/精工阀门/五洲阀门/良工阀门/立信阀门/无锡美瑞克"]
["4","TM20250508151413645843d","蝶阀","D41F-16C   DN65  WCB","","台","2.00","","","","","","介质：蒸汽，温度150℃，档距约110mm（不含凸面），226A换热站/中国上正阀门/精工阀门/五洲阀门/良工阀门/立信阀门/无锡美瑞克"]
["5","TM202505081514136468fec","衬氟隔膜阀","G41F46-16     32mm","","台","1.00","","","","","","2号脱硫塔底出料泵冲洗水手阀备用阀门"]
["6","TM2025050815141364796b8","减压阀","YK43X-16C，压力：1.6MPa,通径;50mm,进口压力：0.5MPa,出口压力：0.1-0.04MPa,温度≤120℃。","","台","1.00","","","","","","污水事故事故火炬分液管线配管"]
["7","TM20250508151413647a7af","阀板","圆形阀板，阀板直径：950mm(带外环板)/878mm（不带外环板），阀板厚度：6mm；阀板外环板宽度：84mm，厚度：6mm；阀板上部带6根肋板，肋板长：345mm，高：50mm，壁厚：5mm；阀板中心筒孔径：65mm，高：45mm，壁厚：4mm；阀板中心孔直径：22mm；阀板材质：WCB，阀板外环板与主阀板采用材质为316L，M6×25螺栓（带弹簧垫平垫）24个连接固定","动力布袋除尘器提升阀用（修改后）","套","3.00","","","","","","动力布袋除尘器提升阀阀板检修"]
["8","TM202505081514136488f98","闸阀","Z41Y-16C，DN50,RF   WCB/STL","","件","2.00","","","","","","污水事故事故火炬分液管线配管"]
["9","TM20250508151413649568b","闸阀","Z41Y-16C DN80 RF  PN16  WCB/STL","--煤化工专用","台","1.00","","","","","","污水事故事故火炬分液管线配管"]
["10","TM20250508151413650db03","闸阀","Z41Y-16P  DN80  PN16  RF  L=203mm  CF8/STL","","台","1.00","","","","","","2#活性炭出口阀"]
["11","TM202505081514136506f8c","过滤器球阀","DN15-PN16，螺纹连接，黄铜","","个","1.00","","","","","","补充水泵出口多功能阀到压管阀门"]
["12","TM20250508151413651df5d","蝶阀","D371X-16C DN300 L=77mm WCB/橡胶 GB/T 12238-2008","","台","1.00","","","","","","污水出水泵进口阀更换"]
["13","TM2025050815141365253a3","截止阀","J41H-16P   DN20   RF  CF8/304","","台","2.00","","","","","","法兰标准：HG/T20615-2009，介质：脱盐水，温度：40℃，动力小锅炉厂房采暖系统水箱液位计增加根部阀"]
["14","TM20250508151413652714f","止回阀","H41X-16  DN150 RF L=210mm\t阀体：铸钢，密封圈：丁腈橡胶","","台","1.00","","","","","","调节池提升泵出口止回阀更换"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]