{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":19,"n_cols":13,"rows_kept":19,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["江苏徐矿能源股份有限公司物资供销分公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","TM202508291639512734b6f","水质浊度分析仪","壁挂式安装浊度仪（含二次仪表 投入式浊度仪探头 连接线 接头 管子等附件）量程：0-400NTU 精度±1%FS 二次仪表供电电压220VAC带配套配电箱","","套","1.00","","","","","","热控：合理化建议 脱硫澄清池溢流口加装壁挂式浊度仪/"]
["2","TM202508291639512758899","压力表","WIKA量程：0-16bar EN837-1 精度等级：CL1.6 接口螺纹尺寸G1/4","","块","2.00","","","","","","热控：EH油循环泵出口母管压力使用2块/"]
["3","TM20250829163951276ea91","水质浊度分析仪","MZX-01流通池式浊度仪（含二次仪表 浊度仪探头 流通池 连接线 接头 管子等附件）量程：0-30NTU 精度±1%FS 二次仪表供电电压220VAC带配套配电箱","","套","2.00","","","","","","热控材料：安全整改 空擦滤池浊度恢复/"]
["4","TM2025082916395127746d6","投入式液位变送器","ELE-802 量程0-10m 输出4-20mA 两线制 带配套LED液位显示变送器及二次仪表（带四组开关量输出及一组模拟量4-20mA输出）","","套","2.00","","","","","","热控材料： 合理化建议 #2机组胶球泵泵坑排污泵自动启停功能改造使用/"]
["5","TM202508291639512779d96","干湿度计","实验室高精度温湿度计,不锈钢材质,高精度进口机芯,带校准证书,CNAS认可,支撑挂钩两用,物理感应无需电池,温度范围-20-50℃,湿度范围0%-100%","","个","4.00","","","","","","煤质分析/"]
["6","TM202508291639512786031","泵吸式四合一气体检测仪","产品名称:GY520泵吸式 仪器尺:190*80*35(mm) 气体检测仪 显示屏幕:2.4寸彩色TFT 采样方式:泵吸式 报警方式:语音、声光、震动 操作语言:中文/英文 仪器充电:5V2A充电器 电池容量:7.4V 2000mAh 外壳材质:ABS+PC 气泵流量:≤800mL/min 防护等级:IP65 防爆等级:ExiaII CT4 工作湿度:10%RH~95%RH 工作温度:-20℃~55℃ 仪器重量:350g","","台","1.00","","","","","","煤场及动火作业前使用（安全整改）/"]
["7","TM202508291639512797627","指针式电流表","型号6L2 量程15A 变比15/5 开孔尺寸 74*74mm","","个","2.00","","","","","","#1机EH油循环泵使用/"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]