{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":14,"n_cols":13,"rows_kept":14,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["陕西长青能源化工有限公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","TM20250604091319486d72a","防爆云台摄像机","防爆等级：EX db ⅡC T6 Gb/EX Tb tb ⅢC T80°C Db;304不锈钢材质设计，400万像素，支持25倍光学变倍，16倍数字变倍，逐行扫描1/2.8\"CMOS；支持最大2560×1440@30fps高清画面输出；支持超低照度，0.005Lux/F1.6（彩色），0.001Lux/F1.6（黑白），0Lux with IR；支持ICR红外滤片式自动切换；支持宽动态、3D数字降噪；","支持3D定位，可通过鼠标框选目标以实现目标的快速定位与捕捉；支持开放型网络视频接口、ISUP；支持360°水平旋转，垂直方向-90°～90°；具有雨刷功能；支持H.265编码，红外100m。一路音频输入和输出；内置两路报警输入和一路报警输出，支持报警联动功能，IP68，TVS 6000V防雷、防浪涌和防突波保护；配套安装支架。内置GPU芯片，支持深度算法学习。能够对接公司安全生产智能化管控平台","台","15.00","","","","","","动力、净化合成、气化增加视频监控"]
["2","TM202506040913194888235","防爆移动布控球摄像机","防爆等级：EX db ib Ⅱ T6 Gb/EX ib tb ⅢC T80°C Db，400万分辨率，支持MIC、扬声器，实现昼夜监控、自动彩转黑、支持车辆及目标检测，区域入侵，佩戴安全帽检测，作业岗位检查，抽烟检查、打电话等违规行为检测，支持目标对比，可存储30W张人脸名单（需配TF卡）。","设备自身小屏可显示电池电量、GPS状态、4G/5G状态、录像状态、存储容量、平台链接状态、WiFi状态、智能算法模式；可通过移动端app实时查看现场视频情况，可对接公司安全生产智能化管控平台。","台","2.00","","","","","","现场受限空间作业监控"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]