{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":30,"n_cols":13,"rows_kept":30,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["江苏徐矿能源股份有限公司物资供销分公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","TM20250711160731764140e","流量计","SANKE GN37C 4-40L/H WATER带接头","","个","2.00","","","","","","热控：十米取样仪表使用/"]
["2","TM202507111607317673b2c","远传水表","LXS-50-JSPN10.DN50 带两侧法兰盘及配套垫片（需具备远传功能)","","块","1.00","","","","","","热控材料:住宅楼换热站内安装水表/"]
["3","TM202507111607317670e85","投入式液位变送器","FB0803WF3 长度≥2m，供电电压：12～36VDC （标定值为24VDC），输出信号：4～20mA 二线制，测量精度：±0.2%F.S ±0.3%F.S ±0.5%F.S","","个","1.00","","","","","","热控材料:住宅楼换热站补水箱使用/"]
["4","TM202507111607317682c77","打光笔","GFB220 2.5mm通用接口 输出模式：CW/1Hz/2Hz 输出功率：20mW","","支","1.00","","","","","","热控：火焰电视、云母水位计等设备、监控维护使用/"]
["5","TM20250711160731769085d","近电预警器","YJ-AM-3 220V-10KV-35KV三档位","","个","23.00","","","","","","电气：安全帽内部近电预警器（电气13热控10）/"]
["6","TM202507111607317706a2b","单相交流电流表","型号：T1-A/5/R 辅助电源：DC/AC 85-265V 额定电流：AC 5A CT：750A/5A 尺寸：46*46mm方形","","个","3.00","","","","","","电气：中水泵房MCC开关整改/"]
["7","TM2025071116073177023c2","万用表表笔","红+黑探针软线 万用表型号：FLUKE 17B+","","套","6.00","","","","","","电气：班组万用表表笔更换/"]
["8","TM202507111607317718c27","不锈钢隔膜压力表","YTP-100MF 法兰款式 GH/T2059 DN25 PN25 RF法兰款式 0-1.6MPa（带上下限三色标识）上自仪、安徽天康、重庆川仪三品牌之一","","块","2.00","","","","","","热控材料：尿素区输送泵B出口压力使用/"]
["9","TM20250711160731772f562","人车分离雷达","PLUTO 外形：162mm*110mm*65mm检测高度：2.5m-9.0m检测速度：5cm/s-25km/h","","个","1.00","","","","","","输煤汽车门备件/"]
["10","TM2025071116073177236bf","红外线装置","ABT-30","","套","2.00","","","","","","输煤汽车门备件/"]
["11","TM202507111607317731c97","防爆型压差变送器","EJA110E-JFS5J-912EA/NF2","","个","1.00","","","","","","气膜煤场备件/"]
["12","TM202507111607317749b51","壁挂式温湿度传感器","APEG-WH-2S 温度：-40至80℃ 湿度：0-100%RH 误差：±3%RH 电压：24V","","个","1.00","","","","","","气膜煤场备件/"]
["13","TM202507111607317750c96","工业及商业用途点型可燃气体探测器","3T-ASD5300 气体：甲烷 测量范围：3-100%LEL 防爆标识：ExdII CT6 Gb","","个","1.00","","","","","","气膜煤场备件/"]
["14","TM20250711160731775d6f9","有毒有害气体检测（报警）仪","ASD5300C 气体：一氧化碳 测量范围：0-1000ppm 防爆标识：ExdII CT6 Gb","","个","1.00","","","","","","气膜煤场备件/"]
["15","TM202507111607317768aba","粉尘浓度传感器","GGG1000","","个","1.00","","","","","","气膜煤场备件/"]
["16","TM2025071116073177773d8","风速传感器","LE2151","","个","1.00","","","","","","气膜煤场备件/"]
["17","TM202507111607317779a68","氧气回火防止器","pmax=0.15Mpa 74mm*15.8mm","","个","4.00","","","","","","输煤检修日常维护用/"]
["18","TM20250711160731778b965","乙炔回火防止器","pmax=0.15Mpa 74mm*15.8mm","","个","4.00","","","","","","输煤检修日常维护用/"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]