{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":39,"n_cols":13,"rows_kept":39,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["陕西长青能源化工有限公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","TM2025102909222719304b5","不锈钢防爆按钮装置","BZA8050-G-A2（启、停）","","个","6.00","","","","","","气化破渣机现场控制柜用，红色3个，绿色3个"]
["2","TM202510290922271951204","交流接触器","SC-N4/SE[80]   DC48V","","只","2.00","","","","","","气化、煤运、动力电梯控制柜内接触器"]
["3","TM2025102909222719658fa","防爆行程开关","DLXK-D   电流10A  电压220v/380v  防爆等级：Exdb IIC T6/Extb IIIC T80","","只","6.00","","","","","","任小平计划 ：硫磺造粒机旧行程开关更换"]
["4","TM20251029092227197582f","打滑检测器","EXDH-III  220VAC  3A  防爆等级：ExtD A21 IP66，皮带速度范围:0.3-5.0m/s","-长青","个","2.00","","","","","","煤储运现场检修使用"]
["5","TM202510290922271974369","高频独立电路板正线","高频独立电路板，用母卡添加子卡的模式，正线分体","","个","30.00","","","","","","维修用"]
["6","TM2025102909222719814f7","高频独立电路板反线","高频独立电路板，用母卡添加子卡的模式，反线分体","","个","30.00","","","","","","维修用"]
["7","TM20251029092227199f9a6","温控器","HS-602A","","只","3.00","","","","","","食堂用"]
["8","TM20251029092227199f80f","鼠标","M110     USB接口，线缆长度1.8米","","个","5.00","","","","","","装置操作站用"]
["9","TM2025102909222720053f0","电脑主机电源","航嘉500W  ATS12V","","台","5.00","","","","","","仪器工作站电脑用"]
["10","TM202510290922272019ac2","防爆人体静电释放报警器","CD-PSA-V  锂电","","个","10.00","","","","","","带声光报警，质保五年，防爆等级Exia IIC T6 Ga，净化合成区域使用（卢帅）"]
["11","TM20251029092227202aab2","电机接线盒","型号：Y2-200-225 功率：37kW 安装孔距：132×132mm 固定孔距：192*175mm 高度：97mm 材质：加厚铁皮 带胶垫","","件","2.00","","","","","","要求带M48*2超薄锁紧螺母2个；P409K1/K2电机更换"]
["12","TM2025102909222720221b9","防爆挠性连接管","BNG-25*600 (一端G1\"活套内螺纹，一端G1\"活套外螺纹）材质：橡胶，防爆等级：ExdIICT4","","根","4.00","","","","","","重大危险源气体报警器更换使用"]
["13","TM20251029092227203731f","自控温电热带专用防爆电源接线盒","型号：FDH，额定电压220V/380V，额定电流40A，防爆标志：EX edmbIICT4Gb","气化分析取样预处理箱电伴热","个","2.00","","","","","","硫回收分析仪表预处理箱整改"]
["14","TM20251029092227204a503","自控温电热带专用防爆温度控制器","型号：BJW，额定电压220V/380V，额定电流16A，防爆标志：EX edmbIICT4Gb","气化分析取样预处理箱电伴热","个","7.00","","","","","","2#合成分析仪表预处理箱整改"]
["15","TM20251029092227205b22b","一体化三阀组","DN5-250P，配EJA110A-EMS4A-97DA/NS1差压变送器使用","动力驰放气总管流量计","台","1.00","","","","","","氢回收非渗透气FT3403检修用"]
["16","TM20251029092227206ae7c","烟气取样器","额定电压AC230V 150W 耐温180℃，机柜控温，反吹阀 24V、探杆长度1米、杆粗30mm、探杆头加滤芯、DN50法兰法兰外径165mm，水平孔距88-90mm","符合《水污染源在线监测系统安装技术规范》HJ 353-2019要求  技术参数见附件","台","1.00","","","","","","动力脱硝B炉氮氧化物取样备用"]
["17","TM20251029092227207cdc3","快插接头","1/4NPT-φ6","铜","件","20.00","","","","","","供水装置，铜"]
["18","TM202510290922272070cc8","快插接头","1/4NPT-φ8  PN20","铜","件","10.00","","","","","","供水装置，铜"]
["19","TM20251029092227208b37e","针头过滤器","希波氏,25mm/NYL/0.45um，100pcs","","盒","20.00","","","","","","分析耗材"]
["20","TM20251029092227209250a","通用湿度过滤器","型号：SS-2T,Max:4bar","脱硝A炉控制柜用","个","1.00","","","","","","脱硝C炉控制柜"]
["21","TM20251029092227209e31f","压力表接头","PN63 M20*1.5/Φ14 304","","只","10.00","","","","","","打压泵接头制作"]
["22","TM20251029092227210d317","保护箱","保护箱,800(高)x600(宽)x500(深),带安装支架,CS","3","只","2.00","","","","","","主装置/空分循环水去旁滤器流量计保护箱更换"]
["23","TM20251029092227211b3b8","回讯器","0.6A 125VDC,0.3A 250VDC,16A 125/250VAC,接口：1/2NPT  防爆等级：EXdbIICT4 EXtbIIIC Db 防护等级：IP66/IP67（铭牌带EX标识）","西美尔","个","1.00","","","","","","硫磺造粒机阀门更换，西美尔"]
["24","TM2025102909222721176b4","二苯胺磺酸钠","AR 25g/瓶","","瓶","1.00","","","","","","实验室分析用"]
["25","TM2025102909222721289be","电梯轿厢通讯板","RS32 V1.2 V1.0 DBA26800J1","气化、动力、煤储运电梯主控板","个","1.00","","","","","","煤储运筒仓电梯使用，通讯板为西子奥的斯电梯配套专用，需向原供应商采购，否则影响功能配套要求；西子奥的斯"]
["26","TM202510290922272127a0a","门禁电源控制器","型号：CU-P9  输入电压AC110-240V 50/60HZ   输出电压DC12-14V   48VA  延时范围0-15S 外形尺寸90*90*35mm  产品重量300g","","只","1.00","","","","","","厂前区大会堂电动门控制器，电动门配套配件，与主机相配套的核心部件。高优(COUNS深圳市高优科技有限公司)"]
["27","TM20251029092227213e4fa","电磁阀","DSG-02-2B8-LW","动力布袋除尘器提升阀用，苏州科亚液压气动有限公司（品牌台湾DANXIN）","个","2.00","","","","","","动力锅炉液压关断门电磁阀检修，锅炉重要设备，附件必须保持与原有采购项目的一致性，其他品牌无法替代，附照片，苏州科亚液压气动有限公司（品牌台湾DANXIN）"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]