{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":29,"n_cols":13,"rows_kept":29,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["江苏省矿业工程集团有限公司安装分公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","TM202509302209476062bc7","球墨铸铁管","DN250","DN250","m","103.00","","","","","","球墨铸铁管DN300球管压力等级C30，球墨铸铁管防腐采用内衬高铝水泥，外喷涂锌层及红色沥青漆。球墨铸铁管外防腐采用锌+铁红色环氧漆。"]
["2","TM20250930220947607922a","球墨铸铁管","DN1200","DN1200","m","4.00","","","","","","球墨铸铁管DN400球管压力等级C30，球墨铸铁管防腐采用内衬高铝水泥，外喷涂锌层及红色沥青漆。球墨铸铁管外防腐采用锌+铁红色环氧漆"]
["3","TM202509302209476080cee","球墨铸铁管","DN250","DN250","m","90.00","","","","","","球墨铸铁管DN300球管压力等级C30，球墨铸铁管防腐采用内衬高铝水泥，外喷涂锌层及红色沥青漆。球墨铸铁管外防腐采用锌+铁红色环氧漆"]
["4","TM20250930220947608b5ec","塑料管","EN1280Bu/φ12χφ8(单机配35M)","EN1280Bu/φ12χφ8(单机配35M)","m","60.00","","","","","","1、材质及规格：DN80软管（耐磨压）2、其他详见图纸"]
["5","TM202509302209476091860","聚氨酯直埋保温无缝钢管","内管：无缝钢管Φ89×4.0，外管：黑色聚乙烯Φ155×3.0,聚氨酯发泡保温层厚度：30.0,两端法兰连接，压力（1.6MPA）","内管：无缝钢管Φ89×4.0，外管：黑色聚乙烯Φ155×3.0,聚氨酯发泡保温层厚度：30.0,两端法兰连接，压力（1.6MPA）","m","4.30","","","","","","1、规格、压力等级：钢管D273X62、其他详见图纸"]
["6","TM20250930220947609cb32","聚氨酯直埋保温无缝钢管","内管：无缝钢管Φ89×4.0，外管：黑色聚乙烯Φ155×3.0,聚氨酯发泡保温层厚度：30.0,两端法兰连接，压力（1.6MPA）","内管：无缝钢管Φ89×4.0，外管：黑色聚乙烯Φ155×3.0,聚氨酯发泡保温层厚度：30.0,两端法兰连接，压力（1.6MPA）","m","3.30","","","","","","1、规格、压力等级：钢管D325*72、其他详见图纸"]
["7","TM202509302209476109881","高清网络摄像机","DS-2CD3T45-I5","DS-2CD3T45-I5","台","5.00","","","","","","400W像素,1080P,0.1LUX低照度日夜转换,22倍变焦,云台控制可选,配供24V电源适配器,室内安装防护等级IP54,室外安装防护等级IP67"]
["8","TM20250930220947610a730","安装支架","定制","定制","个","5.00","","","","","","1、名称：摄像机立杆（基础支架落地基础）2、规格：杆高4.0m，不锈钢304，含底座、基础、接闪器等 3、其他未注明事项详见图纸要求"]
["9","TM20250930220947611cd3c","分体式高清视频终端","终端：Group310(1080P60帧)：含编解码主机、鹰眼四代摄像头、数字全向麦克风、线缆及遥控器。分体式设计、H.323/SIP标准、H.264 AVC/SVC，，(1080P/60/30fps、720P/60/30fps)，Siren22（22KHz）高清音频，2路高清输入，2路高清输出","终端：Group310(1080P60帧)：含编解码主机、鹰眼四代摄像头、数字全向麦克风、线缆及遥控器。分体式设计、H.323/SIP标准、H.264 AVC/SVC，，(1080P/60/30fps、720P/60/30fps)，Siren22（22KHz）高清音频，2路高清输入，2路高清输出","套","2.00","","","","","","1、名称：视频终端箱2、类别：箱内设置开关电源、8口POE交换机、光纤终端盒等3、其他未注明事项详见图纸要求"]
["10","TM2025093022094761196bc","防雷器","1625120142PLT-XL01","1625120142PLT-XL01","件","2.00","","","","","","1、名称：电源信号二合一防雷器2、其他未注明事项详见图纸要求"]
["11","TM20250930220947612b935","磁盘阵列","DE2000H，4816G FC口，冗电和双控，3*2T-电厂","DE2000H，4816G FC口，冗电和双控，3*2T-电厂","台","1.00","","","","","","1、名称：监控磁盘阵列2、规格：不少于24个硬盘位,单盘最大支持8T3、其他未注明事项详见图纸要求"]
["12","TM20250930220947612dc6e","NAS用存储硬盘","企业级ST33000650NS","企业级ST33000650NS","块","3.00","","","","","","1、名称：监控专用存储硬盘2、规格：8T3、其他未注明事项详见图纸要求"]
["13","TM2025093022094761319ea","电力电缆","YJV-0.6/1KV  3*4","YJV-0.6/1KV  3*4","m","300.00","","","","","","型号：YJV-0.6/1kV-3×4"]
["14","TM202509302209476136435","单模光纤","GYTA  4 芯 单模  铠装PE外套管","GYTA  4 芯 单模  铠装PE外套管","m","300.00","","","","","","四芯单模光纤"]
["15","TM202509302209476143b38","超五类室外双层阻水防水网线","HSYVY-5E 4*2*0.5","HSYVY-5E 4*2*0.5","m","150.00","","","","","","室外防水型超五类网线"]
["16","TM20250930220947614423f","电源线","RVVP  2*1.5","RVVP  2*1.5","m","150.00","","","","","","RW-2*2.5"]
["17","TM20250930220947615bea9","PE管","DN32  PN16（壁厚3.0mm）","DN32  PN16（壁厚3.0mm）","m","500.00","","","","","","PE32"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]