{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":50,"n_cols":13,"rows_kept":50,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["陕西长青能源化工有限公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","TM202110250759034037484","防爆变压器","BAB-1（IIC） 容量：1KVA 初级电压：220/380V；次级电压12V、24V；防护等级IP65；防爆等级：EXdeIICT6 Gb，G1”引入口1个，G3/4”引出口3个","","只","5.00","","","","","","防爆区域用防爆行灯变压器（一级标准化检查要求）"]
["2","TM20211025075903404ce80","行程开关","LX3-11H带重锤，电流5A，电压AC380DC220，触点形式一开一闭","","只","22.00","","","","","","起重机械增加双限位，含安装（脚手架、用电、焊接等由甲方协助提供）"]
["3","TM20211025075903404666e","红外开关","OMRON E3FA-DN  Class2  10 to 30 VDC","","只","1.00","","","","","","动力硫铵包装机用"]
["4","TM20211025075903405f75a","接近开关","1040758  SICK WX1809         IME12-04NNSZW2","","只","2.00","","","","","","动力硫铵包装机用"]
["5","TM202110250759034056cac","黑色按键船型开关","KCD5-201 2路4脚2档，外形尺寸21*24","","只","10.00","","","","","",""]
["6","TM202110250759034053106","防爆指示灯","BD8070 AC220V~380V CNEx17.0443U ExdeIICGb 白色","","个","5.00","","","","","","VOCs DP-37A01防爆控制箱使用  颜色为：白色"]
["7","TM202110250759034057bff","防爆指示灯","BD8030 AC220V-380V EXibIIT6 红色开孔尺寸30mm","","个","10.00","","","","","","新合成厂房一楼润滑油泵使用"]
["8","TM202110250759034062c41","防爆指示灯","BD8030 AC220V-380V EXibIIT6 绿色开孔尺寸30mm","","个","10.00","","","","","","新合成厂房一楼润滑油泵使用"]
["9","TM202110250759034060ecc","复合外套金属氧化物避雷器","YH5WZ6-17/45","","台","3.00","","","","","","Uc:13.6KV  Ur:17KV U1mA:≧24KV  In:5KA 50HZ 压力释放大电流：16KA 小电流：800A ；动力高压室3234柜使用，原厂家：西安神电"]
["10","TM202110250759034060bf4","防爆变频器调速控制柜","下进下出、防爆标准：ExdeIICT4Gb 防护等级：IP65 防腐等级： WF2  额定电压：380/400V （户外配防雨罩）  G=1.1/4\" 进线口1个、G=1\"出线口 4个、3/4\"出线口 2个","","台","1.00","","","","","","具体见设计图、变换氨水提浓泵改造"]
["11","TM20211025075903407c398","防爆连接器","3P+N+PE  16A  电压：380V-415V 防护等级IP66   WF1；防爆等级：EXdeIICT6 Gb  适用电缆外径：9mm-14mm","","套","30.00","","","","","","临时电缆中间接线头使用（一级标准化要求）  GB/EX tD A21  T80℃"]
["12","TM202110250759034073b64","防爆连接器","3P+N+PE  32A 电压：380V-415V 防护等级IP66   WF1；防爆等级：EXdeIICT6 Gb  适用电缆外径：17mm-24mm","","套","30.00","","","","","","临时电缆中间接线头使用（一级标准化要求）  GB/EX tD A21  T80℃"]
["13","TM20211025075903407e81c","变频器","ACS550-01-015A-4（7.5/5.5KW），ABB","","台","1.00","","","","","","动力硫磺包装机改造"]
["14","TM202110250759034082a14","变频器","ACS510-01-07A2-4（3KW)，ABB","","台","1.00","","","","","","变换氨水提浓改造"]
["15","TM20211025075903408462a","热水器","史密斯10B2，包安装及所需辅材，","","台","1.00","","","","","","灌装公共卫生间安装。"]
["16","TM20211025075903408dae8","对讲机电池","型号：BL2409-Ex","海能达","块","15.00","","","","","","部门对讲机用"]
["17","TM20211025075903409d2f0","高伏碱性电池","12V 23A","","节","5.00","","","","","","营销中心电动门和风机遥控器使用。"]
["18","TM20211025075903409d47a","多用插座","公牛GN-403 5米线 2500W 250V 10A     GB2099.3-2008","","只","2.00","","","","","","供水 现场微波炉、饮水机等使用"]
["19","TM202110250759034098a30","防感应电指示灯","SYRC-AC220V-D22R","","个","50.00","","","","","","部分操作柱、抽屉感应电消除（红色）"]
["20","TM20211025075903410ad3a","防感应电指示灯","SYRC-AC220V-D22G","","个","50.00","","","","","","部分操作柱、抽屉感应电消除（绿色）"]
["21","TM20211025075903410a63d","防爆强光工作灯","BAD503 电池规格：14.4V 10Ah  光源规格：24/8W（LED）IP66 ExdeIICT4","","只","2.00","","","","","","现场检修临时照明  GB/EX tD A21  T80℃"]
["22","TM20211025075903410baae","多功能防爆强光探照灯","BAD309E  光源：LED　IP65 底部带磁铁   ExdeIICT4","","只","2.00","","","","","","现场检修临时照明   GB/EX tD A21  T80℃"]
["23","TM20211025075903411697f","防爆人体静电释放报警器","CD-PSA-V  锂电，带声光报警、质保五年","济南辰典电子  山东瑞诺  新安德电子","个","25.00","","","","","","带声光报警、质保五年（故障更换） 罐区、动力静电释放柱更换"]
["24","TM20211025075903411c0ef","ABB变频器控制面板","ACS-CP-D，中文面板，","","件","3.00","","","","","","要求：中文面板，现场ABB变频器中文面板备件"]
["25","TM20211025075903411194d","轴流风机","FT35-11-3.15/220 0.25KW 电压AC220V 安装方式：壁式（I） 壳体材质：风筒及风叶玻璃钢  风机外壳直径外径400mm 内径355mm 深度300mm  防腐等级：F2","","台","3.00","","","","","","压滤机一楼轴流风机更换"]
["26","TM202110250759034122ba2","除尘器控制柜","柜高750mm，宽500mm，厚300mm,底部6个DN25出线孔,DN20带灯按钮21个，防爆标志：ExdBT6，额定电压380/220V；工作频率50HZ；容量6KW；防护等级IP65；","皮带除尘器控制柜","套","7.00","","","","","","煤运8#皮带、10#皮带、13#皮带除尘控制器更换"]
["27","TM20211025075903412c4b7","蓄电池","FP1270 额定容量：12V7AH 20Hr 外形尺寸：151*65*94mm 重量：2.22KG，带附件、质保五年","","块","2.00","","","","","","301总变火灾控制器备用电池更换"]
["28","TM202110250759034138f2c","磁性按钮保护罩","DZ42*42*30","","只","100.00","","","","","","全厂低压进线柜、母联柜急停按钮使用"]
["29","TM202110250759034137ec7","转速探头","Bi5-M18-AN6X 电压10-30VDC  200mA","TURCK","件","1.00","","","","","","动力给煤机皮带秤用"]
["30","TM20211025075903413e009","总线扩展卡","NIC-3200(PC)V1.0","","个","1.00","","","","","","消防控制室上位机总线扩展卡"]
["31","TM20211025075903414b1d7","串口服务器","型号：ZLAN5843A-485,8串口RS232/485转TCP/IP转化器，8串口独立全双工工作，互不干扰。8个RS232/485串口，2个RJ45网口，2个10M/100M以太网接口，电源：9-24VDC,标准电源插座。","","个","1.00","","","","","","动力报警控制系统传输通讯用"]
["32","TM202110250759034141218","黄绿铜导线","黄绿铜导线,6mm2,黄绿PVC护套","","m","200.00","","","","","","多股软铜线，现场接地整改"]
["33","TM20211025075903414aa68","吸尘吸水机","JB070*006/116  功率：双电机2400W，容量：70L，真空吸力2000mmH2O, 高度92cm,桶直径：44cm ,气流量：106L/秒，电压220V,带5米线","","台","1.00","","","","","","班组打扫卫生用"]
["34","TM20211025075903415bd44","锂电电池","MX4加强锂电池\t3.7V/2.2Ah/8Wh,部件号：p/n：17148313-1，","美国英思科，送货须提供商家授权等先关资料","块","2.00","","","","","","MX4多气体检测仪用"]
["35","TM2021102507590341500c9","仪器背袋","XP-3110新宇宙可燃气体测爆仪用","日本新宇宙XP-3110测爆仪，送货须提供商家授权等先关资料","个","5.00","","","","","","日本新宇宙XP-3110测爆仪用"]
["36","TM20211025075903416e445","IR光源","订货号：C79451-A3468-B206，西门子","ULTRAMAT 23气体分析仪用，送货须提供商家授权等先关资料","个","1.00","","","","","","脱硝U23分析仪用，设备后续用零部件，"]
["37","TM202110250759034163d3e","密封组件","Mb100z-xb6-ps  SMC","送货须提供商家授权等先关资料","套","5.00","","","","","","动力布袋除尘器提升阀气缸检修，SMC气缸配套零部件，"]
["38","TM202110250759034160ecc","执行机构电路板","BYPTZT-V08，与白云电力电动执行机构DZW120配套","白云电力机械厂","件","2.00","","","","","","动力主给水前电动阀检修用；电动执行机构配套用电路板，配套零部件，"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]