{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":33,"n_cols":13,"rows_kept":33,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["陕西长青能源化工有限公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","TM20211018122401834c797","圆钢","φ14mm  Q235B","","kg","50.00","","","","","","L1201从动辊修复"]
["2","TM20211018122401835866b","不锈钢板","钢板δ6,S31603,GB/T4237-2007,","316L","m2","6.00","","","","","","脱硫塔贴补"]
["3","TM20211018122401835291a","无缝碳钢管","DN15 Sch.40    尺寸标准：HG20553(Ia) 20 制造标准：GB/T8163-2008","--煤化工专用","m","54.00","","","","","","密闭取样器新增伴热管线"]
["4","TM202110181224018369455","无缝碳钢管","DN15 Sch.40    尺寸标准：HG20553(Ia) 20 制造标准：GB/T8163-2008","--煤化工专用","m","90.00","","","","","","季度计划"]
["5","TM202110181224018379dd6","无缝碳钢管","DN32 Sch.40（φ42.4*3.6）    HG/T20553(Ia)  20# GB/T8163-2008","","m","120.00","","","","","","F1301燃烧室加护栏、煤浆制备吊装口加护栏"]
["6","TM20211018122401838e228","无缝碳钢管","DN32  Sch.40 （Φ42.4×3.6）     Q235B   GB/T8163-2008","","m","30.00","","","","","","现场整改使用"]
["7","TM20211018122401838e2c7","无缝不锈钢管","DN250 Sch.40   尺寸标准; HG/T20553(IA)  304  制造标准：GB/T14976-2012","","m","1.50","","","","","","硫铵料仓增加旁路管线"]
["8","TM20211018122401839754f","镀锌钢管","DN25  Q235-B热浸锌,GB/T 3091-2008","","m","180.00","","","","","","季度计划"]
["9","TM20211018122401839c8fe","镀锌钢管","DN32  Q235-B热浸锌,GB/T 3091-2008","","m","24.00","","","","","","变换氨水提浓泵改造"]
["10","TM2021101812240184022d7","镀锌角钢","∠50*50*5 热浸锌角钢   Q235B,   GB/T706-2008","","m","6.00","","","","","","变换氨水提浓泵改造"]
["11","TM202110181224018408177","槽钢","[16b   160×65×8.5  Q235B  ,GB707-88,","10.007kg/m","m","30.00","","","","","","现场爬梯整改用"]
["12","TM202110181224018404780","槽钢","[18b   180×70×9  Q235B  ,GB707-88,","22.99kg/m","m","18.00","","","","","","污水集水池提升泵支架"]
["13","TM2021101812240184153f6","圆钢","圆钢φ20,Q235A,GB13013-1991","","m","96.00","","","","","","H1201滚筒筛加高、换热器堵漏"]
["14","TM20211018122401841d2d4","圆钢","圆钢φ22,Q235B,GB13013-1991","","m","6.00","","","","","","加工丝堵，补工程材料"]
["15","TM20211018122401842cdbd","圆钢","圆钢φ16，316L  GB/T1220-2007","","m","60.00","","","","","","季度计划"]
["16","TM202110181224018423e92","扁钢","扁钢30*4,Q235B,GB/T702-2008","","m","60.00","","","","","","季度计划"]
["17","TM20211018122401843cd4b","扁钢","扁钢50X5,Q235B,GB/T702-2008","","m","60.00","","","","","","季度计划"]
["18","TM202110181224018434046","镀锌扁钢","扁钢40*4 热浸锌扁钢, Q235B, GB/T702-2008","","m","60.00","","","","","","季度计划"]
["19","TM20211018122401843feb2","镀锌扁钢","扁钢40*4 热浸锌扁钢, Q235B, GB/T702-2008","","m","120.00","","","","","","F1301燃烧室加护栏、煤浆制备吊装口加护栏"]
["20","TM20211018122401844fcac","不锈钢扁钢","扁钢30*3 304, GB/T702-2008","","m","120.00","","","","","","季度计划"]
["21","TM202110181224018441399","花纹钢板","扁豆 δ5  型花纹钢板, Q235A, GB/T3277-1991,","","m2","90.00","","","","","","季度计划"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]