{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":31,"n_cols":13,"rows_kept":31,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["陕西长青能源化工有限公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","TM20210816112026787751e","24V电源模块","S-25-24 输入：220V AC，输出：24V 1A","","件","3.00","","","","","","煤储运洗车机控制柜电源模块"]
["2","TM20210816112026788dd81","警示灯","NY-01J,功率3W，声音：100-105分贝，光源：LED灯珠发光，发光方式：模拟旋转，安装：强磁吸附安装，充电式","","个","6.00","","","","","","装置断路使用。"]
["3","TM20210816112026788a074","散热风扇","F2E-250B-230 220AC-50HZ 32/31W 0.36/0.4A","上海雷普电气有限公司","个","5.00","","","","","","各变电所低压柜柜后门风扇"]
["4","TM202108161120267892aab","铜接线端子","DT-35","","件","20.00","","","","","","动力密封风机变频改造零星工程，库存2件，已利库，不够用"]
["5","TM20210816112026789685f","铜接线端子","DT-70","","件","30.00","","","","","","动力密封风机变频改造零星工程"]
["6","TM2021081611202678981f2","波力通灯管","FSL YZ10 T8/880 10W","","支","35.00","","","","","","动力DCS系统机柜带灯管故障更换"]
["7","TM20210816112026790bca9","烤肠机","7管 全自动","","台","1.00","","","","","",""]
["8","TM20210816112026790f8c0","饭卡","长青食堂网络程序饭卡","西安佳速游","个","50.00","","","","","","后勤部50"]
["9","TM2021081611202679010d3","无线鼠标","罗技","","个","1.00","","","","","","技术部1"]
["10","TM20210816112026790a6a6","高清网络摄像机","IPD3002；带安装支架","海康威视、大华、烽火科技","台","1.00","","","","","","雨水增加监控摄像头"]
["11","TM20210816112026791aff6","断路器","25A 3P带漏电保护","","个","2.00","","","","","","现场照明箱、插座箱备件"]
["12","TM202108161120267919c47","粉盒","HP M403d 原装","","只","1.00","","","","","","HPM403d 原装  技术部1"]
["13","TM20210816112026791a63a","感温光纤","长度：2000m，探测单元长度：0.5m，供电方式：AC220V/50HZ，执行标准：GB/T 21197-2007 温度分辨率：0.1℃ 温度精度：±1℃，具有内屏蔽层，可应用于强电磁干扰场所，具有高强度挤压护套，抗腐蚀耐磨，系统可以通过RS232\\RS485、内置继电器或其他工业协议等输出形式与PC、消防报警系统等其他控制设备进行联动，可接入盛赛尔火灾探测器系统","甲醇罐区罐体感温光纤更换，DST光纤，单根2000米","m","2000.00","","","","","","甲醇罐区DST感温光纤更换"]
["14","TM202108161120267922e40","防爆断路器","BXD52 2P带漏电保护 16A  ExdeIIct4 Ip65","","只","1.00","","","","","","食堂甲醇泵开关更换，220V，开关与箱子整套。"]
["15","TM202108161120267929875","漏电断路器","DZ47LE-40/4PTN，带漏电保护","","只","3.00","","","","","","厂前区食堂、煤运控制室使用"]
["16","TM2021081611202679342cc","微型断路器","C65H C63A  4P  带漏电保护器一体","","个","6.00","","","","","","厂前区食堂、现场控制室使用"]
["17","TM20210816112026793b588","微型断路器","C40A  2P  带漏电保护一体","","套","6.00","","","","","","厂前区食堂、煤运控制室使用"]
["18","TM20210816112026794025e","三基色灯管","T4 22W 长71.2cm 白光","","支","15.00","","","","","","长青驿站使用"]
["19","TM20210816112026794f164","直流电压表","DS3-NDV300 输入DC0-300V 电源DC48-260V","","只","2.00","","","","","","301总变直流屏更换"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]