{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":29,"n_cols":13,"rows_kept":29,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["陕西长青能源化工有限公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","TM20211218094844546cf9f","固态硬盘","256G(SATA）接口","","块","2.00","","","","","","营销部2"]
["2","TM20211218094844547841a","电脑屏幕支架","22寸屏幕上下双屏，底座式","","个","3.00","","","","","","双屏电脑用"]
["3","TM202112180948445471236","移动硬盘","5TB  USB3.0接口","","块","1.00","","","","","","办公室1"]
["4","TM202112180948445487efc","HDMI转VGA转换器","绿联","","件","1.00","","","","","","畅卫兴计划；150控制室安全预警系统投屏"]
["5","TM20211218094844548fa41","HDMI高清线","20m（标准HDMI接口、接口镀金处理、支持4K/60HZ）","","根","2.00","","","","","","畅卫兴计划；150控制室安区预警系统投屏（标准HDMI接口、接口镀金处理、支持4K/60HZ）"]
["6","TM20211218094844549d823","网线","QS2608  AT305\t 超五类非屏蔽305米/箱","","m","305.00","","","","","","视频监控系统用刘良栋"]
["7","TM20211218094844549befc","多模光纤跳线","ST-ST 2M","","根","2.00","","","","","","动力脱硝控制站"]
["8","TM20211218094844549c892","多模光纤跳线","ST-SC 2M","","根","4.00","","","","","","动力脱硝控制站"]
["9","TM20211218094844550c339","内存条","8G（DDR3）","","个","5.00","","","","","","8G（DDR3）营销部5"]
["10","TM202112180948445509b9c","内存条","8G（DDR4）","","个","1.00","","","","","","8G（DDR4）营销部1"]
["11","TM202112180948445500de8","硒鼓","惠普LP400  LS-CF280A ，","格之格、莱盛、惠普","个","1.00","","","","","","惠普LP400  LS-CF280A    营销部1"]
["12","TM2021121809484455151ad","粉盒","惠普LP400  LS-CF280A ，大容量","格之格、莱盛、惠普","只","1.00","","","","","","惠普LP400  LS-CF280A   营销部1"]
["13","TM202112180948445529c71","粉盒","HP P2015d，大容量","格之格、莱盛、惠普","只","2.00","","","","","","HP P2015d打印机 机动部2"]
["14","TM2021121809484455228cd","粉盒","HPM277DW  红色2 黄色2 青色2，原装大容量","惠普","只","6.00","","","","","","HPM277DW  红色2 黄色2 青色2 / 办公室6  希望原装"]
["15","TM2021121809484455351ef","粉盒","HP Laserjet MFP M277-M231，原装大容量","惠普","只","2.00","","","","","","党群部/原装/HP Laserjet MFP M277-M231"]
["16","TM20211218094844553e59c","粉盒","TOSHIBA  E.STUDIO 2309A","格之格、莱盛、东芝","只","2.00","","","","","","111办公室打印机"]
["17","TM2021121809484455420bc","防爆红外一体机摄像头","600万像素  防爆型 、带云台360度、带ONVIF协议 防爆等级：ExdⅡCT6，Gb/ExtD A21 防护等级：IP68， T80℃ 机械性能材质：304不锈钢表面处理不锈钢原色，可选电抛光，防护等级IP68，水平转动范围0-355°垂直转动范围±90°水平转速6°/sec垂直转速4°/sec接口规格：G-3/4，重量≤28kg，安装方式：壁装，电器性能：输入电压AC220V（模拟流≤2000mA红外距离80/100m波长850","海康威视、浙江大华、武汉烽火","台","2.00","","","","","","视频监控系统用"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]