{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":34,"n_cols":13,"rows_kept":34,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["陕西长青能源化工有限公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","TM202112181018258154b85","防爆电话机","KTH15","","部","1.00","","","","","","灌装站增加消防电话"]
["2","TM20211218101825816099f","刷卡机按键","射频卡计费终端/A111","","套","3.00","","","","","","食堂"]
["3","TM20211218101825816deec","防爆推车式电缆盘","BXX53-2/16/220 220V 1P+N+PE 16A ExdeIICT6Gb WF2 IP66  带两组漏电保护，进线电缆长度50米","","套","2.00","","","","","","防爆区域临时用电使用"]
["4","TM2021121810182581770b8","防爆推车式电缆盘","BXX53-2/16/380 380V 3P+N+PE 16A ExdeIICT6Gb WF2 IP66  带两组漏电保护，进线电缆长度50米","","套","2.00","","","","","","防爆区域临时用电使用"]
["5","TM20211218101825817e01d","饮水机","YL9725W   沁园","","台","5.00","","","","","","技术部1 后勤部4"]
["6","TM20211218101825818f3be","通讯模块","ET200m(1m153-1  153-1AA03-0XBO)","","件","1.00","","","","","","煤运PLC模块更换"]
["7","TM20211218101825818e133","绞肉机","RY-22S  1500W  全不锈钢机头","","台","1.00","","","","","","食堂 不锈钢"]
["8","TM20211218101825818cf03","数字式电容器组保护单元","HWCZB-1（A） AC/DC85～265V 系统电压：100VAC 零序电压：100VAC 采样电流：1A 额定频率：50HZ 10倍额定电流：允许10s  40倍额定电流：允许1s 隔离耐压：4KV","","台","2.00","","","","","","冯家山水库电容器柜保护单元更换，采购时及时与机动部专工沟通"]
["9","TM202112181018258199de2","防爆接线箱","箱体：304不锈钢材质350*250*125，防爆等级Ex-e IIC T4，防护等级IP65，底部进出线 箱体正面带不锈钢位号牌（白底黑字，宋体），带螺栓螺母垫圈等安装附件，接线箱、安装挂耳及用于安装的螺栓螺母垫圈等材质为304SS，接线箱表面进行机械拉丝处理，箱体及箱门壁厚≥1.5±0.1mm，安装挂耳壁厚≥3±0.1mm，箱体抗冲击不小于7JNm，并提供抗冲击测试报告，箱门与箱体密封材料采用无缝对接整片式硅橡胶，","接线端子：2.5mm2，带编号牌，单行排列，带端子固定件，接地：箱体带贯通型黄铜双头螺柱接地组件。堵头：黄铜镀镍，M20x1.5(M)，数量=12-N。接线端子：37个（连续编号，包含12个分屏屏蔽线端子和1个总屏屏蔽线端子） 。电缆口：12进1出  。防爆型电缆密封接头(Ex dIIBT4)，黄铜镀镍材料M20x1.5(M)-G1/2(F)-Φ10，数量=N，用于非铠装电缆；M40x1.5(M)-G1 1/2(F)-Φ24.5， 数量=1，用于非铠装电","套","2.00","","","","","","一级安全标准化整改"]
["10","TM20211218101825819091c","急停按钮","急停开关NP4-11ZS 自锁控制按钮 带蘑菇头自锁保护 一开一闭","热电现场控制柜急停开关损坏更换 技","个","5.00","","","","","","成品甲醇罐、液化气罐进口切断阀增加手动关阀按钮"]
["11","TM20211218101825820c785","电机风叶罩","电机型号：YPSH-132S1-2 5.5KW 50HZ 380/660V 11/6.4A Δ/Y接 2900r/min IP54","","件","1.00","","","","","","动力装置脱硫鼓风机电机零件缺失，原厂家上海电机成套联合有限公司"]
["12","TM2021121810182582042b3","电机风叶罩","电机型号：YX3 132S-4 5.5KW 50HZ 380V 11A 1445r/min IP54","","件","1.00","","","","","","H1201A/B低压油泵电机原厂家佳木斯电机股份有限公司"]
["13","TM20211218101825821f0cd","电机风叶罩","电机型号：YFB3 180L-6WF1 15KW IP55 50HZ 380V 31.8A 防爆标志：DIPA21TAT4","","件","1.00","","","","","","M1104A/B叶轮给煤机电机使用，原厂家佳木斯电机股份有限公司"]
["14","TM2021121810182582136b5","电机风叶罩","电机型号：YBBP3 160M2-8W 5.5KW   IP54 Δ/Y接法 50HZ 380/660V 13.8/7.9A 5HZ-50HZ 720r/min  ExdIIBT4Gb  卧式安装","","件","1.00","","","","","","总变电机库房E2306硫回收蒸汽冷凝器电机零件缺失，原厂家佳木斯电机股份有限公司"]
["15","TM202112181018258229fbe","电机风叶罩","电机型号：YPSH-200L1-2 30KW 50HZ 380/660V 55.4/31.9A 接法Δ/Y 2950r/min IP54","","件","1.00","","","","","","电流装置脱硫引风机零件缺失，原厂家上海电机成套联合有限公司"]
["16","TM20211218101825822896e","电机风叶罩","电机型号：YE3-200L1-6 18.5KW 380V 37.8A 50HZ 985r/min IP55","","件","1.00","","","","","","动力装置动力破渣机零件缺失，原厂家江苏士林电机有限公司"]
["17","TM202112181018258237670","电机风叶罩","电机型号：YB3-225S-4  37KW 50HZ IP55 380/660V70.5/40.6A 1480r/min ExdIIBT4Gb Δ/Y接","","件","1.00","","","","","","C406A均质调节池罗茨风机使用，原厂家安徽皖南电机股份有限公司"]
["18","TM20211218101825823d3b5","电机前轴外小盖","电机型号：YBBP3 160M2-8W 5.5KW   IP54 Δ/Y接法 50HZ 380/660V 13.8/7.9A 5HZ-50HZ 720r/min  ExdIIBT4Gb  卧式安装","","个","1.00","","","","","","总变电机库房E2306硫回收蒸汽冷凝器电机零件缺失，原厂家佳木斯电机股份有限公司"]
["19","TM20211218101825824c397","电机后轴外小盖","电机型号：Y 200L1-2 50HZ IP55 30KW 380V 56A  2950r/min","","个","1.00","","","","","","P22201系列原水泵电机使用，原厂家南阳防爆集团微特电机有限公司"]
["20","TM20211218101825824548a","电机前端盖","电机参数：YBBP3-160M2-8W 5.5KW 380V 13.6A 720r/min         标准编号JB/T7565.1-2004","","个","1.00","","","","","","IP54 Δ/Y接法 50HZ  ExdIIBT4Gb  卧式安装  原厂家佳木斯电机股份有限公司"]
["21","TM20211218101825825dd68","电机接线盒盖","电机型号：YBBP3 160M2-8W 5.5KW   IP54 Δ/Y接法 50HZ 380/660V 13.8/7.9A 5HZ-50HZ 720r/min  ExdIIBT4Gb  卧式安装","","个","1.00","","","","","","总变电机库房E2306硫回收蒸汽冷凝器电机零件缺失，原厂家佳木斯电机股份有限公司"]
["22","TM202112181018258254cc1","电机接线盒盖","电机型号：YB3 112M-2 4KW  IP54 50HZ 400V 7.5A 2868r/min  ExdIIBT4Gb","","个","1.00","","","","","","动力装置P4307集水自吸泵电机零件缺失，原厂家佳木斯电机股份有限公司"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]