{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":58,"n_cols":13,"rows_kept":58,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["陕西长青能源化工有限公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","TM202110250802501395aa4","平头螺丝","M6×80 ，不锈钢，全螺纹，带配套螺母","","套","10.00","","","","","","硫铵包装机用"]
["2","TM20211025080250140a95c","玻璃刀","3# (8803)","","把","2.00","","","","","","消防队"]
["3","TM20211025080250140c85c","广口塑料瓶","250ml","","只","25.00","","","","","",""]
["4","TM202110250802501417823","美纹纸胶带","50mm*50m","","盘","50.00","","","","","","消防队"]
["5","TM20211025080250141d493","镀锌管帽","DN25","","个","10.00","","","","","","全厂水暖管线"]
["6","TM202110250802501411303","不锈钢铜芯把手锁","MS308-3","","个","9.00","","","","","","干渣机现场控制柜、脱硝照明柜、布袋除尘控制柜等现场电控柜使用，常用备件"]
["7","TM20211025080250142a69d","反光漆","白","","kg","40.00","","","","","","消防队"]
["8","TM202110250802501421577","黏胶去除剂","BK810  500ml/瓶","","瓶","3.00","","","","","","消防队"]
["9","TM2021102508025014240e3","脚踏式垃圾桶","长48.5CM/宽47CM/高84CM，食堂用/100L 带轮子","","只","1.00","","","","","","食堂用/100L 带轮子"]
["10","TM202110250802501435458","中性笔","0.5  长青办公用品发放","","支","20.00","","","","","","服务队20"]
["11","TM20211025080250143b242","中性笔芯","0.5  长青办公用品发放","","支","184.00","","","","","","服务队40  技术部24  机动部120"]
["12","TM202110250802501437349","电力安全工具柜","高2000mm*宽1200mm*深600mm,柜内具有不锈钢接地线架，五层间隔，柜子材质厚1mm，表面有玻璃，双开门","","件","2.00","","","","","","301总变"]
["13","TM202110250802501435019","订书针","办公用品发放","","盒","3.00","","","","","","服务队3"]
["14","TM202110250802501441610","磁铁","办公用品发放","","个","20.00","","","","","","服务队20"]
["15","TM2021102508025014458a6","长尾夹","25mm","","盒","2.00","","","","","","服务队2"]
["16","TM2021102508025014462ec","电缆绝缘支架","高度58cm，槽内8.5cm，卡扣款，三面标语支架，PVC材质加厚版， GB/EX tD A21  T80℃","","个","30.00","","","","","","临时电缆不落地支架（一级标准化检查要求）"]
["17","TM2021102508025014494ce","安全警示贴","印刷字体：当心触电，带触电标识 规格：30mm*30mm 材质：PVC 背面带胶 厚度0.8mm 防晒","-长青","个","500.00","","","","","","全厂配电箱、电源箱粘贴"]
["18","TM20211025080250145c3bb","安全警示贴","印刷字体：当心触电，带触电标识 规格：50mm*50mm 材质：PVC 背面带胶 厚度0.8mm 防晒","-长青","个","400.00","","","","","","全厂配电箱、电源箱粘贴"]
["19","TM2021102508025014535ba","安全警示贴","印刷字体：当心触电，带触电标识 规格：80mm*80mm 材质：PVC 背面带胶 厚度0.8mm 防晒","-长青","个","300.00","","","","","","全厂配电箱、电源箱粘贴"]
["20","TM202110250802501455681","钥匙箱","24位，200*60*310mm","","个","3.00","","","","","","变电所“6S”整改"]
["21","TM202110250802501468379","炒菜勺子","14.6cm*50.8cm，/木手柄","","个","5.00","","","","","","食堂用/木手柄"]
["22","TM2021102508025014628b7","牙签","1000/包","","包","2.00","","","","","","食堂用"]
["23","TM2021102508025014623fc","一次性包装牙签","一次性纸袋密封单独包装2根牙签，带有图案，不带字体","","件","1.00","","","","","","食堂招待用"]
["24","TM20211025080250146f7f9","柜子多层收纳架","可伸缩，宽度：42cm，长度：28.5-36cm，高：33cm  材质：不锈钢+PP","","个","4.00","","","","","","气化 员工柜子使用"]
["25","TM20211025080250147d02c","锅刷","竹制，长度30cm","","把","4.00","","","","","","食堂用/长度30cm"]
["26","TM202110250802501474194","牙签筒（陶瓷）","4.8×4.8×7cm","","个","4.00","","","","","","食堂招待用"]
["27","TM20211025080250147090d","吸料机","加厚不锈钢，管子直径：φ160   长9米，配电机型号为：YE2-112M-4  380V  4.0KW  1440r/min  8.8A  △  IP55  F","","台","1.00","","","","","","供水班掏树脂用"]
["28","TM20211025080250148f3fb","磁性白板","需喷绘表格（样式内容见附件，制作前确定样式）双面磁性、可擦、可挂式白板 90*120，","","块","1.00","","","","","","供水 氯酸钠间记录用  白板内容见附件  可不带磁性"]
["29","TM2021102508025014855db","磁条","蓝色，内置橡胶磁条，优质ABS塑料，强力不脱磁，长度20cm","","个","70.00","","","","","","部门张贴文件用  蓝色，内置橡胶磁条，优质ABS塑料，强力不脱磁，长度20cm"]
["30","TM20211025080250148a07e","O型密封圈","Φ250×4.0丁腈橡胶  GB/T 3452.1-2005","","件","2.00","","","","","","动力磨煤机进口混合风门气缸用密封圈"]
["31","TM20211025080250149e96c","LBH密封圈","内圆：235mm，外圆：238mm，内圈高：16mm，外圈高：14.2mm，内外圈间隙：3mm，内圈厚：3mm，外圈厚：2mm，材质：氟橡胶","","件","2.00","","","","","","动力磨煤机进口混合风门气缸用密封圈"]
["32","TM2021102508025014925d9","密封胶条","材质：氟橡胶，宽52mm×厚9mm，耐受温度：250℃，耐腐蚀","","m","20.00","","","","","","动力引风机出口烟道插板阀阀板用密封胶条"]
["33","TM202110250802501499b1e","聚氨酯阻燃卷材","CPU-101 厚度0.6mm  宽度500mm，（需附检测报告）","","m2","50.00","","","","","","现场保冷维护"]
["34","TM20211025080250149192a","气瓶固定架","8L气瓶，四瓶固定支架，高度60cm，底板90cm*20cm，进口直径18cm,颜色：白色。","","个","7.00","","","","","","全厂分析小屋固定气瓶用"]
["35","TM20211025080250150879a","直通终端锥管接头","D0=12 NPT3/8 材质06Cr19Ni10 耐压6.4MPa","","个","2.00","","","","","","K2201用于充氮回气"]
["36","TM20211025080250150748b","直通终端锥管接头","D0=14 NPT3/8 材质06Cr19Ni10 耐压6.4MPa","","个","2.00","","","","","","K2201用于填料进回水"]
["37","TM2021102508025015061e9","直通终端接头","NPT1/2-27×3  材质20 耐压6.4MPa","","个","2.00","","","","","","K2201二级气缸缸盖循环水进/出口"]
["38","TM202110250802501515729","直通终端接头","NPT3/4-42×3.5  材质20 耐压6.4MPa","","个","2.00","","","","","","K2201二级气缸缸体循环水进/出口"]
["39","TM20211025080250151aad0","直通终端接头","NPT1-21×3   材质20 耐压6.4MPa","","个","4.00","","","","","","K2201填料冷却水进/出水分管"]
["40","TM20211025080250151470e","弯通终端接头","D0=12 NPT3/8 材质06Cr19Ni10 耐压6.4MPa","","个","2.00","","","","","","K2201用于充氮回气"]
["41","TM2021102508025015249a7","弯通终端接头","D0=14 NPT3/8 材质06Cr19Ni10 耐压6.4MPa","","个","2.00","","","","","","K2201用于填料进回水"]
["42","TM202110250802501529fe1","外螺纹针型阀","J23W-160P DN10   316","","只","2.00","","","","","","P23A01AD"]
["43","TM202110250802501522f3c","六角头螺栓","M12*1.25*20全螺纹,316L,HG/T20634-2009","","个","30.00","","","","","","动力引风机出口烟道插板阀阀板密封胶条压板用螺栓。"]
["44","TM20211025080250152cca5","全螺纹螺栓带母","M82*3*550    8.8级  带管法兰专用螺母M82 35CrMoA/30CrMo HG/T20634-2009","","套","6.00","","","","","","C1301工艺气进口法兰螺栓"]
["45","TM20211025080250153359d","粘接剂","迪普特粘接剂，SC2008，1kg/听，含固化剂","","kg","2.00","","","","","","皮带日常维护，1、目前使用的力普特粘接剂使用效果不理想；2、粘接剂品牌繁多，质量参差不齐，质量好坏对设备平稳运行有较大影响，故指定品牌。"]
["46","TM202110250802501535b44","定制鼠标垫","800mm*350mm*4mm","","个","8.00","","","","","","材质：皮革  301总变、发电机岗位鼠标垫。定制内容见附表"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]