{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":61,"n_cols":13,"rows_kept":61,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["陕西长青能源化工有限公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","TM202112070828334050ead","不锈钢螺母","5，M5,304 HG20634-1997，配套弹垫、平垫，","","十只","20.00","","","","","","M5,304 HG20634-1997，配套弹垫、平垫，现场防静电跨接线、接地线螺母生锈更换"]
["2","TM2021120708283340650c6","不锈钢六角螺母","10，M10,304 HG20634-1997，配套弹垫、平垫，","","十只","50.00","","","","","","M10,304 HG20634-1997，配套弹垫、平垫，现场防静电跨接线、接地线螺母生锈更换"]
["3","TM20211207082833407f138","不锈钢螺母","12，M12,304 HG20634-1997，配套弹垫、平垫","","十只","14.00","","","","","","M12,304 HG20634-1997，配套弹垫、平垫，现场防静电跨接线、接地线螺母生锈更换"]
["4","TM202112070828334075562","不锈钢螺母","14，M14,304 HG20634-1997，配套弹垫、平垫，","","十只","20.00","","","","","","M14,304 HG20634-1997，配套弹垫、平垫，现场防静电跨接线、接地线螺母生锈更换"]
["5","TM2021120708283340703ac","插板固定双面胶","长5m×宽5cm×厚度2mm   透明色，纳米强力胶","","卷","1.00","","","","","","财务部1"]
["6","TM20211207082833408d599","消防钉","25#（钉长25mm,底部直径7.5mm,顶部直径16mm）","","个","500.00","","","","","","现场标识牌安装使用"]
["7","TM2021120708283340865ab","消防钉","32#（钉长32mm,底部直径8.5mm,顶部直径20mm）","","个","500.00","","","","","","现场标识牌安装使用"]
["8","TM202112070828334083424","U型管卡","DN15  1/4\"  Ф20  304  带双螺母","","个","50.00","","","","","","常用"]
["9","TM20211207082833409015c","金属镀锌电缆桥架线槽（含盖板）","宽100mm*高100mm*厚1mm 热镀锌金属槽盒（配套盖板及附件）长2米","","m","50.00","","","","","","部分装置区桥架腐蚀更换"]
["10","TM202112070828334097ed3","反光漆","黄","","kg","40.00","","","","","","消防队胡"]
["11","TM202112070828334091d97","硅胶专用速干胶","5562 粘接金属（表面有油漆）和硅胶 20g/支","","支","100.00","","","","","","储罐踏步，要求水性"]
["12","TM202112070828334101995","小便器","壁挂式(联排式)冲水方式：感应式；排水方式：挂壁地排式；尺寸：290*130*600mm；出水口离地高度：1340mm，配感应器及安装所必须的配件。","","件","1.00","","","","","","机修楼卫生间"]
["13","TM2021120708283341044a3","复印纸（打印纸）","A3 500张*5包/箱","","箱","4.00","","","","","","生产部3  技术部1"]
["14","TM20211207082833410dbf4","警戒绳","盘式50米","","个","15.00","","","","","","消防队胡"]
["15","TM20211207082833411d4bd","蓝黑墨水","英雄 60ml","","瓶","2.00","","","","","","办公室2"]
["16","TM20211207082833411dc3e","档案盒","310*220*40（牛皮纸）","","个","20.00","","","","","","库房整理资料用"]
["17","TM20211207082833411d9a9","内存条","DDR31600 4G台式","","个","1.00","","","","","","DDR31600 4G台式  财务部1"]
["18","TM20211207082833412f1d3","尺子","40cm","","把","1.00","","","","","","40cm  财务部1"]
["19","TM20211207082833412919e","信封","办公用品发放","","包","1.00","","","","","","牛皮纸颜色  50个  环保部50个"]
["20","TM2021120708283341298d3","长把铁簸箕","","","个","10.00","","","","","","各班组打扫卫生用"]
["21","TM20211207082833413e4c6","物品标识贴","圆形：直径5cm,厚度0.45mm. 蓝色  材质：PVC磨砂","","个","20.00","","","","","","鼠标贴  生产部20"]
["22","TM20211207082833413a25e","危险废弃物标志牌","200*200*2mm 反光贴，带危废标志，废油、废试剂，废催化剂，废油桶、试剂瓶，废树脂","","块","100.00","","","","","","化学名称：废试剂瓶，：醒目的橘黄色，危险类别标识为有毒标识"]
["23","TM20211207082833414dca2","饭卡","长青食堂网络程序饭卡","西安佳速游","个","50.00","","","","","","食堂用"]
["24","TM2021120708283341440d2","亚克力A4插盒","单层竖款","210*297","个","25.00","","","","","","保洁用"]
["25","TM202112070828334143f15","翻饼竹板","90*3cm","","个","2.00","","","","","","食堂用"]
["26","TM20211207082833415d745","硅胶U型密封条","高≥30mm 可卡厚度3mm  白色或透明","","m","400.00","","","","","","储罐踏步"]
["27","TM2021120708283341571d1","消防救援三角架","多功能便携消防救援三角架  伸缩起重电动葫芦支架，全套1800磅，双向自锁手摇绞盘     材质：铝合金","","件","2.00","","","","","","供水 地井受限空间用"]
["28","TM20211207082833416eba0","围脖","热虹吸温控技术，高弹性棉纶面料，3D编织，吸湿排汗","","个","14.00","","","","","","营销部"]
["29","TM202112070828334160a40","护膝","帆布","","付","14.00","","","","","","营销部"]
["30","TM202112070828334162a02","直角弯头","ZG3/4\"","","件","20.00","","","","","","技改工程用"]
["31","TM20211207082833417d37d","长柄尼龙地板刷","40CM","","支","3.00","","","","","","食堂用"]
["32","TM202112070828334173156","密封胶条","材质：氟橡胶，宽52mm×厚9mm，耐受温度：250℃，耐腐蚀","","m","18.00","","","","","","动力3台锅炉布袋除尘器旁通阀检修"]
["33","TM202112070828334178afc","钢丝骨架复合PE管","dn50*4.5，PN1.6Mpa，黑色+蓝条，CJ/T189-2007","","m","18.00","","","","","","零星工程：煤储运生活水PE管更换"]
["34","TM20211207082833418bb81","钢丝骨架复合PE电熔直通接头","dn50*4.5   PN1.6Mpa  黑色+蓝条   CJ/T189-2007","","件","4.00","","","","","","零星工程：煤储运生活水PE管更换"]
["35","TM20211207082833418aa97","钢丝骨架复合PE电熔90度弯头","dn50   PN1.6Mpa  黑色   CJ/T189-2007","","件","6.00","","","","","","零星工程：煤储运生活水PE管更换"]
["36","TM20211207082833418ad5c","玻璃钢管","DN65-PN16，RF，乙烯基，HG/T21633-1991  长丝缠绕玻璃钢管道（含碳化硅防磨层厚度2.5mm）","","m","3.00","","","","","","脱硫事故返回管线漏检修"]
["37","TM2021120708283341901c5","玻璃钢管","DN80-PN16，RF，乙烯基，HG/T21633-1991  长丝缠绕玻璃钢管道（含碳化硅防磨层厚度2.5mm）","","m","1.00","","","","","","脱硫后系统浆液管线用"]
["38","TM202112070828334198b57","玻璃钢等径三通","DN65-PN16，RF，乙烯基，HG/T21633-1991  长丝缠绕玻璃钢管道（含碳化硅防磨层厚度2.5mm）","","件","1.00","","","","","","事故返回泵出口管线用"]
["39","TM20211207082833419d513","玻璃钢等径三通","DN65-PN16，RF，乙烯基，HG/T21633-1991  长丝缠绕玻璃钢管道（含碳化硅防磨层厚度2.5mm）","","件","1.00","","","","","","脱硫事故返回管线漏检修"]
["40","TM202112070828334206474","玻璃钢法兰","DN65-PN16，RF，乙烯基，HG/T21633-1991  长丝缠绕玻璃钢管道（含碳化硅防磨层厚度2.5mm）","","件","2.00","","","","","","事故返回泵出口管线用"]
["41","TM202112070828334207471","玻璃钢法兰","DN65-PN16，RF，乙烯基，HG/T21633-1991  长丝缠绕玻璃钢管道（含碳化硅防磨层厚度2.5mm）","","件","4.00","","","","","","脱硫事故返回管线漏检修"]
["42","TM202112070828334216e13","玻璃钢法兰","DN80-PN16，RF，乙烯基，HG/T21633-1991  长丝缠绕玻璃钢管道（含碳化硅防磨层厚度2.5mm）","","件","2.00","","","","","","脱硫后系统浆液管线用"]
["43","TM202112070828334212a18","球阀保护套","DN25 PN16 PVC 透明","","个","8.00","","","","","","硫回收阀门保护"]
["44","TM20211207082833422f7e4","球阀保护套","DN40 PN16 PVC 透明","","个","8.00","","","","","","硫回收阀门保护"]
["45","TM202112070828334221244","球阀保护套","DN50 PN16 PVC 透明","","个","15.00","","","","","","硫回收阀门保护"]
["46","TM20211207082833422f469","快插终端接头","1/4NPT-φ10","","件","10.00","","","","","","气化P1302隔膜阀用"]
["47","TM20211207082833423395b","螺栓/螺母","G1-1/8×200 35CrMo/30CrMo ASME B18.31.2（美标双头）","","套","12.00","","","","","","工艺气止逆阀顶盖螺栓"]
["48","TM20211207082833423fe1c","快插中间接头","∮8.","","个","20.00","","","","","","全厂水系统气动阀用"]
["49","TM202112070828334244e8f","胶木连杆","隔离开关型号：GN22-12用","仪征市爱特电器有限公司","根","12.00","","","","","","总变大容量开关操作机构胶木连杆"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]