{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":117,"n_cols":13,"rows_kept":117,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["江苏徐矿能源股份有限公司张双楼煤矿物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","TM20250609165305953e829","移机","1.5P挂机","1.5P挂机","台","1.00","","","","","",""]
["2","TM20250609165305955f26f","拆机","1.5P挂机","1.5P挂机","台","1.00","","","","","",""]
["3","TM2025060916530595677d6","装机","1.5P挂机","1.5P挂机","台","1.00","","","","","",""]
["4","TM20250609165305957edb1","维修电脑板","1.5P挂机","1.5P挂机","台","1.00","","","","","",""]
["5","TM20250609165305957c653","更换电脑板","1.5P挂机","1.5P挂机","台","1.00","","","","","",""]
["6","TM20250609165305958caec","漏水处理","1.5P挂机","1.5P挂机","台","1.00","","","","","",""]
["7","TM2025060916530595922a9","加长铜管","1.5P挂机","1.5P挂机","米","1.00","","","","","",""]
["8","TM2025060916530596050bc","更换传感器","1.5P挂机","1.5P挂机","台","1.00","","","","","",""]
["9","TM202506091653059607f00","更换四通阀","1.5P挂机","1.5P挂机","台","1.00","","","","","","含加氟"]
["10","TM20250609165305961eed9","更换交流接触器","1.5P挂机","1.5P挂机","台","1.00","","","","","",""]
["11","TM202506091653059624fd6","外机支架","1.5P挂机","1.5P挂机","台","1.00","","","","","",""]
["12","TM20250609165305962e122","加氟","1.5P挂机","1.5P挂机","台","1.00","","","","","",""]
["13","TM2025060916530596398d8","补氟","1.5P挂机","1.5P挂机","兆帕","1.00","","","","","",""]
["14","TM202506091653059643bd6","简单清洗","1.5P挂机","1.5P挂机","台","1.00","","","","","","对内机的蒸发器翅片、过滤网、外壳等部件尘埃污物的清洗；对风叶、外壳等部件尘埃污物的清洗"]
["15","TM202506091653059648825","深度清洗","1.5P挂机","1.5P挂机","台","1.00","","","","","","对内机的蒸发器内部部件、外机的冷凝器翅片、风叶、过滤网及外壳部件表面的深度清洗。"]
["16","TM20250609165305965f332","更换内风机电机","1.5P挂机","1.5P挂机","台","1.00","","","","","",""]
["17","TM202506091653059660b7e","更换外风机电机","1.5P挂机","1.5P挂机","台","1.00","","","","","",""]
["18","TM20250609165305966e2b4","移机","3P柜机","3P柜机","台","1.00","","","","","",""]
["19","TM20250609165305967889c","拆机","3P柜机","3P柜机","台","1.00","","","","","",""]
["20","TM20250609165305968431f","装机","3P柜机","3P柜机","台","1.00","","","","","",""]
["21","TM202506091653059688e10","维修内机电脑板","3P柜机","3P柜机","台","1.00","","","","","",""]
["22","TM202506091653059693a5b","维修外内电脑板","3P柜机","3P柜机","台","1.00","","","","","",""]
["23","TM202506091653059697afa","更换内机电脑板","3P柜机","3P柜机","台","1.00","","","","","",""]
["24","TM20250609165305970af58","更换外内电脑板","3P柜机","3P柜机","台","1.00","","","","","",""]
["25","TM202506091653059717152","漏水处理","3P柜机","3P柜机","台","1.00","","","","","",""]
["26","TM20250609165305971a36d","加长铜管","3P柜机","3P柜机","米","1.00","","","","","",""]
["27","TM202506091653059723d3b","更换传感器","3P柜机","3P柜机","台","1.00","","","","","",""]
["28","TM20250609165305972ae79","更换四通阀","3P柜机","3P柜机","台","1.00","","","","","","含加氟"]
["29","TM20250609165305973a62c","更换交流接触器","3P柜机","3P柜机","台","1.00","","","","","",""]
["30","TM202506091653059745cba","外机支架","3P柜机","3P柜机","台","1.00","","","","","",""]
["31","TM202506091653059744c8c","加氟","3P柜机","3P柜机","台","1.00","","","","","",""]
["32","TM20250609165305975c230","补氟","3P柜机","3P柜机","兆帕","1.00","","","","","",""]
["33","TM20250609165305975df95","简单清洗","3P柜机","3P柜机","台","1.00","","","","","","对内机的蒸发器翅片、过滤网、外壳等部件尘埃污物的清洗；对风叶、外壳等部件尘埃污物的清洗"]
["34","TM202506091653059767b77","深度清洗","3P柜机","3P柜机","台","1.00","","","","","","对内机的蒸发器内部部件、外机的冷凝器翅片、风叶、过滤网及外壳部件表面的深度清洗。"]
["35","TM20250609165305977b604","更换内风机电机","3P柜机","3P柜机","台","1.00","","","","","",""]
["36","TM20250609165305977194d","更换外风机电机","3P柜机","3P柜机","台","1.00","","","","","",""]
["37","TM20250609165305978bc49","移机","5P柜机","5P柜机","台","1.00","","","","","",""]
["38","TM202506091653059791a07","拆机","5P柜机","5P柜机","台","1.00","","","","","",""]
["39","TM2025060916530597947fd","装机","5P柜机","5P柜机","台","1.00","","","","","",""]
["40","TM20250609165305980da28","维修内机电脑板","5P柜机","5P柜机","台","1.00","","","","","",""]
["41","TM202506091653059815cad","维修外内电脑板","5P柜机","5P柜机","台","1.00","","","","","",""]
["42","TM20250609165305981c58e","更换内机电脑板","5P柜机","5P柜机","台","1.00","","","","","",""]
["43","TM20250609165305982772a","更换外内电脑板","5P柜机","5P柜机","台","1.00","","","","","",""]
["44","TM2025060916530598283b4","漏水处理","5P柜机","5P柜机","台","1.00","","","","","",""]
["45","TM20250609165305983eef2","加长铜管","5P柜机","5P柜机","米","1.00","","","","","",""]
["46","TM2025060916530598468ab","更换传感器","5P柜机","5P柜机","台","1.00","","","","","",""]
["47","TM202506091653059858794","更换四通阀","5P柜机","5P柜机","台","1.00","","","","","","含加氟"]
["48","TM20250609165305985a329","更换交流接触器","5P柜机","5P柜机","台","1.00","","","","","",""]
["49","TM20250609165305986662e","外机支架","5P柜机","5P柜机","台","1.00","","","","","",""]
["50","TM20250609165305987848c","加氟","5P柜机","5P柜机","台","1.00","","","","","",""]
["51","TM202506091653059874fbf","补氟","5P柜机","5P柜机","兆帕","1.00","","","","","",""]
["52","TM202506091653059882c62","简单清洗","5P柜机","5P柜机","台","1.00","","","","","","对内机的蒸发器翅片、过滤网、外壳等部件尘埃污物的清洗；对风叶、外壳等部件尘埃污物的清洗"]
["53","TM20250609165305988c33b","深度清洗","5P柜机","5P柜机","台","1.00","","","","","","对内机的蒸发器内部部件、外机的冷凝器翅片、风叶、过滤网及外壳部件表面的深度清洗。"]
["54","TM2025060916530598921ed","更换内风机电机","5P柜机","5P柜机","台","1.00","","","","","",""]
["55","TM20250609165305990c2a7","更换外风机电机","5P柜机","5P柜机","台","1.00","","","","","",""]
["56","TM20250609165305990348b","移机","10匹","10匹","台","1.00","","","","","",""]
["57","TM202506091653059914627","拆机","10匹","10匹","台","1.00","","","","","",""]
["58","TM202506091653059928c48","装机","10匹","10匹","台","1.00","","","","","",""]
["59","TM2025060916530599231e6","维修内机电脑板","10匹","10匹","台","1.00","","","","","",""]
["60","TM202506091653059938317","维修外机电脑板","10匹","10匹","台","1.00","","","","","",""]
["61","TM20250609165305993c239","更换内机电脑板","10匹","10匹","台","1.00","","","","","",""]
["62","TM20250609165305994e8fb","更换外机电脑板","10匹","10匹","台","1.00","","","","","",""]
["63","TM202506091653059959068","漏水处理","10匹","10匹","台","1.00","","","","","",""]
["64","TM202506091653059958fc3","加长铜管","10匹","10匹","米","1.00","","","","","",""]
["65","TM202506091653059961891","更换传感器","10匹","10匹","台","1.00","","","","","",""]
["66","TM202506091653059968c6b","更换四通阀","10匹","10匹","台","1.00","","","","","","含加氟"]
["67","TM202506091653059971fc0","更换交流接触器","10匹","10匹","台","1.00","","","","","",""]
["68","TM202506091653059971f47","外机支架","10匹","10匹","台","1.00","","","","","",""]
["69","TM202506091653059987fb7","加氟","10匹","10匹","台","1.00","","","","","",""]
["70","TM20250609165305999f7ef","补氟","10匹","10匹","兆帕","1.00","","","","","",""]
["71","TM2025060916530599918ef","简单清洗","10匹","10匹","台","1.00","","","","","","对内机的蒸发器翅片、过滤网、外壳等部件尘埃污物的清洗；对风叶、外壳等部件尘埃污物的清洗"]
["72","TM202506091653060005dfa","深度清洗","10匹","10匹","台","1.00","","","","","","对内机的蒸发器内部部件、外机的冷凝器翅片、风叶、过滤网及外壳部件表面的深度清洗。"]
["73","TM202506091653060018e68","更换内风机电机","10匹","10匹","台","1.00","","","","","",""]
["74","TM20250609165306001541b","更换外风机电机","10匹","10匹","台","1.00","","","","","",""]
["75","TM202506091653060022297","管路清洗","10匹","10匹","台","1.00","","","","","",""]
["76","TM20250609165306002c737","移机","10匹以上","10匹以上","台","1.00","","","","","",""]
["77","TM20250609165306003d821","拆机","10匹以上","10匹以上","台","1.00","","","","","",""]
["78","TM20250609165306003cb95","装机","10匹以上","10匹以上","台","1.00","","","","","",""]
["79","TM202506091653060049c34","维修外机电脑板","10匹以上","10匹以上","台","1.00","","","","","",""]
["80","TM20250609165306004f035","维修内机电脑板","10匹以上","10匹以上","台","1.00","","","","","",""]
["81","TM20250609165306005f2fa","更换外机电脑板","10匹以上","10匹以上","台","1.00","","","","","",""]
["82","TM202506091653060056d81","更换内机电脑板","10匹以上","10匹以上","台","1.00","","","","","",""]
["83","TM2025060916530600683ba","漏水处理","10匹以上","10匹以上","台","1.00","","","","","",""]
["84","TM20250609165306006c413","加长铜管","10匹以上","10匹以上","米","1.00","","","","","",""]
["85","TM202506091653060070921","更换传感器","10匹以上","10匹以上","台","1.00","","","","","",""]
["86","TM202506091653060085e81","更换四通阀","10匹以上","10匹以上","台","1.00","","","","","","含加氟"]
["87","TM20250609165306008e68b","更换交流接触器","10匹以上","10匹以上","台","1.00","","","","","",""]
["88","TM202506091653060094c1c","外机支架","10匹以上","10匹以上","台","1.00","","","","","",""]
["89","TM2025060916530600934a0","加氟","10匹以上","10匹以上","台","1.00","","","","","",""]
["90","TM2025060916530601036f5","补氟","10匹以上","10匹以上","兆帕","1.00","","","","","",""]
["91","TM202506091653060103ba7","内机清洗","10匹以上","10匹以上","台","1.00","","","","","",""]
["92","TM202506091653060116f3d","拆机清洗","10匹以上","10匹以上","台","1.00","","","","","",""]
["93","TM202506091653060110b87","更换内风机电机","10匹以上","10匹以上","台","1.00","","","","","",""]
["94","TM2025060916530601213f8","更换外风机电机","10匹以上","10匹以上","台","1.00","","","","","",""]
["95","TM202506091653060124eba","管路清洗","10匹以上","10匹以上","台","1.00","","","","","",""]
["96","TM20250609165306013022b","更换风机电容","格力原厂","格力原厂","台","1.00","","","","","",""]
["97","TM202506091653060133ccf","更换压缩机电容","格力原厂","格力原厂","台","1.00","","","","","",""]
["98","TM2025060916530601453cc","更换变压器","格力原厂","格力原厂","个","1.00","","","","","",""]
["99","TM20250609165306014fe0f","更换信号控制连接线","通用","通用","根","1.00","","","","","",""]
["100","TM20250609165306015dfe6","更换内外机连接电源线","通用","通用","根","1.00","","","","","",""]
["101","TM20250609165306015ba14","万能遥控器","通用","通用","个","1.00","","","","","",""]
["102","TM202506091653060169810","原厂遥控器","格力原厂","格力原厂","个","1.00","","","","","",""]
["103","TM2025060916530601628e4","漏电保护器","格力原厂","格力原厂","个","1.00","","","","","",""]
["104","TM202506091653060171074","漏点焊接修复","通用","通用","点","1.00","","","","","",""]
["105","TM202506091653060184a18","吊车","吊车","吊车","台班","1.00","","","","","",""]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]