{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":43,"n_cols":13,"rows_kept":43,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["苏能（锡林郭勒）发电有限公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","TM202508040942503210365","密封环","150XHPR-52B","","个","1.00","","","","","","锅炉——低温凝结水升压泵"]
["2","TM20250804094250322c775","密封环","200XHPR-54B","","个","1.00","","","","","","锅炉——高温凝结水升压泵"]
["3","TM20250804094250323032d","滤芯","CNAXIATT06/E10/80/120L","","个","4.00","","","","","","锅炉——磨煤机润滑油站"]
["4","TM20250804094250324b7ae","滤芯","CNAX/ATT06/F10/400/10/L","","个","4.00","","","","","","锅炉——磨煤机液压油站作用力"]
["5","TM20250804094250325e42e","密封环","300XHPR-48B","","个","1.00","","","","","","锅炉——热媒水循环泵"]
["6","TM20250804094250326c2b1","溢流阀","CNAX/PV03/2T/S1/N1/20/100","","个","2.00","","","","","","锅炉——磨煤机液压油站"]
["7","TM2025080409425032614ab","反作用力过滤器滤芯","CNAX/ATT06/F10/160/10/L","","个","2.00","","","","","","锅炉——磨煤机液压油站"]
["8","TM20250804094250327f655","弯头","￠108×4    90°碳钢弯头","","个","10.00","","","","","","灰硫——管道替换使用"]
["9","TM20250804094250328f169","圆盘排气阀","DN65   PG10（400℃）","","台","2.00","","","","","","灰硫——气力输灰用（江苏苏达）"]
["10","TM20250804094250329dfdb","拷贝淋","DN40  材质：UPVC","","个","10.00","","","","","","化学——日常维护"]
["11","TM202508040942503306661","拷贝淋","DN50、材质：UPVC","","个","10.00","","","","","","化学——日常维护"]
["12","TM202508040942503303d2e","拷贝淋","DN40-48  材质：不锈钢","","个","100.00","","","","","","化学——日常维护"]
["13","TM20250804094250331b9fc","篮式过滤器","\"滤芯 SBL-25C/100\"","","套","1.00","","","","","","锅炉——脱硝系统生产用"]
["14","TM20250804094250332d204","篮式过滤器","\"滤芯 SBL-10P/100\"","","套","1.00","","","","","","锅炉——脱硝系统生产用"]
["15","TM2025080409425033363d8","Y型过滤器","\"滤芯 GL41W-10P/20\"","","套","1.00","","","","","","锅炉——脱硝系统生产用"]
["16","TM202508040942503335873","Y型过滤器","\"滤芯 GL41W-10P/25\"","","套","1.00","","","","","","锅炉——脱硝系统生产用"]
["17","TM20250804094250334dfa9","Y型过滤器","\"滤芯 GL41W-10P/40\"","","套","1.00","","","","","","锅炉——脱硝系统生产用"]
["18","TM20250804094250346d42a","金属缠绕垫","\"DN15 20*50*4\"","","片","5.00","","","","","","锅炉——脱硝系统生产用"]
["19","TM20250804094250347641e","金属缠绕垫","\"DN20 25*55*4\"","","片","5.00","","","","","","锅炉——脱硝系统生产用"]
["20","TM202508040942503487be7","金属缠绕垫","\"DN25 32*65*4\"","","片","5.00","","","","","","锅炉——脱硝系统生产用"]
["21","TM20250804094250349ef88","金属缠绕垫","\"DN32 38*78*4\"","","片","5.00","","","","","","锅炉——脱硝系统生产用"]
["22","TM20250804094250349055f","金属缠绕垫","\"DN40 45*85*4\"","","片","10.00","","","","","","锅炉——脱硝系统生产用"]
["23","TM20250804094250350da0c","金属缠绕垫","\"DN50 57*100*4\"","","片","10.00","","","","","","锅炉——脱硝系统生产用"]
["24","TM20250804094250351ce09","金属缠绕垫","\"DN65 76*140*4\"","","片","10.00","","","","","","锅炉——脱硝系统生产用"]
["25","TM202508040942503528325","金属缠绕垫","\"DN80 89*135*4\"","","片","10.00","","","","","","锅炉——脱硝系统生产用"]
["26","TM20250804094250352dd7c","金属缠绕垫","\"DN100 108*155*4\"","","片","10.00","","","","","","锅炉——脱硝系统生产用"]
["27","TM20250804094250353a1fa","金属缠绕垫","\"DN125 133*185*4\"","","片","10.00","","","","","","锅炉——脱硝系统生产用"]
["28","TM202508040942503542df8","金属缠绕垫","\"DN150 170*218*4\"","","片","5.00","","","","","","锅炉——脱硝系统生产用"]
["29","TM20250804094250355e05d","金属缠绕垫","\"DN200 222*273*4\"","","片","5.00","","","","","","锅炉——脱硝系统生产用"]
["30","TM202508040942503555dce","机械密封","65XHPR-55-10（集成式）","","套","1.00","","","","","","灰硫——脱硫工业水泵用，建议品牌昕恒"]
["31","TM202508040942503562fbf","机械密封","100XHPR-45-10（集成式）","","套","1.00","","","","","","灰硫——脱硫充水泵，建议品牌昕恒"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]