{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":24,"n_cols":13,"rows_kept":24,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["陕西长青能源化工有限公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","TM202506041715528331b80","机封轴套","P3506B杂醇油泵 CZ32-250 流量6m3/h 扬程71m 出厂编号21032601","","件","1.00","","","","","","P3506B泵用/江苏大耐泵业有限公司"]
["2","TM202506041715528357c3a","叶轮","P406C 调节池提升泵 KQW 150/235-15/4 出厂编号FIB005393-01","","件","1.00","","","","","","调节池提升泵P406C/上海凯泉"]
["3","TM20250604171552836e800","油杯","总成 附图","","件","4.00","","","","","","P1306"]
["4","TM20250604171552837db35","油视镜","M27*1.5  铝合金  GB1160.2-95","","件","8.00","","","","","","P2204A检修"]
["5","TM202506041715528389660","雾化喷嘴","介质脱盐水，水雾粒径≤25微米，接口为外螺纹M14*1 材质：304  0.6MPa时，喷雾角度80度，100只总流量：100m3/h，含过滤网","","只","10.00","","","","","","精馏空冷风机用"]
["6","TM20250604171552838db9f","弹性块","YOXⅡ400","0","件","1.00","","","","","","4#皮带减速机联轴器"]
["7","TM20250604171552839c851","泵体口环","外径φ345.15mm*内径φ319.5mm*厚度28mm，铸钢","P406D污水循环泵/上海凯泉","套","1.00","","","","","","污水循环泵检修"]
["8","TM202506041715528401f9f","减速机","型号：WMRV5010-80B14-FL2，速比：10，法兰：80B14，编号：S2003/95330-1,电机轴径：19mm，搅拌轴轴径：25mm","","台","2.00","","","","","","回用水PAM搅拌器减速机"]
["9","TM20250604171552841345e","储水式电热水器","防水等级：IPX4，工作条件：密闭式，额定压力：0.8MPa，额定电压/频率：220V/50Hz，额定功率：2000W，额定容量：10L，外形尺寸：350*280*300mm，挂墙固定","","件","3.00","","","","","","装载机楼、供水装置（配挂墙用膨胀螺栓及必需的配件）"]
["10","TM202506041715528420d08","叉车轮胎","6.5-10-10PR 含轮毂","","套","2.00","","","","","","高压清洗机检修"]
["11","TM202506041715528437417","雾炮机喷头","2分，内丝，铜镀镍","","只","10.00","","","","","","渣场雾炮机喷头更换"]
["12","TM20250604171552844b2a0","氧气减压阀固定螺母","G5/8内螺纹、材质：铜、内牙：22.5mm、高度23mm、牙距：1.814mm、外径：22.9mm、小径：20.587mm","","个","2.00","","","","","","减压阀备件"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]