{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":23,"n_cols":13,"rows_kept":23,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["江苏徐矿能源股份有限公司物资供销分公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","TM20250711140427938424a","机械密封","泵型号：40DFCL8-50、流量7m3/h、扬程45m、转速2900r/min、原厂家：上海东方泵业（集团）有限公司","/阿克苏电厂","套","1.00","","","","","","机务：住宅楼换热站循环泵机封更换/"]
["2","TM20250711140427940ef6b","机械密封","管道泵型号：DFG125-160/2、流量143m3/h、扬程32m、转速2950r/min、功率22KW、效率75%、原厂家：上海东方泵业（集团）有限公司","/阿克苏电厂","套","2.00","","","","","","机务：住宅楼换热站循环泵机封更换/"]
["3","TM202507111404279411331","板换板片","换热器型号：M100B-1.6/150，原厂家：兰州兰石换热设备有限责任公司","/阿克苏电厂","片","20.00","","","","","","机务：住宅楼换热站换热器板片更换/"]
["4","TM20250711140427942c695","板换胶条","换热器型号：M100B-1.6/150，原厂家：兰州兰石换热设备有限责任公司","/阿克苏电厂","个","120.00","","","","","","机务：住宅楼换热站换热器清洗胶条更换/"]
["5","TM202507111404279430693","机械密封","泵型号IS50-32-200 JOHTN32AP001；流量：8m3/h；扬程：50m；长沙天鹅工业泵股份有限公司","/阿克苏电厂","套","2.00","","","","","","机务：脱硫#2滤布冲洗泵机封更换（用一备一）/"]
["6","TM202507111404279433c28","机械密封","泵型号：50DT-B40(37）；扬程：50m；流量：50m3/h；必需气蚀余量：6m；轴功率：17.2KW；转速：1470r/min；效率：40%；配用功率：22KW；粒度：≤14mm；原厂家：石家庄工业泵厂有限公司","/阿克苏电厂","套","2.00","","","","","","机务：脱硫#2清水泵使用（用一备一）/"]
["7","TM20250711140427944b0cf","端头滤布","XMYZ80/920-UB；原厂家：杭州雅顿过滤机械有限公司；进泥侧：板框侧100*100cm，中间孔φ100mm，孔长340mm，进泥法兰侧φ210mm，油缸侧：100*100cm","/阿克苏电厂","套","2.00","","","","","","机务：脱硫压泥机使用（用一套备一套）/"]
["8","6015180025","气囊及底座","DU5.4M2/900配套","","套","2.00","","","","","","机务：#1、2皮带脱水机更换"]
["9","6015180030","群边挡板","SE-QB-900","","套","2.00","","","","","","机务：#1、2皮带脱水机更换"]
["10","6699000313","机械密封","泵型号IS80-50-200A JOHTQ12AP001；流量：40m3/h；扬程：45m；转速：2900rpm；汽蚀余量2.5；配套功率11KW；长沙天鹅工业泵股份有限公司","","套","2.00","","","","","","机务：脱硫#1工艺水泵机封更换（用一备一）"]
["11","6704030009","滤布","XMYZ80/920-UB","","个","128.00","","","","","","XMYZ80/920-UB；原厂家：杭州雅顿过滤机械有限公司；尺寸：100*100cm，中间孔φ100mm，孔长60mm，脱硫压泥机使用"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]