{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":17,"n_cols":13,"rows_kept":17,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["江苏徐矿综合利用发电有限公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","无税单价（元）","总价（元）","品牌","备注"]
["1","TM20250912112651307eb29","#2机除氧器溢流电动阀","NKZ64Y-25，PN2.5 DN200","阀门内漏","套","1.00","","","","","","拆解阀门、研磨密封面、更换密封件后安装，无内漏"]
["2","TM20250912112651311e612","#2机高排通风阀","气动蝶阀D661Y-64C，DN150，接管尺寸Φ159*7，公称压力6.4MPa","阀门内漏","套","1.00","","","","","","切割拆解阀门拆解阀门、研磨密封面、更换密封件后安装，无内漏"]
["3","TM2025091211265131619ad","#2机#1高加危急疏水阀","阀前Φ219×12，材质20G/阀后Φ273×14 材质12CrMoVG，设计温度℃：343/293，设计压力28MPa","阀门内漏","套","1.00","","","","","","拆解阀门、研磨密封面、更换密封件后安装，无内漏"]
["4","TM20250912112651319802d","#2机#2高加危急疏水阀","阀前Φ219×7，材质20G/阀后Φ273×9 材质12CrMoVG，设计温度℃：277/257，设计压力28MPa","阀门内漏","套","1.00","","","","","","拆解阀门、研磨密封面、更换密封件后安装，无内漏"]
["5","TM20250912112651320e98b","#2机#3高加危急疏水阀","300×250，设计温度℃：240/220，设计压力28MPa","阀门内漏","套","1.00","","","","","","拆解阀门、研磨密封面、更换密封件后安装，无内漏"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]