{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":185,"n_cols":13,"rows_kept":185,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["徐州长城基础工程有限公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","无税单价（元）","总价（元）","品牌","备注"]
["1","TM2025102317031431408e3","临街房维修","临街房屋清理、垃圾清理转运人工","","日","3.00","","","","","","工期要求：根据实际情况履行"]
["2","TM20251023170314316d6aa","临街房维修","单层 SBS改性沥青防水卷材 热熔满铺法(10㎡）","","㎡","10.01","","","","","","工期要求：根据实际情况履行"]
["3","TM20251023170314317377f","平房维修、出租房维修","拆除平瓦屋面(10㎡）","","㎡","3.65","","","","","","工期要求：根据实际情况履行"]
["4","TM202510231703143181386","平房维修、出租房维修","拆除平瓦屋面 芦帘(10㎡）","","㎡","3.65","","","","","","工期要求：根据实际情况履行"]
["5","TM20251023170314319c06a","平房维修、出租房维修","翻换席(帘)(10㎡）","","㎡","3.65","","","","","","工期要求：根据实际情况履行"]
["6","TM202510231703143202cc3","平房维修、出租房维修","单层 SBS改性沥青防水卷材 冷粘法(10㎡）","","㎡","3.65","","","","","","工期要求：根据实际情况履行"]
["7","TM202510231703143210342","平房维修、出租房维修","翻铺瓦(10㎡）","","㎡","3.65","","","","","","工期要求：根据实际情况履行"]
["8","TM202510231703143211b26","平房维修、出租房维修","墙、柱梁面 灰泥浆底、纸筋灰面(10㎡）","","㎡","5.34","","","","","","工期要求：根据实际情况履行"]
["9","TM2025102317031432283f2","平房维修、出租房维修","混凝土及砖表面 1:3水泥砂浆底 1:1:6水泥白石屑浆面(10㎡）","","㎡","5.34","","","","","","工期要求：根据实际情况履行"]
["10","TM202510231703143233efc","平房维修、出租房维修","抹灰脚手架 高3.6m以内(10㎡）","","㎡","3.65","","","","","","工期要求：根据实际情况履行"]
["11","TM202510231703143244beb","平房维修、出租房维修","煤建路出租房维修、卫生间高水箱更换下水","","日","6.00","","","","","","工期要求：根据实际情况履行"]
["12","TM2025102317031432504ec","舜华厨房拆除","彩钢板人工下楼、水管维修","","日","11.00","","","","","","工期要求：根据实际情况履行"]
["13","TM202510231703143261877","舜华厨房拆除","拆除彩钢复合板屋面（10㎡）","","㎡","13.98","","","","","","工期要求：根据实际情况履行"]
["14","TM202510231703143279526","南岗卫生间","大便槽冲洗水箱 下水48L（10套）","","套","0.05","","","","","","工期要求：根据实际情况履行"]
["15","TM2025102317031432796bf","南岗卫生间","南岗卫生间维修下水管、更换电子感应装置","","日","4.00","","","","","","工期要求：根据实际情况履行"]
["16","TM20251023170314328f43d","南岗卫生间","点型探测器 总线制 红外光束","","个","2.00","","","","","","工期要求：根据实际情况履行"]
["17","TM202510231703143298f0e","南岗卫生间","PVC管排水  阳台PVC通水落管φ50 斜长每增、减100mm（10只）","","只","0.40","","","","","","工期要求：根据实际情况履行"]
["18","TM20251023170314330e077","南岗卫生间","PVC水落管 Φ50（10m）","","m","0.40","","","","","","工期要求：根据实际情况履行"]
["19","TM2025102317031433170b4","南岗卫生间","PVC管排水  阳台PVC通水落管φ50 斜长在1000mm（10只）","","只","0.30","","","","","","工期要求：根据实际情况履行"]
["20","TM202510231703143319c6c","南岗卫生间","排水栓安装 带存水弯 50（10组）","","组","0.10","","","","","","工期要求：根据实际情况履行"]
["21","TM20251023170314332c417","南岗卫生间","水龙头安装 公称直径20mm以内三角阀（10个）","","个","0.10","","","","","","工期要求：根据实际情况履行"]
["22","TM202510231703143339c12","南岗卫生间","洗手盆安装 冷水（10组）","","组","0.20","","","","","","工期要求：根据实际情况履行"]
["23","TM20251023170314334d1fb","南岗卫生间","大便槽自动冲洗水箱 40L（10套）","","套","0.50","","","","","","工期要求：根据实际情况履行"]
["24","TM20251023170314334207a","南岗清理杂树","南岗2号库北、4号库东砍伐杂树","","日","18.00","","","","","","工期要求：根据实际情况履行"]
["25","TM20251023170314335f15c","南岗清理杂树","2号库北巷道伐树","","日","12.00","","","","","","工期要求：根据实际情况履行"]
["26","TM202510231703143353d89","南岗清理杂树","人工转运、截断树木、垃圾人工装车","","日","10.00","","","","","","工期要求：根据实际情况履行"]
["27","TM2025102317031433615a1","南岗清理杂树","载货汽车6t场外运输费垃圾、树木外运","","次","3.00","","","","","","工期要求：根据实际情况履行"]
["28","TM202510231703143376e31","南岗危房拆除","拆拆危房、红瓦拆除转运、拆拆彩钢板房、清理杂物下水道人工清理、红砖铺地、排水口焊钢筋盖板","","日","60.00","","","","","","工期要求：根据实际情况履行"]
["29","TM20251023170314338bc99","南岗危房拆除","履带式挖掘机1m3以内 场外运输费用","","次","1.00","","","","","","工期要求：根据实际情况履行"]
["30","TM20251023170314338d9c4","南岗危房拆除","履带式单斗挖掘机(液压) 斗容量1m3","","台班","3.00","","","","","","工期要求：根据实际情况履行"]
["31","TM20251023170314339c8d3","南岗危房拆除","自卸汽车碎砖转运","","台班","3.00","","","","","","工期要求：根据实际情况履行"]
["32","TM20251023170314339a2e2","南岗危房拆除","垃圾汽车外运","","台班","6.00","","","","","","工期要求：根据实际情况履行"]
["33","TM20251023170314340bfef","南岗三防","人工铲沙入池","","日","1.00","","","","","","工期要求：根据实际情况履行"]
["34","TM20251023170314340700b","南岗三防","中砂","","t","14.00","","","","","","工期要求：根据实际情况履行"]
["35","TM20251023170314341db20","南岗库房、办公室屋面修漏","清扫拾漏南岗库房屋面维修(10㎡）","","㎡","254.40","","","","","","工期要求：根据实际情况履行"]
["36","TM202510231703143414d37","南岗库房、办公室屋面修漏","翻铺瓦办公室屋面翻修(10㎡）","","㎡","39.33","","","","","","工期要求：根据实际情况履行"]
["37","TM20251023170314342be5b","南岗库房、办公室屋面修漏","放射源屋面SBS卷材(10㎡）","","㎡","3.00","","","","","","工期要求：根据实际情况履行"]
["38","TM202510231703143431b87","南岗库房、办公室屋面修漏","煤建路卷帘门维修(10㎡）","","㎡","0.30","","","","","","工期要求：根据实际情况履行"]
["39","TM20251023170314346ca2e","南岗库房、办公室屋面修漏","办公室塑钢门更换(10㎡）","","㎡","0.11","","","","","","工期要求：根据实际情况履行"]
["40","TM202510231703143476b1f","南岗库房、办公室屋面修漏","煤建路出租房维修、南岗卫生间更换拉手下水","","日","6.00","","","","","","工期要求：根据实际情况履行"]
["41","TM20251023170314347170e","南岗2号库北及办公室西北电动车棚，混凝土地坪","一类干土 槽深1.5m内","","m3","0.11","","","","","","工期要求：根据实际情况履行"]
["42","TM202510231703143489589","南岗3号库北及办公室西北电动车棚，混凝土地坪","高颈杯形基础","","m3","0.11","","","","","","工期要求：根据实际情况履行"]
["43","TM20251023170314348df3c","南岗4号库北及办公室西北电动车棚，混凝土地坪","钢屋架(型钢) 制作","","m3","0.10","","","","","","工期要求：根据实际情况履行"]
["44","TM202510231703143492055","南岗5号库北及办公室西北电动车棚，混凝土地坪","单层彩钢板(10㎡）","","㎡","3.20","","","","","","工期要求：根据实际情况履行"]
["45","TM20251023170314350c56d","南岗6号库北及办公室西北电动车棚，混凝土地坪","接地极板 钢板","","块","1.00","","","","","","工期要求：根据实际情况履行"]
["46","TM202510231703143504ee2","南岗7号库北及办公室西北电动车棚，混凝土地坪","钢结构支架配管 电线管公称直径15mm以内（100m）","","m","0.16","","","","","","工期要求：根据实际情况履行"]
["47","TM20251023170314351f77f","南岗8号库北及办公室西北电动车棚，混凝土地坪","管内穿线 照明线路 导线截面4mm2以内 铝芯(100m单线)","","m","1.08","","","","","","工期要求：根据实际情况履行"]
["48","TM202510231703143519403","南岗9号库北及办公室西北电动车棚，混凝土地坪","接线盒明装 普通接线盒(10个)","","个","0.60","","","","","","工期要求：根据实际情况履行"]
["49","TM20251023170314352536d","南岗10号库北及办公室西北电动车棚，混凝土地坪","单相明插座15A 5孔（10套）","","套","0.60","","","","","","工期要求：根据实际情况履行"]
["50","TM202510231703143536fbe","南岗11号库北及办公室西北电动车棚，混凝土地坪","节能座灯头（10套）","","套","0.10","","","","","","工期要求：根据实际情况履行"]
["51","TM2025102317031435400c1","南岗12号库北及办公室西北电动车棚，混凝土地坪","白炽灯泡安装（10套）","","套","0.10","","","","","","工期要求：根据实际情况履行"]
["52","TM20251023170314354fb7c","南岗13号库北及办公室西北电动车棚，混凝土地坪","配电(电源)屏 低压开关柜安装","","台","1.00","","","","","","工期要求：根据实际情况履行"]
["53","TM20251023170314355b799","南岗14号库北及办公室西北电动车棚，混凝土地坪","直埋电缆线路 16mm2电缆线 电缆规格VV22-3*16（1000m）","","m","0.12","","","","","","工期要求：根据实际情况履行"]
["54","TM202510231703143564f68","南岗15号库北及办公室西北电动车棚，混凝土地坪","人工清理杂物、人工地坪翻整、人工垃圾转运、爬墙虎清理","","日","15.00","","","","","","工期要求：根据实际情况履行"]
["55","TM202510231703143570f71","南岗16号库北及办公室西北电动车棚，混凝土地坪","碎石(道渣) 干铺","","m3","12.52","","","","","","工期要求：根据实际情况履行"]
["56","TM202510231703143570aa5","南岗17号库北及办公室西北电动车棚，混凝土地坪","混凝土面层(厚度) 100mm(10㎡）","","㎡","25.04","","","","","","工期要求：根据实际情况履行"]
["57","TM202510231703143589b6b","南岗18号库北及办公室西北电动车棚，混凝土地坪","锯缝机锯缝（10m）","","m","2.19","","","","","","工期要求：根据实际情况履行"]
["58","TM20251023170314358e7d6","南岗19号库北及办公室西北电动车棚，混凝土地坪","水泥混凝土 棉毡养护(100㎡）","","㎡","2.50","","","","","","工期要求：根据实际情况履行"]
["59","TM20251023170314359a292","南岗20号库北及办公室西北电动车棚，混凝土地坪","拆除插座、拆除电源线、拆除胶木支架、焊电源支架","","日","4.00","","","","","","工期要求：根据实际情况履行"]
["60","TM2025102317031436009d5","南岗21号库北及办公室西北电动车棚，混凝土地坪","接地极板 钢板","","块","1.00","","","","","","工期要求：根据实际情况履行"]
["61","TM2025102317031436099e1","南岗22号库北及办公室西北电动车棚，混凝土地坪","钢结构支架配管 电线管公称直径15mm以内(100m)","","m","0.24","","","","","","工期要求：根据实际情况履行"]
["62","TM20251023170314361935e","南岗23号库北及办公室西北电动车棚，混凝土地坪","管内穿线 照明线路 导线截面4mm2以内 铝芯（100m单线）","","m","0.72","","","","","","工期要求：根据实际情况履行"]
["63","TM2025102317031436104db","南岗24号库北及办公室西北电动车棚，混凝土地坪","接线盒明装 普通接线盒(10个)","","个","0.40","","","","","","工期要求：根据实际情况履行"]
["64","TM202510231703143622363","南岗25号库北及办公室西北电动车棚，混凝土地坪","单相明插座15A 5孔(10套)","","套","0.40","","","","","","工期要求：根据实际情况履行"]
["65","TM202510231703143628b76","南岗26号库北及办公室西北电动车棚，混凝土地坪","节能座灯头(10套)","","套","0.10","","","","","","工期要求：根据实际情况履行"]
["66","TM20251023170314363ba4e","南岗27号库北及办公室西北电动车棚，混凝土地坪","白炽灯泡安装(10套)","","套","0.10","","","","","","工期要求：根据实际情况履行"]
["67","TM20251023170314363845e","南岗28号库北及办公室西北电动车棚，混凝土地坪","成套配电箱安装 悬挂嵌入式 半周长1m","","台","1.00","","","","","","工期要求：根据实际情况履行"]
["68","TM202510231703143642cac","南岗29号库北及办公室西北电动车棚，混凝土地坪","漏电保护开关安装 单式 单极","","个","4.00","","","","","","工期要求：根据实际情况履行"]
["69","TM202510231703143657597","南岗30号库北及办公室西北电动车棚，混凝土地坪","插接式空气开关箱安装 ≤100A","","台","1.00","","","","","","工期要求：根据实际情况履行"]
["70","TM20251023170314365dee4","南岗31号库北及办公室西北电动车棚，混凝土地坪","线槽内敷设500V截面16mm2铜芯塑料电线（100m）","","m","0.18","","","","","","工期要求：根据实际情况履行"]
["71","TM2025102317031436601be","南岗下水道","南岗原下水道口人工找挖、挖水渠坡道","","日","2.00","","","","","","工期要求：根据实际情况履行"]
["72","TM20251023170314366091b","南岗下水道","现浇混凝土构件钢筋 Φ12mm内","","t","0.15","","","","","","工期要求：根据实际情况履行"]
["73","TM2025102317031436700ad","南岗下水道","混凝土","","m3","0.46","","","","","","工期要求：根据实际情况履行"]
["74","TM202510231703143674956","南岗下水道","1/2砖墙 新砌","","m3","1.03","","","","","","工期要求：根据实际情况履行"]
["75","TM20251023170314368a3a1","南岗下水道","混凝土及砖外墙面 水泥砂浆底、面(10㎡）","","㎡","1.72","","","","","","工期要求：根据实际情况履行"]
["76","TM202510231703143693392","南岗下水道","四类干土 槽深1.5m内","","m3","3.24","","","","","","工期要求：根据实际情况履行"]
["77","TM20251023170314369bd39","南岗下水道","人工转运土方、砸洞","","日","4.00","","","","","","工期要求：根据实际情况履行"]
["78","TM20251023170314370bbe6","南岗下水道","一砖墙 新砌","","m3","1.04","","","","","","工期要求：根据实际情况履行"]
["79","TM2025102317031437139da","南岗下水道","混凝土及砖表面 1:3水泥砂浆底 1:1:6水泥白石屑浆面(10㎡）","","㎡","0.43","","","","","","工期要求：根据实际情况履行"]
["80","TM20251023170314372f6b9","南岗下水道","细石混凝土 厚40mm(10㎡）","","㎡","0.27","","","","","","工期要求：根据实际情况履行"]
["81","TM20251023170314373ad91","南岗下水道","居民蔬菜挖埋重栽","","日","2.00","","","","","","工期要求：根据实际情况履行"]
["82","TM20251023170314373f5af","南岗下水道","挖机挖土埋钢塑下水道、回填土","","台班","3.00","","","","","","工期要求：根据实际情况履行"]
["83","TM202510231703143748014","南岗下水道","塑料排水管(粘接) 公称外径50mm以内(10m)","","m","1.20","","","","","","工期要求：根据实际情况履行"]
["84","TM2025102317031437593e7","南岗下水道","下水道挖坡道","","日","2.00","","","","","","工期要求：根据实际情况履行"]
["85","TM20251023170314375346f","南岗下水道","现浇混凝土构件钢筋 Φ12mm内","","t","0.15","","","","","","工期要求：根据实际情况履行"]
["86","TM20251023170314376fefb","南岗下水道","混凝土","","m3","0.46","","","","","","工期要求：根据实际情况履行"]
["87","TM202510231703143770697","南岗下水道","1/2砖墙 新砌","","m3","1.03","","","","","","工期要求：根据实际情况履行"]
["88","TM202510231703143786fab","南岗下水道","混凝土及砖外墙面 水泥砂浆底、面(10㎡）","","㎡","1.72","","","","","","工期要求：根据实际情况履行"]
["89","TM202510231703143782d97","南岗空调","南岗仓库空调移机4台","","项","1.00","","","","","","工期要求：根据实际情况履行"]
["90","TM20251023170314379ef04","南岗空调","办公室空调器安装 墙上式 重量0.1t以内","","台","2.00","","","","","","工期要求：根据实际情况履行"]
["91","TM20251023170314380f0ef","南院综合楼蓄水池","南院综合楼蓄水池","","项","1.00","","","","","","工期要求：根据实际情况履行"]
["92","TM20251023170314380a1cc","南院综合楼蓄水池","南院移动公司仪器库房上方水库抽水","","日","4.00","","","","","","工期要求：根据实际情况履行"]
["93","TM20251023170314381db31","焊大棚材料","材料 焊条3箱、配电箱1套、燕尾钉3盒、氧气6瓶、乙炔4瓶、石笔2盒、105切割片2盒、125切割片1盒、350切割片10片、48焊管3支、中灰防锈漆1桶","","项","1.00","","","","","","工期要求：根据实际情况履行"]
["94","TM20251023170314382c11f","南院综合楼消防管改造","彩钢复合板屋面(10㎡）","","㎡","10.88","","","","","","工期要求：根据实际情况履行"]
["95","TM2025102317031438221e8","南院综合楼消防管改造","人工转运垃圾下楼、清理垃圾","","日","8.00","","","","","","工期要求：根据实际情况履行"]
["96","TM2025102317031438307d9","南院综合楼消防管改造","单级离心泵及耐腐蚀泵拆除 设备重量(t以内) 1","","台","1.00","","","","","","工期要求：根据实际情况履行"]
["97","TM20251023170314383ea08","南院综合楼消防管改造","离心式杂质泵重1.0t内","","台","1.00","","","","","","工期要求：根据实际情况履行"]
["98","TM202510231703143840d33","南院综合楼消防管改造","控制箱安装","","台","1.00","","","","","","工期要求：根据实际情况履行"]
["99","TM20251023170314385520b","南院综合楼消防管改造","四芯矿物绝缘电力电缆(水平) 4芯 水平 电缆截面4mm2(100m）","","m","0.08","","","","","","工期要求：根据实际情况履行"]
["100","TM2025102317031438553f5","南院综合楼消防管改造","拆除石膏板封板(10㎡）","","㎡","0.24","","","","","","工期要求：根据实际情况履行"]
["101","TM20251023170314386336b","南院综合楼消防管改造","恢复细木工板、纸面石膏板(100m）","","m","0.02","","","","","","工期要求：根据实际情况履行"]
["102","TM202510231703143878167","南院综合楼消防管改造","低压管件 碳钢管件(螺纹连接) 公称直径40mm以内（10个）","","个","0.10","","","","","","工期要求：根据实际情况履行"]
["103","TM20251023170314387a891","南院综合楼消防管改造","6楼西水池抽水、人工清池、修坏水管","","日","12.00","","","","","","工期要求：根据实际情况履行"]
["104","TM20251023170314388738c","南院综合楼消防管改造","低压管道 塑料管(热风焊) 管外径75mm以内（10m）","","m","0.60","","","","","","工期要求：根据实际情况履行"]
["105","TM202510231703143888412","南院综合楼消防管改造","低压管件 塑料管件(热风焊) 管外径75mm以内（10个）","","个","0.20","","","","","","工期要求：根据实际情况履行"]
["106","TM20251023170314389437b","南院综合楼消防管改造","低压管道 塑料管(热风焊) 管外径40mm以内（10m）","","m","0.30","","","","","","工期要求：根据实际情况履行"]
["107","TM202510231703143904a10","南院综合楼消防管改造","低压管件 塑料管件(热风焊) 管外径40mm以内（10个）","","个","0.40","","","","","","工期要求：根据实际情况履行"]
["108","TM20251023170314390c006","南院综合楼消防管改造","低压阀门 螺纹阀门 公称直径40mm以内","","个","2.00","","","","","","工期要求：根据实际情况履行"]
["109","TM202510231703143911bcb","南院综合楼消防管改造","浮球液位控制器安装","","个","1.00","","","","","","工期要求：根据实际情况履行"]
["110","TM20251023170314391246e","南院综合楼消防管改造","低压阀门 止回阀 公称直径100mm以内","","个","1.00","","","","","","工期要求：根据实际情况履行"]
["111","TM2025102317031439225fc","南院综合楼消防管改造","低压管件 消防管三通公称直径100mm以内（10个）","","个","0.10","","","","","","工期要求：根据实际情况履行"]
["112","TM202510231703143933160","南院综合楼消防管改造","1-5楼消防管注水、检查消防栓","","日","4.00","","","","","","工期要求：根据实际情况履行"]
["113","TM202510231703143930f60","南院综合楼消防管改造","栏杆制作 型钢为主","","t","0.03","","","","","","工期要求：根据实际情况履行"]
["114","TM202510231703143943336","南院综合楼消防管改造","单层彩钢板墙(10㎡）","","㎡","0.50","","","","","","工期要求：根据实际情况履行"]
["115","TM20251023170314395fcdf","南院综合楼消防管改造","铁门焊合页、砌踏步、打水泥地","","日","4.00","","","","","","工期要求：根据实际情况履行"]
["116","TM20251023170314395b38a","南院综合楼消防管改造","载货汽车8t场外运输费","","次","1.00","","","","","","工期要求：根据实际情况履行"]
["117","TM20251023170314396a6ee","南院综合楼消防管改造","南院电梯更换钢丝绳人工搬运","","日","2.00","","","","","","工期要求：根据实际情况履行"]
["118","TM20251023170314396a32d","南岗高压电线维修","南岗高压电线维修","","日","9.00","","","","","","工期要求：根据实际情况履行"]
["119","TM20251023170314397a7ad","南岗高压电线维修","绝缘胶布 20m/卷","","卷","62.00","","","","","","工期要求：根据实际情况履行"]
["120","TM20251023170314397adfa","南岗高压电线维修","移动脚手架(10m3）","","m3","1.44","","","","","","工期要求：根据实际情况履行"]
["121","TM20251023170314398d674","煤建路屋面维修、增加漏保","煤建路屋面维修、增加漏保(10m3）","","m3","1.00","","","","","","工期要求：根据实际情况履行"]
["122","TM20251023170314398db83","煤建路屋面维修、增加漏保","门面房屋面修漏、增加漏保","","日","6.00","","","","","","工期要求：根据实际情况履行"]
["123","TM20251023170314399a75f","煤建路屋面维修、增加漏保","BV铜芯聚氯乙烯绝缘线 450V/750V4mm2","","m","2.00","","","","","","工期要求：根据实际情况履行"]
["124","TM202510231703144003e0a","煤建路屋面维修、增加漏保","漏保","","个","5.00","","","","","","工期要求：根据实际情况履行"]
["125","TM202510231703144002d19","煤建路屋面维修、增加漏保","自粘聚脂胎乙烯膜卷材 δ2mm","","㎡","30.00","","","","","","工期要求：根据实际情况履行"]
["126","TM202510231703144019fca","煤建路屋面维修、增加漏保","南岗办公室、2#3#4#库房维修","","日","18.00","","","","","","工期要求：根据实际情况履行"]
["127","TM202510231703144018d53","煤建路屋面维修、增加漏保","南岗人工伐2#南、4#库巷道大树","","日","4.00","","","","","","工期要求：根据实际情况履行"]
["128","TM20251023170314402e2c3","南院屋面修漏","南院屋面修漏","","日","1.00","","","","","","工期要求：根据实际情况履行"]
["129","TM202510231703144039b3e","南院屋面修漏","南院修漏","","日","18.00","","","","","","工期要求：根据实际情况履行"]
["130","TM20251023170314403c0a0","南院屋面修漏","自粘聚脂胎乙烯膜卷材 δ2mm","","㎡","40.00","","","","","","工期要求：根据实际情况履行"]
["131","TM2025102317031440422e4","南院屋面修漏","硅酮结构胶","","L","4.00","","","","","","工期要求：根据实际情况履行"]
["132","TM202510231703144048eba","集装箱改办公室","木龙骨、木板、纤维板、板条抹灰间壁拆除(10㎡）","","㎡","13.87","","","","","","工期要求：根据实际情况履行"]
["133","TM20251023170314405fd3f","集装箱改办公室","电线管拆除 公称直径（mm） 20（100m）","","m","0.40","","","","","","工期要求：根据实际情况履行"]
["134","TM20251023170314405bfa1","集装箱改办公室","暗插座拆除（10个）","","个","1.60","","","","","","工期要求：根据实际情况履行"]
["135","TM20251023170314406bac5","集装箱改办公室","拆除泡沫保温板(10㎡）","","㎡","0.69","","","","","","工期要求：根据实际情况履行"]
["136","TM20251023170314407dac0","集装箱改办公室","多联体空调器室拆除 制冷量(KW以内) 20","","台","4.00","","","","","","工期要求：根据实际情况履行"]
["137","TM202510231703144073e8e","集装箱改办公室","电线暗配 硬质聚氯乙烯管公称直径25mm以内（100m）","","m","0.81","","","","","","工期要求：根据实际情况履行"]
["138","TM20251023170314408fe37","集装箱改办公室","管内穿线 照明线路 导线截面4mm2以内 铜芯（100m单线）","","m","2.42","","","","","","工期要求：根据实际情况履行"]
["139","TM20251023170314408ff5f","集装箱改办公室","单相暗插座15A 5孔（10套）","","套","2.20","","","","","","工期要求：根据实际情况履行"]
["140","TM20251023170314409e611","集装箱改办公室","半圆球吸顶灯 灯罩直径350mm以内（10套）","","套","0.40","","","","","","工期要求：根据实际情况履行"]
["141","TM20251023170314409b53f","集装箱改办公室","室内焊角铁、扁铁架撑","","t","0.11","","","","","","工期要求：根据实际情况履行"]
["142","TM20251023170314410ee2f","集装箱改办公室","彩钢夹芯板屋面 75mm(10㎡）","","㎡","13.87","","","","","","工期要求：根据实际情况履行"]
["143","TM20251023170314411d900","集装箱改办公室","碳晶板 贴在基层板底(10㎡）","","㎡","13.87","","","","","","工期要求：根据实际情况履行"]
["144","TM2025102317031441131eb","集装箱改办公室","聚氨酯防水层1.5mm厚(10㎡）","","㎡","0.94","","","","","","工期要求：根据实际情况履行"]
["145","TM20251023170314412c57e","集装箱改办公室","成品塑钢 推拉窗安装(10㎡）","","㎡","0.51","","","","","","工期要求：根据实际情况履行"]
["146","TM20251023170314412f02c","集装箱改办公室","塑钢纱窗(10㎡扇面积）","","㎡","0.30","","","","","","工期要求：根据实际情况履行"]
["147","TM202510231703144138e86","集装箱改办公室","装弹子门锁","","把","1.00","","","","","","工期要求：根据实际情况履行"]
["148","TM20251023170314413935c","集装箱改办公室","金属面防火涂料 超薄型 4遍(10㎡）","","㎡","11.38","","","","","","工期要求：根据实际情况履行"]
["149","TM202510231703144144744","集装箱改办公室","字标外墙喷绘","","个","6.00","","","","","","工期要求：根据实际情况履行"]
["150","TM202510231703144150ddb","集装箱改宿舍","木龙骨、木板、纤维板、板条抹灰间壁拆除(10㎡）","","㎡","26.99","","","","","","工期要求：根据实际情况履行"]
["151","TM2025102317031441590e2","集装箱改宿舍","电线管拆除 公称直径（mm） 20（100m）","","m","0.72","","","","","","工期要求：根据实际情况履行"]
["152","TM20251023170314416f5a5","集装箱改宿舍","暗插座拆除（10个）","","个","2.40","","","","","","工期要求：根据实际情况履行"]
["153","TM20251023170314417c382","集装箱改宿舍","拆除夹心隔断(10㎡）","","㎡","2.40","","","","","","工期要求：根据实际情况履行"]
["154","TM20251023170314417519b","集装箱改宿舍","多联体空调器室拆除 制冷量(KW以内) 20","","台","4.00","","","","","","工期要求：根据实际情况履行"]
["155","TM20251023170314418c433","集装箱改宿舍","电线暗配 硬质聚氯乙烯管公称直径25mm以内（100m）","","m","1.25","","","","","","工期要求：根据实际情况履行"]
["156","TM20251023170314418d573","集装箱改宿舍","管内穿线 照明线路 导线截面4mm2以内 铜芯（100m单线）","","m","3.74","","","","","","工期要求：根据实际情况履行"]
["157","TM20251023170314419061a","集装箱改宿舍","单相暗插座15A 5孔（10套）","","套","3.90","","","","","","工期要求：根据实际情况履行"]
["158","TM20251023170314420b0f9","集装箱改宿舍","半圆球吸顶灯 灯罩直径350mm以内（10套）","","套","0.60","","","","","","工期要求：根据实际情况履行"]
["159","TM202510231703144218df7","集装箱改宿舍","室内焊角铁、扁铁架撑","","t","0.21","","","","","","工期要求：根据实际情况履行"]
["160","TM20251023170314421975b","集装箱改宿舍","彩钢夹芯板屋面 75mm(10㎡）","","㎡","20.77","","","","","","工期要求：根据实际情况履行"]
["161","TM202510231703144223041","集装箱改宿舍","聚氨酯防水层1.5mm厚(10㎡）","","㎡","1.04","","","","","","工期要求：根据实际情况履行"]
["162","TM202510231703144235c8b","集装箱改宿舍","成品塑钢 推拉窗安装(10㎡）","","㎡","0.18","","","","","","工期要求：根据实际情况履行"]
["163","TM20251023170314423771b","集装箱改宿舍","塑钢纱窗（扇面积）(10㎡）","","㎡","0.30","","","","","","工期要求：根据实际情况履行"]
["164","TM20251023170314424c45c","集装箱改宿舍","钢防盗门安装(10㎡）","","㎡","0.20","","","","","","工期要求：根据实际情况履行"]
["165","TM202510231703144250fab","集装箱改宿舍","金属面防火涂料 超薄型 4遍(10㎡）","","㎡","21.37","","","","","","工期要求：根据实际情况履行"]
["166","TM20251023170314426e42f","集装箱改仓库","木龙骨、木板、纤维板、板条抹灰间壁拆除(10㎡）","","㎡","13.87","","","","","","工期要求：根据实际情况履行"]
["167","TM202510231703144264c40","集装箱改仓库","电线管拆除 公称直径（mm） 20（100m）","","m","0.40","","","","","","工期要求：根据实际情况履行"]
["168","TM20251023170314427e926","集装箱改仓库","暗插座拆除（10个）","","个","1.00","","","","","","工期要求：根据实际情况履行"]
["169","TM202510231703144280893","集装箱改仓库","拆除泡沫保温板(10㎡）","","㎡","0.69","","","","","","工期要求：根据实际情况履行"]
["170","TM202510231703144290109","集装箱改仓库","多联体空调器室拆除 制冷量(KW以内) 20","","台","2.00","","","","","","工期要求：根据实际情况履行"]
["171","TM20251023170314429a4de","集装箱改仓库","卷材屋面  SBS改性沥青防水卷材 热熔空铺法 单层(10㎡）","","㎡","1.56","","","","","","工期要求：根据实际情况履行"]
["172","TM20251023170314430c4ed","集装箱改仓库","金属面防火涂料 超薄型 4遍(10㎡）","","㎡","11.38","","","","","","工期要求：根据实际情况履行"]
["173","TM202510231703144319d78","集装箱改仓库","载货汽车8t场外运输费垃圾合计","","次","3.00","","","","","","工期要求：根据实际情况履行"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]