{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":38,"n_cols":13,"rows_kept":38,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["苏能（锡林郭勒）发电有限公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","TM20250604163744192ae71","非金属膨胀节蒙皮","蒙皮宽度mm440，厚度8.5mm 材质：夹丝陶瓷纤维布1.5mm、无碱玻纤布1.5mm、聚四氟乙烯布0.2mm、聚四氟乙烯薄膜0.3mm、增强纤维布1.5mm、玻璃纤维布1.0mm，复合硅橡胶布1.5mm、316L不锈钢丝网等复合而成。风道（硅橡胶）","","米","10.00","","","","","","使用位置：热风"]
["2","TM202506041637441932d09","非金属膨胀节蒙皮","蒙皮宽度mm330，厚度8.5mm  材质：夹丝陶瓷纤维布1.5mm、无碱玻纤布1.5mm、聚四氟乙烯布0.2mm、聚四氟乙烯薄膜0.3mm、增强纤维布1.5mm、玻璃纤维布1.0mm，复合硅橡胶布1.5mm、316L不锈钢丝网等复合而成，风道（硅橡胶）","","米","10.00","","","","","","使用位置：热风"]
["3","TM20250604163744194669d","非金属膨胀节蒙皮","蒙皮宽度mm360，厚度8.5mm  材质：夹丝陶瓷纤维布1.5mm、无碱玻纤布1.5mm、聚四氟乙烯布0.2mm、聚四氟乙烯薄膜0.3mm、增强纤维布1.5mm、玻璃纤维布1.0mm，复合硅橡胶布1.5mm、316L不锈钢丝网等复合而成，风道（硅橡胶）","","米","10.00","","","","","","使用位置：热风"]
["4","TM20250604163744195fd44","非金属膨胀节蒙皮","蒙皮宽度mm750，厚度8.5mm  材质：夹丝陶瓷纤维布1.5mm、无碱玻纤布1.5mm、聚四氟乙烯布0.2mm、聚四氟乙烯薄膜0.3mm、增强纤维布1.5mm、玻璃纤维布1.0mm，复合氟橡胶布1.5mm、316L不锈钢丝网等复合而成，烟道(氟橡胶)","","米","20.00","","","","","","使用位置：省煤器出口"]
["5","TM202506041637441963e83","非金属膨胀节蒙皮","蒙皮宽度mm460，厚度8.5mm  材质：夹丝陶瓷纤维布1.5mm、无碱玻纤布1.5mm、聚四氟乙烯布0.2mm、聚四氟乙烯薄膜0.3mm、增强纤维布1.5mm、玻璃纤维布1.0mm，复合氟橡胶布1.5mm、316L不锈钢丝网等复合而成，烟道(氟橡胶)","","米","20.00","","","","","","使用位置：脱硝出口烟道后，空预器旁路烟道前/室外圆形烟道"]
["6","TM2025060416374419771a1","非金属膨胀节蒙皮","蒙皮宽度mm320，厚度8.5mm  材质：夹丝陶瓷纤维布1.5mm、无碱玻纤布1.5mm、聚四氟乙烯布0.2mm、聚四氟乙烯薄膜0.3mm、增强纤维布1.5mm、玻璃纤维布1.0mm，复合氟橡胶布1.5mm、316L不锈钢丝网等复合而成，烟道(氟橡胶)","","米","15.00","","","","","","使用位置：烟道空预器入口处"]
["7","TM202506041637441984fc7","非金属膨胀节蒙皮","蒙皮宽度mm300，厚度8.5mm  材质：夹丝陶瓷纤维布1.5mm、无碱玻纤布1.5mm、聚四氟乙烯布0.2mm、聚四氟乙烯薄膜0.3mm、增强纤维布1.5mm、玻璃纤维布1.0mm，复合氟橡胶布1.5mm、316L不锈钢丝网等复合而成，烟道(氟橡胶)","","米","40.00","","","","","","使用位置：烟道空预器出口处/空预器旁路出口与耦合烟道入口相接处"]
["8","TM20250604163744198150c","非金属膨胀节蒙皮","蒙皮宽度mm280，厚度8.5mm 材质：夹丝陶瓷纤维布1.5mm、无碱玻纤布1.5mm、聚四氟乙烯布0.2mm、聚四氟乙烯薄膜0.3mm、增强纤维布1.5mm、玻璃纤维布1.0mm，复合氟橡胶布1.5mm、316L不锈钢丝网等复合而成，烟道(氟橡胶)","","米","15.00","","","","","","使用位置：烟道空预器出口与空预器旁路相接处"]
["9","TM20250604163744199daea","非金属膨胀节蒙皮","蒙皮宽度mm400，厚度8.5mm  材质：夹丝陶瓷纤维布1.5mm、无碱玻纤布1.5mm、聚四氟乙烯布0.2mm、聚四氟乙烯薄膜0.3mm、增强纤维布1.5mm、玻璃纤维布1.0mm，复合氟橡胶布1.5mm、316L不锈钢丝网等复合而成，烟道(氟橡胶)","","米","10.00","","","","","","使用位置：空预器旁路入口/出口/耦合烟道入口"]
["10","TM202506041637442000643","非金属膨胀节蒙皮","蒙皮宽度mm440，厚度8.5mm  材质：夹丝陶瓷纤维布1.5mm、无碱玻纤布1.5mm、聚四氟乙烯布0.2mm、聚四氟乙烯薄膜0.3mm、增强纤维布1.5mm、玻璃纤维布1.0mm，复合氟橡胶布1.5mm、316L不锈钢丝网等复合而成，烟道(氟橡胶)","","米","10.00","","","","","","使用位置：耦合烟道出口"]
["11","TM202506041637442013510","单球橡胶短接","KXT-I型 DN200PG10（橡胶","","个","2.00","","","","","","灰硫——检修使用"]
["12","TM20250604163744201ce25","直接接头","PVC材质   DN20","","个","10.00","","","","","","化学——检修使用"]
["13","TM20250604163744202f806","直接接头","PVC材质   DN25","","个","10.00","","","","","","化学——检修使用"]
["14","TM20250604163744203e4cc","直接接头","PVC材质   DN40","","个","10.00","","","","","","化学——检修使用"]
["15","TM202506041637442049453","直接接头","PVC材质   DN32","","个","10.00","","","","","","化学——检修使用"]
["16","TM20250604163744204985e","法兰","304材质   DN25 16公斤 1.6兆帕","","片","4.00","","","","","","化学——检修使用"]
["17","TM20250604163744205f6e5","法兰","304材质   DN20 16公斤 1.6兆帕","","片","4.00","","","","","","化学——检修使用"]
["18","TM20250604163744205e465","法兰","304材质   DN32 16公斤 1.6兆帕","","片","4.00","","","","","","化学——检修使用"]
["19","TM202506041637442068214","法兰","304材质   DN40 16公斤 1.6兆帕","","片","4.00","","","","","","化学——检修使用"]
["20","TM20250604163744207a443","管道","PVC材质   DN20","","米","6.00","","","","","","化学——检修使用"]
["21","TM20250604163744208baba","管道","PVC材质   DN25","","米","6.00","","","","","","化学——检修使用"]
["22","TM20250604163744208febb","管道","PVC材质   DN32","","米","6.00","","","","","","化学——检修使用"]
["23","TM20250604163744209369d","拷贝淋","PVC材质 （带胶套）  DN50","","个","10.00","","","","","","化学——检修使用"]
["24","TM20250604163744209b113","博斯倍福磁力泵蜗壳","SHM 65-50 PVDF-FPM，尺寸800*400*500，功率4kw，材质：PVDF","","台","2.00","","","","","","酸、碱、次氯酸钠各一台"]
["25","TM202506041637442101578","博斯倍福磁力泵蜗壳","SHM 65-50 PVDF-FPM，尺寸800*400*500，功率5.5kw，材质：PVDF","","台","1.00","","","","","","酸、碱、次氯酸钠各一台"]
["26","TM20250604163744211799c","钢骨架PE复合管","PE材质  DN300  PN16 一根6米","","根","1.00","","","","","","消防使用"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]