{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":33,"n_cols":13,"rows_kept":33,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["江苏徐矿能源股份有限公司物资供销分公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","TM20250428155047228cd54","双色水位计","TC-SMW22，ⅡB型","","组","20.00","","","","","","机务：汽包水位计使用/"]
["2","TM20250428155047230d190","乙炔减压器","AR-03K型","","个","6.00","","","","","","/"]
["3","TM20250428155047230dc2b","氧气减压器","OR-03K型","","个","6.00","","","","","","/"]
["4","TM20250428155047231331e","万向磁性表座","强磁磁力：60-80KG；原品牌：力易得","","套","3.00","","","","","","机务：检修使用/"]
["5","TM202504281550472321713","耐震压力表","YN100 0-6Mpa（带上下限三色标识）重要设备 需从上自仪、安徽天康、重庆川仪三品牌中选择","","块","2.00","","","","","","热控材料：现场检修使用/"]
["6","TM202504281550472338bda","耐震压力表","YN150 0-25Mpa（带上下限三色标识）重要设备 需从上自仪、安徽天康、重庆川仪三品牌中选择","","块","4.00","","","","","","热控材料：现场检修使用/"]
["7","TM20250428155047233e8f6","双金属温度计","0-400℃ 接头M15*1.0 揷深130mm 上自仪、安徽天康、重庆川仪三品牌之一","","支","3.00","","","","","","热控材料 高加疏水管道使用3支/"]
["8","TM20250428155047234738d","双金属温度计","0-300℃ 接头M15*1.0 揷深250mm 上自仪、安徽天康、重庆川仪三品牌之一","","支","3.00","","","","","","热控材料 高加出水管道使用3支/"]
["9","TM20250428155047235d979","管段式超声波流量计","型号:TDS-100Y 电源：DC24V 管径：DN125 连接方式:法兰连接（含配套密封垫）","","个","1.00","","","","","","热控：凝汽器雾化补水流量计更换1个/"]
["10","TM20250428155047236bcb3","膜盒压力表","YN100 0-25kpa 带上下线颜色标识 上自仪、安徽天康、重庆川仪三品牌之一","","块","5.00","","","","","","热控材料 磨煤机风压表使用5块/"]
["11","TM20250428155047237c6cf","膜盒压力表","YN100 0-40kpa 带上下线颜色标识 上自仪、安徽天康、重庆川仪三品牌之一","","块","2.00","","","","","","热控材料 磨煤机风压表使用2块/"]
["12","TM202504281550472378a9a","耐震压力表","YN100 -0.1-0.15Mpa（带上下限三色标识） 上自仪、安徽天康、重庆川仪三品牌之一","","块","3.00","","","","","","热控材料：凝结水泵出口使用3块/"]
["13","TM20250428155047238f309","耐震压力表","YN100 -0.1-0Mpa（带上下限三色标识） 上自仪、安徽天康、重庆川仪三品牌之一","","块","2.00","","","","","","热控材料：真空压力使用2块/"]
["14","TM20250428155047239248d","耐震压力表","YN100 0-2.5Kpa（带上下限三色标识）上自仪、安徽天康、重庆川仪三品牌之一","","块","2.00","","","","","","热控材料：一次风、二次风压力表更换2块/"]
["15","TM202504281550472393296","耐震压力表","YN100 0-16Kpa（带上下限三色标识）上自仪、安徽天康、重庆川仪三品牌之一","","块","2.00","","","","","","热控材料：火检冷却风使用2块/"]
["16","TM20250428155047240915d","耐震压力表","YN100 0-0.6Mpa（带上下限三色标识）上自仪、安徽天康、重庆川仪三品牌之一","","块","10.00","","","","","","热控材料：给水泵区域、磨煤机区域使用10块（发黄压力表更换）/"]
["17","TM20250428155047241c582","耐震压力表","YN100 0-1Mpa（带上下限三色标识）重要设备 需从上自仪、安徽天康、重庆川仪三品牌中选择","","块","13.00","","","","","","热控材料：给水泵区域、闭式水区域使用13块（发黄压力表更换）/"]
["18","TM202504281550472425791","耐震压力表","YN150 0-1Mpa（带上下限三色标识）重要设备 需从上自仪、安徽天康、重庆川仪三品牌中选择","","块","3.00","","","","","","热控材料：汽机十米励端油压表更换3块（发黄压力表更换）/"]
["19","TM20250428155047243de15","耐震压力表","YN100 0-1.6Mpa（带上下限三色标识）重要设备 需从上自仪、安徽天康、重庆川仪三品牌中选择","","块","4.00","","","","","","热控材料：汽机五米区域更换4块/"]
["20","TM20250428155047244e3f0","耐震压力表","YN100 0-2.5Mpa（带上下限三色标识）重要设备 需从上自仪、安徽天康、重庆川仪三品牌中选择","","块","4.00","","","","","","热控材料：低加五米区域及除氧器区域更换4块/"]
["21","TM2025042910245752009c4","导热块","φ6 R29 304材质 耐温1000℃以上 带配套固定卡箍",".","个","200.00","","","","","","热控：配合管道更换固定温度元件使用"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]