{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":48,"n_cols":13,"rows_kept":48,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["江苏新美建筑工程有限公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","TM20250402172957419407e","铲除油漆面","铲除部位名称:墙面","","m2","493.02","","","","","","详见比质比价文件"]
["2","TM2025040217295742286cc","平面块料拆除","1.拆除的基层类型：吊顶\n2.龙骨高度及底座尺寸：18cm高铁架底座600*600","","m2","192.96","","","","","","详见比质比价文件"]
["3","TM20250402172957424942c","金属门窗拆除","门窗洞口尺寸:1.5*2.1","","樘","4.00","","","","","","详见比质比价文件"]
["4","TM202504021729574242fd8","砖砌体拆除","拆除砌体的截面尺寸:1*2.4","","m3","1.44","","","","","","详见比质比价文件"]
["5","TM202504021729574251b3b","天棚面龙骨及饰面拆除","1.拆除的基层类型:吊顶\n2.龙骨及饰面种类:矿棉板","","m2","105.22","","","","","","详见比质比价文件"]
["6","TM2025040217295742661c2","平面块料拆除","1.拆除的基层类型:块料面层\n2.饰面材料种类:0.8*0.8瓷砖","","m2","64.00","","","","","","详见比质比价文件"]
["7","TM202504021729574278f06","暖气罩拆除","","","个","9.00","","","","","","详见比质比价文件"]
["8","TM20250402172957428cdd2","隔断隔墙拆除","拆除隔墙的骨架种类:玻璃","","m2","13.86","","","","","","详见比质比价文件"]
["9","TM20250402172957429941c","管内配线","1.类型:电线\n2.材质:绝缘电线\n3.规格、型号:bv-4mm","","m","72.00","","","","","","详见比质比价文件"]
["10","TM202504021729574296a24","凿（压)槽","1.名称:凿（压)槽\n2.规格:20mm\n3.填充(恢复)方式:混凝土\n4.混凝土标准:C30","","m","40.60","","","","","","详见比质比价文件"]
["11","TM20250402172957432ca3f","配管","1.名称:刚性阻燃管\n2.材质:ＫＢＪ\n3.规格:DN20\n4.配置形式:暗配","","m","28.60","","","","","","详见比质比价文件"]
["12","TM202504021729574328004","管内配线","1.类型:电线\n2.材质:绝缘电线\n3.规格、型号:bv-2.5mm","","m","245.00","","","","","","详见比质比价文件"]
["13","TM202504021729574336a1d","荧光灯","1.名称:双管荧光灯\n2.型号:吊链式 双管","","套","7.00","","","","","","详见比质比价文件"]
["14","TM202504021729574344cbf","插座","1.名称:插座\n2.材质:PVC\n3.规格:五孔插座\n4.安装方式:暗装","","个","10.00","","","","","","详见比质比价文件"]
["15","TM20250402172957435bc4d","照明开关","1.名称:开关\n2.材质:ＰＶＣ\n3.规格:单开三联开关\n4.安装方式:暗装","","个","3.00","","","","","","详见比质比价文件"]
["16","TM20250402172957435de6a","镀锌钢管","1.安装部位:地上\n2.介质:水\n3.规格、压力等级:DN32\n4.连接形式:螺纹连接","","m","13.20","","","","","","详见比质比价文件"]
["17","TM20250402172957436f83e","综合人工","1.零工","","工日","4.00","","","","","","详见比质比价文件"]
["18","TM202504021729574369b4e","砌块墙","1.砌块品种、规格、强度等级:加气混凝土砌块\n2.墙体类型:内墙\n3.砂浆强度等级:水泥砂浆M7.5","","m3","1.94","","","","","","详见比质比价文件"]
["19","TM2025040217295743711c7","墙面一般抹灰","1.墙体类型:内墙\n2.底层厚度、砂浆配合比:20mm 1:2水泥砂浆\n3.面层厚度、砂浆配合比:水泥砂浆1:2.5\n4.装饰面材料种类:水泥砂浆","","m2","393.68","","","","","","详见比质比价文件"]
["20","TM20250402172957438c11d","垫层","1.垫层材料种类、配合比、厚度:18cm厚C30混凝土","","m3","34.73","","","","","","详见比质比价文件"]
["21","TM20250402172957438f467","块料楼地面","1.结合层厚度、砂浆配合比:水泥砂浆1:3\n2.面层材料品种、规格、颜色:0.8*0.8，瓷砖价格不低于90元/m2","","m2","220.36","","","","","","详见比质比价文件"]
["22","TM2025040217295743984ad","吊顶天棚","1.吊顶形式、吊杆规格、高度:不上人\n2.龙骨材料种类、规格、中距:U型轻钢龙骨\n3.基层材料种类、规格:矿棉吸音板\n4.面层材料品种、规格:0.6*0.6\n5.压条材料种类、规格:不锈钢压条","","m2","112.78","","","","","","详见比质比价文件"]
["23","TM20250402172957439b16f","墙面喷刷涂料","1.基层类型:内墙面\n2.刮腻子要求:3遍\n3.涂料品种、喷刷遍数:乳胶漆","","m2","686.70","","","","","","详见比质比价文件"]
["24","TM20250402172957440af6f","木质门","1.门代号及洞口尺寸:1*2.4","","樘","3.00","","","","","","详见比质比价文件"]
["25","TM202504021729574403375","钢质防盗门","1.门代号及洞口尺寸:1.5*2.4\n2.门框、扇材质:空腹钢材","","樘","1.00","","","","","","详见比质比价文件"]
["26","TM202504021729574419769","楼（地）面涂膜防水","1.防水膜品种:聚氨酯防水涂料\n2.涂膜厚度、遍数:2遍 1.5mm厚","","m2","130.68","","","","","","详见比质比价文件"]
["27","TM20250402172957442ed40","墙面涂膜防水","1.防水膜品种:聚氨酯防水涂料\n2.涂膜厚度、遍数:2遍 1.5mm厚","","m2","184.80","","","","","","详见比质比价文件"]
["28","TM20250402172957442caf5","块料踢脚线","1.踢脚线高度:100mm\n2.粘贴层厚度、材料种类:20mm 1：2水泥砂浆\n3.面层材料品种、规格、颜色:瓷砖踢脚线","","m2","111.80","","","","","","详见比质比价文件"]
["29","TM20250402172957443682c","玻璃隔断","1.边框材料种类、规格:75型隔热断桥铝\n2.玻璃品种、规格、颜色:1.2mm厚双层钢化玻璃","","m2","39.40","","","","","","详见比质比价文件"]
["30","TM202504021729574439ed4","金属（塑钢、断桥）窗","1.窗代号及洞口尺寸:0.6*1\n2.框、扇材质:75型隔热断桥铝\n3.玻璃品种、厚度:双层普通玻璃 厚度6mm","","樘","2.00","","","","","","详见比质比价文件"]
["31","TM20250402172957444efd7","金属(塑钢）门","1.门代号及洞口尺寸:0.8*2.2\n2.门框、扇材质:隔热断桥铝\n3.玻璃品种、厚度:双层普通玻璃 厚度6mm","","樘","1.00","","","","","","详见比质比价文件"]
["32","TM2025040217295744428b4","金属装饰线","1.基层类型:装饰抹灰面\n2.线条材料品种、规格、颜色:铝合金方管壁厚1.5mm","","m","228.00","","","","","","详见比质比价文件"]
["33","TM202504021729574444e19","木质装饰线","1.基层类型:装饰抹灰面\n2.线条材料品种、规格、颜色:折弯工艺、木装饰线 角线 宽度 ≤50mm","","m","30.00","","","","","","详见比质比价文件"]
["34","TM2025040217295744567dd","墙面装饰板","1.龙骨材料种类、规格、中距:断面≤13cm2 木龙骨平均中距≤45cm\n2.基层材料种类、规格:木板隔墙\n3.面层材料品种、规格、颜色:木纹饰面板","","m2","184.56","","","","","","详见比质比价文件"]
["35","TM2025040217295744593c2","天棚抹灰","1.基层类型:天棚\n2.找平层砂浆厚度、配合比:三遍腻子两遍乳胶漆","","m2","468.00","","","","","","详见比质比价文件"]
["36","TM202504021729574465cdd","天棚抹灰","1.基层类型:筒型造型天棚\n2.抹灰厚度、材料种类:三遍腻子两遍乳胶漆","","m2","2.22","","","","","","详见比质比价文件"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]