{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":24,"n_cols":13,"rows_kept":24,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["江苏徐矿能源股份有限公司物资供销分公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","1515061023","压力表","0-2.5Mpa    表盘直径40","","只","10.00","","","","","","以下产品符合规格型号参数，严格执行化工标准等国家、行业强制认证规定，直发长青能源化工有限公司，货到需包含卸车，物流快递需送货上门，交货期为订单下达后15天内送达。报价备注申请付款方式。"]
["2","1515670025","耐震压力表","YN-60  量程：0-2.5MPa；结构形式：径向；精度2.5级； 螺纹连接1/4NPT，表盘直径：60mm,  壳体材质：304","","只","4.00","","","","","",""]
["3","1515700004","耐震压力表","YTN-100 　0.25MPa","","只","4.00","","","","","",""]
["4","1515702060","不锈钢耐震压力表","YFN-100,量程：0-0.6MPa，精度等级：1.6级，法兰连接，法兰：HG/T20592-2009 DN25,PN10,RF 316L C276","-长青","只","2.00","","","","","",""]
["5","1515702996","不锈钢耐震就地压力表","YN-100B 量程：0-0.1MPa；结构形式：径向无边；精度1.6；螺纹连接：M20*1.5；表盘直径：100mm 表壳材质：304","","只","1.00","","","","","",""]
["6","1515721510","耐震隔膜压力表","YTHN-150H/MF，0-1.0MPa  DN50-PN1.0  RF， HG/T20592-2009   精度1.6，隔膜材质：C-276,表壳材质：304，法兰材质：316L","","只","2.00","","","","","",""]
["7","1515721516","耐震隔膜压力表","YTHN-150H/MF，0-1.6MPa  DN50-PN1.0  RF， HG/T20592-2009   精度1.6，隔膜材质：C-276,表壳材质：304，法兰材质：316L","","只","1.00","","","","","",""]
["8","1515803001","不锈钢耐震就地压力表","YN-100 量程：0-0.16MPa 结构形式：径向无边；螺纹连接M20*1.5；精度1.6；表盘直径：100mm","","块","3.00","","","","","",""]
["9","1555100104","红外线测温仪","FLUKE 62max+   量程-30°~650°","","台","3.00","","","","","",""]
["10","1568050363","数字测振仪","VC63","","台","1.00","","","","","",""]
["11","1515805050","风压表","Y-50     量程：0-1MPa；结构形式：轴向；精度1.6；螺纹连接：1/4NPT；表盘直径：50mm  壳体材质：304","","块","5.00","","","","","",""]
["12","1515803006","不锈钢耐震就地压力表","YN-100T \t量程：0-0.6MPa；结构形式：径向；精度1.6；螺纹连接：M20*1.5；表盘直径：100mm","","块","6.00","","","","","",""]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]