{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":28,"n_cols":13,"rows_kept":28,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["江苏徐矿能源股份有限公司物资供销分公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","1751040041","手持充电式鼓风机","DLX-DCGF815 配两块7.5AH锂电池、充电器、说明书、电量显示功能、质保三年","","个","1.00","","","","","","通讯专业使用/"]
["2","1944452024","防磨盖板（护瓦）","R60，L=1400mm、材质：1Cr6Si2Mo（每个护瓦带4个压板）","","个","3.00","","","","","","机务：#1锅炉高再使用/"]
["3","1971171030","自动排气阀","外丝螺纹 DN25 材质：UPVC 压力等级：1.0MPa","","个","2.00","","","","","","中水处理次氯酸钠计量泵加装排空阀/"]
["4","1966400069","控制柜平面锁","MS818黑色锌合金把手配弯片H=23mm","","个","10.00","","","","","","热控：现场就地控制柜使用/"]
["5","1971171035","全自动排气阀","FVZF-3压力：0.9Mpa 温度：≤100℃ 304不锈钢 DN15 4分","","个","2.00","","","","","","热控：中水固液分离器浊度使用1备1/"]
["6","5217090100","角磨片JB","100*6*16","","片","20.00","","","","","",""]
["7","6012010141","钢板（鳍片）","厚：5mm  宽：107.5mm  长度：1000mm材质：12CrMoV","","片","9.00","","","","","","机务：炉本体使用"]
["8","1966400068","柜门连杆锁","HD-480","","个","10.00","","","","","","翻车机系统控制柜/"]
["9","1979760745","万向节球头","SQZL16-RS-1 M16*1.5 高强度锌合金材质 表面硬度58-64HRC 直杆正牙","","个","2.00","","","","","","热控：#1机组中主门使用/"]
["10","1979760750","万向节球头","SQZL16-RS-1 M16*1.5 高强度锌合金材质 表面硬度58-64HRC 直杆反牙","","个","2.00","","","","","","热控：#1机组中主门使用/"]
["11","1947429025","四氟垫片","22mm*18mm*2mm","","个","100.00","","","","","","热控：现场检修使用/"]
["12","1986906032","钢踏板","长*宽*高*厚3000*250*50*1.5mm","","块","6.00","","","","","","现场检修搭设脚手架使用（狭小空间使用）/"]
["13","1986900050","键坯","b*h*L  10*8*1000","","根","1.00","","","","","",""]
["14","1986900052","键坯","b*h*L  14*9*1000","","根","1.00","","","","","",""]
["15","1719110010","尖头铣","2# 425*295*235  锰钢淬火","","把","2.00","","","","","","1.2米木柄铁锹，尖头"]
["16","1719210010","方头铣","1# 420*295*245mm 锰钢淬火","","把","4.00","","","","","","1.2米木柄铁锹，方头"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]