{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":22,"n_cols":13,"rows_kept":22,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["陕西长青能源化工有限公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","TM2025040914292852003d6","打滑检测器","EXDH-III  220VAC  3A  防爆等级：ExtD A21 IP66，皮带速度范围:0.3-5.0m/s","-长青","个","1.00","","","","","","张煜计划：煤运皮带使用"]
["2","TM2025040914292852214b0","电源模块","ABL2REM24045H INPUT：100-240,2-1A OUTPUT：24V 4.5A 100W","施耐德","个","1.00","","","","","","X1402A压滤机使用"]
["3","TM202504091429285230fe0","防爆摇头扇罩","直径：80CM，材质：碳钢喷黑漆（钢筋粗1.6mm），适用于型号为FB-750型风扇，转速1450r/min,功率0.75kW,电压380V","","个","1.00","","","","","","动力班组风扇配件更换"]
["4","TM202504091429285238562","LED一体化灯管带支架","T5  1.2米，功率14W ,色温6500K, 白光","","套","100.00","","","","","","厂前区二楼视频会议室使用，光效率90Lm/w"]
["5","TM202504091429285247833","LED一体化灯管带支架","T5   0.6米，功率14W ,色温4000K,白光","","套","20.00","","","","","","厂前区二楼视频会议室使用，光效90Lm/w"]
["6","TM202504091429285256ffa","防爆接线箱","箱体：304不锈钢材质200*200*300，防爆等级ExeIICT5，防护等级IP65，底部进出线 箱体正面带不锈钢位号牌（白底黑字，宋体），带螺栓螺母垫圈等安装附件。其他要求见附件","","套","1.00","","","","","","2#合成分析小屋电源箱整改"]
["7","TM2025040914292852539dd","低压LED防爆免维护投光灯","BHJ-12V,100W,防爆等级:EXIICT6 防护等级IP66，12V/50HZ","","盏","10.00","","","","","","大检修受限空间照明使用"]
["8","TM202504091429285267b34","碎纸机","","","个","1.00","","","","","","安监部1"]
["9","TM20250409142928526117c","镀锌电缆槽盒","200*100*1.0 带盖板及安装附件 骑马 铁膨胀 七字扣","","m","210.00","","","","","","除尘器改造工程"]
["10","TM20250409142928527ffa7","铝合金防踩线槽","铝合金，银色6号，圆弧形，自带背胶","","m","3.00","","","","","","办公楼二楼会议室音响摄像头加增改造"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]