{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":50,"n_cols":13,"rows_kept":50,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["陕西长青能源化工有限公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","TM20250514093313359e37d","轴用弹性挡圈","60mm","","十只","1.00","","","","","","L1301"]
["2","TM202505140933133610d57","玻璃纤维绝缘板","宽50cm，厚0.8cm","","m","13.00","","","","","","变配电室绝缘挡鼠板"]
["3","TM20250514093313362c886","鱼缸氧气泵","AP-30A,供电方式：插电，纯铜电机，磁悬浮活塞技术，（低噪音）16W（带调节）气盘套机12米6气盘1止","","只","1.00","","","","","","食堂用"]
["4","TM202505140933133634045","消防钉","32#（钉长32mm,底部直径8.5mm,顶部直径20mm）","","个","100.00","","","","","","现场标识牌安装使用"]
["5","TM202505140933133645eaf","手推车轮内胎","4.1/3.50-4充气轮","","条","2.00","","","","","","供水班组手推车轮子更换"]
["6","TM20250514093313365416a","蓝月亮手洗专用洗衣液","净含量：1KG，不含磷，计量泵头，风清白兰","","瓶","12.00","","","","","","驿站用"]
["7","TM20250514093313365fdde","一次性双层剃须刀","软膜袋包装，含6g剃须膏","","把","20.00","","","","","","驿站用"]
["8","TM202505140933133667f3a","洗漱包","10件套：1、舒肤佳沐浴露100ml；2、海飞丝洗发水80ml；3、多芬护发素100ml；4、佳洁士牙膏40g；5、毛巾25*50cm;6、沐浴球；7、洗漱杯；8、高露洁牙刷；9、直柄梳子；10、洗漱包","","套","12.00","","","","","","驿站用"]
["9","TM20250514093313367159d","不锈钢晒被夹","长11cm宽2.5cm","","个","50.00","","","","","","食堂用"]
["10","TM202505140933133685d4c","特大号盖菜罩","材质：涤纶，尺寸：190*80，加粗骨架","","个","6.00","","","","","","食堂用"]
["11","TM20250514093313369af60","大号盖菜罩","材质：涤纶，尺寸：90*80，加粗骨架","","个","3.00","","","","","","食堂用"]
["12","TM20250514093313370624d","驱鸟器","HT-41型","","个","4.00","","","","","","厂外架空线路使用"]
["13","TM20250514093313370d0cb","实木马扎折叠便携凳","长36，宽29，高42。（不带靠背，结实耐用）","","把","10.00","","","","","","灌装工现场休息用"]
["14","TM20250514093313371bfb2","4G智能头箍","型号EQ-D6（HB) DC3.85V，防爆标志：Ex ib ⅡC T4 Gb，产品标准：Q/AKNT 001-2025","","个","2.00","","","","","","应急救援备用"]
["15","TM20250514093313372ee77","吊钩","3T","","个","1.00","","","","","","钢丝绳电葫芦吊钩，重量9KGa以上,铸钢滑轮，防脱钩，加厚钢板3-5mm"]
["16","TM2025051409331337333ca","八角弹性体","T型八角弹性块   170*81*35  八爪  聚氨酯","","件","2.00","","","","","","真空泵用"]
["17","TM20250514093313374a5d2","密封胶条","材质：橡胶，宽20mm×厚5mm，耐受温度：常温","","m","250.00","","","","","","动力装置各变配电所大门密封，要求带自粘功能，附照片"]
["18","TM202505140933133750464","PVC排水管堵头","φ110，白色","","个","1.00","","","","","","卫生间下水管堵头"]
["19","TM20250514093313376d1af","PVC扣封管托","dn20 灰色 PVC-U 带固定螺栓","","只","2.00","","","","","","回用水加药管线固定"]
["20","TM202505140933133775f5e","PVC扣封管托","dn25 灰色 PVC-U 带固定螺栓","","只","3.00","","","","","","回用水加药管线固定"]
["21","TM2025051409331337862c0","PVC扣封管托","dn32 灰色 PVC-U 带固定螺栓","","只","3.00","","","","","","回用水加药管线固定"]
["22","TM202505140933133791b1e","PVC扣封管托","dn40 灰色 PVC-U 带固定螺栓","","只","2.00","","","","","","回用水加药管线固定"]
["23","TM202505140933133797d24","弯头","DN75，PPR","","个","2.00","","","","","","驿站楼热水管线消漏（规格为dn75）"]
["24","TM20250514093313380510d","玻璃钢法兰","DN50-PN16，RF，乙烯基，HG/T21633-1991  长丝缠绕玻璃钢管道（含碳化硅防磨层厚度2.5mm）","","件","1.00","","","","","","液力搅拌泵出口总管新增压力变送器，全乙烯基一体成型"]
["25","TM202505140933133815727","O型密封圈","内径 135*3.55 mm  介质温度：220℃   材质：Aflas","","个","3.00","","","","","","P23A04A导淋更换"]
["26","TM20250514093313382fe22","反渗透专用阻垢剂","DS701","","kg","25.00","","","","","","华膜食品级/食堂用"]
["27","TM202505140933133839813","O型密封圈","内径 70*3.55  mm  介质温度：220℃  材质：Aflas","中国上正阀门/精工阀门/五洲阀门/良工阀门/立信阀门/无锡美瑞克","个","3.00","","","","","","E2110液相管线法兰维护"]
["28","TM202505140933133847839","玻璃视镜","Φ110× 30mm  材质：玻  璃   热电","","件","1.00","","","","","","给水泵循环水视镜"]
["29","TM2025051409331338411ce","防爆压紧螺母","G3/4, DN20 ,不锈钢","","只","500.00","","","","","","全厂现场防爆问题整改，304不锈钢"]
["30","TM20250514093313385d954","风向袋","荧光  防水型   1.5米长","--煤化工专用","个","10.00","","","","","","消防队用，现场更换及备用"]
["31","TM202505140933133867899","无水乙醇","C2H6OH≥96%\t工业级无水乙醇  GB/T 394.1-2008","","kg","25.00","","","","","","合成  甲醇添加剂使用"]
["32","TM20250514093313386cabb","聚氨酯万向轮","75mm带自锁","","只","4.00","","","","","","现场移动梯更换"]
["33","TM202505140933133879a8f","油封","TC 100×120×12","","件","2.00","","","","","","脱硫A氧化风机用"]
["34","TM20250514093313388caf1","六角头螺栓","M10*25全螺纹带管法兰专用螺母,M10,,35CrMo/30CrMo8.8级HG20634-1997","","件","200.00","","","","","","L1301"]
["35","TM20250514093313389769e","多功能消防水枪","65mm快插接头，流量：12L/S,无后座力，材质：铝合金/橡胶/塑料","","把","2.00","","","","","","水罐消防车及泡沫消防车各增加一个水枪"]
["36","TM202505140933133896ab3","塑封镀锌钢丝绳","6*19M-4","","kg","10.00","","","","","","供水水箱更换就地液位计揽绳，大检修"]
["37","TM202505140933133907569","高分子聚乙烯缆绳","密度：0.97-0.98g/m3  直径：φ10  16股","","m","30.00","","","","","","供水水箱更换就地液位计揽绳，大检修"]
["38","TM202505140933133919777","全螺纹螺栓带母","M16*90，带管法兰专用螺母两个M16 304 HG/T20634-2009","304","套","8.00","","","","","","动力2#脱硫液力搅拌泵出口母管增加压力变送器"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]