{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":36,"n_cols":13,"rows_kept":36,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["陕西长青能源化工有限公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","TM2025071608520030767f7","不锈钢卡套直通接头","φ8-φ8","","只","11.00","","","","","","零星工程：循环水新增非氧化性加药装置"]
["2","TM20250716085200309b406","不锈钢拷贝林卡箍","Φ48含密封圈 材质：304","","个","15.00","","","","","","脱盐水反渗透漏点消漏"]
["3","TM20250716085200309576e","不锈钢喉箍锁紧卡箍","304手拧卡箍21-38 防水防锈","","个","2.00","","","","","","零星工程：循环水新增非氧化性加药装置"]
["4","TM20250716085200310af83","不锈钢喉箍","Φ59-82","","个","30.00","","","","","","渣场  回喷洒水布带上用"]
["5","TM20250716085200311e7c8","不锈钢扎带","304不锈钢 8*2100mm 厚度0.25mm 每包100根","","包","1.00","","","","","","仪表槽盒盖板整改"]
["6","TM202507160852003123aa0","不锈钢下水器套装","110# 上口直径110mm*高80mm*下口直径45mm  带下水管1米  管径45mm","","套","2.00","","","","","","洗手盆下水管"]
["7","TM20250716085200312fe04","不锈钢丝编织软管","DN65 150Lb两端连接型式为卡套式消防水带接头（KD65） 软管和接头材质均为304 L=8米","","件","1.00","","","","","","高压清洗机"]
["8","TM2025071608520031336d6","不锈钢六角外丝直通","DN25  304","","件","4.00","","","","","","气化炉锁斗系统阀门维护"]
["9","TM202507160852003144505","不锈钢内六角丝堵","1/2NPT    材质：304  内六角外丝堵头","","个","200.00","","","","","","气化现场变送器丝堵整改"]
["10","TM20250716085200315f305","不锈钢内六角丝堵","1/2NPT    材质：304  内六角外丝堵头","","个","50.00","","","","","","动力装置变送器丝堵安装"]
["11","TM20250716085200316cd99","拷贝林卡箍密封圈","DN40  材质：三元乙丙","配套拷贝林卡箍用","件","6.00","","","","","","脱盐水反渗透漏点消漏"]
["12","TM20250716085200316913a","粘接式承口等径三通","dn40×3   S6.3    PN1.6MPa     PVC-U    灰色      GB/T 4219.1-2008","","件","5.00","","","","","","回用水氧化剂加药系统配管"]
["13","TM20250716085200317f557","异径三通","DN50*DN40(承口内径:φ63*φ50) PN16 PVC-U","","件","1.00","","","","","","循环水盐酸储罐出口配管"]
["14","TM202507160852003180674","Y型过滤器","DN32（长度221mm，管子外径40mm）\tPVC-U","上海龙猛机械","只","2.00","","","","","","回用水氧化剂加药系统配管"]
["15","TM202507160852003182e1a","玻璃视镜","尺寸：160mm（长）*35mm（宽）*24mm（厚度），两端带弧度 材质：钢化高硼硅玻璃  壳程设计压力6.3MPa 设计温度：-12-120℃","P2205密封液罐用","个","2.00","","","","","","P2205AB密封液罐，带垫片"]
["16","TM202507160852003190945","玻璃视镜","尺寸：280mm（长）*35mm（宽）*24mm（厚度），两端带弧度 材质：钢化高硼硅玻璃  壳程设计压力6.3MPa 设计温度：-12-120℃","P2208AB密封液罐，具体尺寸需要测绘","个","2.00","","","","","","P2208AB密封液罐，带垫片"]
["17","TM2025071608520032022cf","Y型过滤器","Y型过滤器,铸钢(阀体)/304(阀芯),带颈对焊法兰  DN20-150LB  RF 滤芯：过滤精度 20微米","","只","2.00","","","","","","P2205AB甲醇管线"]
["18","TM2025071608520032043dc","接水槽","长*宽*高*厚：500*200*280*2mm，304，底部开孔加接管套丝：DN20","","件","13.00","","","","","","脱盐水混床、精混及回用水机械过滤器"]
["19","TM20250716085200321d2fb","PVC钢丝透明软管","25-32(内径-外径）1\"","","m","20.00","","","","","","供水 酸碱泄露倒罐用"]
["20","TM20250716085200322aa18","塑料软管","10-14mm(内径-外径)  3/8\" 透明塑料  100米/捆","","m","10.00","","","","","","加药计量泵出口管线"]
["21","TM202507160852003229cdc","PVC钢丝软管","φ25mm","","m","5.00","","","","","","零星工程：循环水新增非氧化性加药装置"]
["22","TM20250716085200323448f","PVC线槽","25*14mm","","m","6.00","","","","","","办公楼606档案室"]
["23","TM202507160852003242e6b","下水器","304，直角，0.8米带防臭阀下水管","","个","2.00","","","","","","动力脱硫综合楼"]
["24","TM20250716085200325f8ec","UPVC翻板式底阀","4吋","","个","1.00","","","","","","中和水泵底阀更换"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]