{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":40,"n_cols":13,"rows_kept":40,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["江苏徐矿能源股份有限公司物资供销分公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","8222110005","闸阀","Z41H-150LB，DN40，150LB，RF，阀体/阀芯材质：316L，介质：湿酸气,温度：120℃","","台","1.00","","","","","","使用地点：动力湿酸气减压阀前压力表增加根部阀，直发长青能化，报价含卸车费，投标人需明确投标产品品牌及交货期，付款方式详见附件"]
["2","8222110008","闸阀","Z41H-150lbc，DN80,RF 温度≤425℃，WCB/2Cr13","","台","1.00","","","","","","使用地点：介质：氮气 常压塔塔釜氮气阀（靠塔侧），直发长青能化，报价含卸车费，投标人需明确投标产品品牌及交货期，付款方式详见附件"]
["3","8222113006","闸阀","KZ41H-150LBC DN50 RF 阀体材质：WCB/ANTI-HIC/316？ 介质：富甲醇 ，温度≤45℃","","台","1.00","","","","","","推荐品牌：\u007f中国上正阀门/精工阀门/五洲阀门/良工阀门/立信阀门/无锡美瑞克，使用地点：P2207A出口阀，直发长青能化，报价含卸车费，投标人需明确投标产品品牌及交货期，付款方式详见附件"]
["4","8222210003","闸阀","Z41Y-150LBC  DN25 RF  A105/STL","","台","2.00","","","","","","使用地点：介质：甲醇？温度≤425℃ 零星工程：精馏系统部分管线新增阀门改造，直发长青能化，报价含卸车费，投标人需明确投标产品品牌及交货期，付款方式详见附件"]
["5","8222210003","闸阀","Z41Y-150LBC  DN25 RF  A105/STL","","台","4.00","","","","","","使用地点：介质：甲醇？温度≤425℃？ 回收塔顺、返采阀LV3526B1/B2旁路阀及后手阀更换，直发长青能化，报价含卸车费，投标人需明确投标产品品牌及交货期，付款方式详见附件"]
["6","8222210010","闸阀","Z41Y-150LBC  DN100 RF  WCB/STL","","台","2.00","","","","","","使用地点：E3303B上回水导淋改造，直发长青能化，报价含卸车费，投标人需明确投标产品品牌及交货期，付款方式详见附件"]
["7","8222210010","闸阀","Z41Y-150LBC  DN100 RF  WCB/STL","","台","1.00","","","","","","使用地点：介质：工艺废水（醇含量3%左右）温度≤425℃ 工艺水泵P3511B入口阀锈蚀严重，更换，直发长青能化，报价含卸车费，投标人需明确投标产品品牌及交货期，付款方式详见附件"]
["8","8222210015","闸阀","Z41Y-150LBC  RF  DN150  WCB/STL","","台","2.00","","","","","","推荐品牌：\u007f中国上正阀门/精工阀门/五洲阀门/良工阀门/立信阀门/无锡美瑞克，使用地点：介质： 空气 温度135℃ 氧化空气改造（零星工程），直发长青能化，报价含卸车费，投标人需明确投标产品品牌及交货期，付款方式详见附件"]
["9","8222212005","闸阀","Z41Y-150LBP  DN40   RF         304/304","","台","1.00","","","","","","使用地点：介质：脱盐水 温度≤425℃ 零星工程：精馏系统部分管线新增阀门改造，直发长青能化，报价含卸车费，投标人需明确投标产品品牌及交货期，付款方式详见附件"]
["10","8222212006","闸阀","Z41Y-150LBP  DN50 RF  304/STL","","台","4.00","","","","","","推荐品牌：\u007f中国上正阀门/精工阀门/五洲阀门/良工阀门/立信阀门/无锡美瑞克，使用地点：介质：脱盐水 温度：50℃ 脱盐水导淋等维护，直发长青能化，报价含卸车费，投标人需明确投标产品品牌及交货期，付款方式详见附件"]
["11","8222212006","闸阀","Z41Y-150LBP  DN50 RF  304/STL","","台","2.00","","","","","","使用地点：介质脱盐水，常温。零星工程：预塔进料管线新增脱盐水管线改造，直发长青能化，报价含卸车费，投标人需明确投标产品品牌及交货期，付款方式详见附件"]
["12","8222218209","闸阀","Z41Y-600LBP DN80 CF8/STL RF，介质：冷凝液，温度：50℃。","","台","1.00","","","","","","推荐品牌：\u007f中国上正阀门/精工阀门/五洲阀门/良工阀门/立信阀门/无锡美瑞克，使用地点：LV2219旁路管线，直发长青能化，报价含卸车费，投标人需明确投标产品品牌及交货期，付款方式详见附件"]
["13","8222220203","闸阀","Z41Y-25C DN25 RF PN2.5Mpa  A105/STL","硫回收","台","1.00","","","","","","推荐品牌：\u007f中国上正阀门/精工阀门/五洲阀门/良工阀门/立信阀门/无锡美瑞克，使用地点：介质：脱盐水 温度104℃？除氧器二级水封罐底部导淋手阀填料压盖漏，直发长青能化，报价含卸车费，投标人需明确投标产品品牌及交货期，付款方式详见附件"]
["14","8222220204","闸阀","Z41Y-PN25 DN32 RF  A105/STL","硫回收","台","1.00","","","","","","使用地点：大修项目：污水调节池蒸汽加热阀更换为法兰连接阀门，直发长青能化，报价含卸车费，投标人需明确投标产品品牌及交货期，付款方式详见附件"]
["15","8225240007","截止阀","J41Y-150lbC DN65 RF WCB/STL，温度？，介质？","LV1404用","个","1.00","","","","","","推荐品牌：\u007f中国上正阀门/精工阀门/五洲阀门/良工阀门/立信阀门/无锡美瑞克，使用地点：介质：循环水 温度30℃K2201一段缸体冷却水阀门坏，更换阀门，直发长青能化，报价含卸车费，投标人需明确投标产品品牌及交货期，付款方式详见附件"]
["16","8225246203","截止阀","J41Y-600LbI DN25 RF WC6/STL，介质：蒸汽 温度≤420℃。","","台","2.00","","","","","","推荐品牌：\u007f中国上正阀门/精工阀门/五洲阀门/良工阀门/立信阀门/无锡美瑞克，使用地点：汽轮机轴封蒸汽PV3270前后手阀，直发长青能化，报价含卸车费，投标人需明确投标产品品牌及交货期，付款方式详见附件"]
["17","8225248209","截止阀","J41Y-600LBP DN80 CF8/STL  RF","","台","1.00","","","","","","推荐品牌：\u007f中国上正阀门/精工阀门/五洲阀门/良工阀门/立信阀门/无锡美瑞克，使用地点：介质： 冷凝液 温度45℃ LV2119旁路阀更换，直发长青能化，报价含卸车费，投标人需明确投标产品品牌及交货期，付款方式详见附件"]
["18","8225250802","截止阀","J41Y-100I DN20 温度≤540℃ 介质：过热蒸汽 密封面：FM 材质：WC6","","件","1.00","","","","","","推荐品牌：\u007f中国上正阀门/精工阀门/五洲阀门/良工阀门/立信阀门/无锡美瑞克，使用地点：开工抽气器蒸汽阀门更换，直发长青能化，报价含卸车费，投标人需明确投标产品品牌及交货期，付款方式详见附件"]
["19","8225269406","低温法兰截止阀","DIIJ41Y-150LBP DN50 RF 304/STL，介质：甲醇， ExtentedBonnet&-85℃ Impact Test，设泄压孔。","","台","1.00","","","","","","推荐品牌：\u007f中国上正阀门/精工阀门/五洲阀门/良工阀门/立信阀门/无锡美瑞克，使用地点：LV2234 旁路阀更换，直发长青能化，报价含卸车费，投标人需明确投标产品品牌及交货期，付款方式详见附件"]
["20","8225269506","低温法兰截止阀","DIIJ41Y-300LBP DN50 RF 304/STL，介质 ：丙烯 ，温度-40℃ ， ExtentedBonnet&-85℃ Impact Test，设泄压孔。","","台","1.00","","","","","","推荐品牌：\u007f中国上正阀门/精工阀门/五洲阀门/良工阀门/立信阀门/无锡美瑞克，使用地点：介质 ：丙烯 温度-40℃ 丙烯泵P3201B进口手阀阀杆弯曲，更换阀门，直发长青能化，报价含卸车费，投标人需明确投标产品品牌及交货期，付款方式详见附件"]
["21","8225269506","低温法兰截止阀","DIIJ41Y-300LBP DN50 RF 304/STL，介质 ：丙烯 ，温度-40℃ ， ExtentedBonnet&-85℃ Impact Test，设泄压孔。","","台","1.00","","","","","","推荐品牌：\u007f中国上正阀门/精工阀门/五洲阀门/良工阀门/立信阀门/无锡美瑞克，使用地点：P3201B进口手阀更换，直发长青能化，报价含卸车费，投标人需明确投标产品品牌及交货期，付款方式详见附件"]
["22","8225280006","截止阀","J41W-150LBP DN50  RF  304/304，介质：湿酸气，温度：120℃","","台","1.00","","","","","","推荐品牌：\u007f中国上正阀门/精工阀门/五洲阀门/良工阀门/立信阀门/无锡美瑞克，使用地点：LV2234旁路阀，直发长青能化，报价含卸车费，投标人需明确投标产品品牌及交货期，付款方式详见附件"]
["23","8225430403","截止阀","J61Y-1500LBPF， DN20 F22/STL  密封面堆焊硬质合金 标准号：NB/T47044-2014（电站）","","台","2.00","","","","","","推荐品牌：\u007f中国上正阀门/精工阀门/五洲阀门/良工阀门/立信阀门/无锡美瑞克，使用地点：P2101B暖泵阀，直发长青能化，报价含卸车费，投标人需明确投标产品品牌及交货期，付款方式详见附件"]
["24","8226310102","法兰旋启式止回阀","H44H-300LBC DN20 RF 3Cr13/A105,介质：蒸汽，温度：220℃。","","台","1.00","","","","","","使用地点：合成装置蒸汽疏水改造，直发长青能化，报价含卸车费，投标人需明确投标产品品牌及交货期，付款方式详见附件"]
["25","8226310103","法兰旋启式止回阀","H44H-300LBC DN25 RF 3Cr13/A105，介质：蒸汽，温度：220℃。","","台","1.00","","","","","","使用地点：合成装置蒸汽疏水改造，直发长青能化，报价含卸车费，投标人需明确投标产品品牌及交货期，付款方式详见附件"]
["26","8226314009","法兰旋启式止回阀","KH44H-150LBC DN80 RF WCB/ANTI-HIC/316，介质：富甲醇，温度：-40℃。","","台","1.00","","","","","","推荐品牌：\u007f中国上正阀门/精工阀门/五洲阀门/良工阀门/立信阀门/无锡美瑞克，使用地点：P2207A出口阀，直发长青能化，报价含卸车费，投标人需明确投标产品品牌及交货期，付款方式详见附件"]
["27","8226990020","旋启式止回阀配件","DN600-300LB 止回阀配件：阀瓣 摇臂 摇杆 现场测绘制作  材质：304","","套","1.00","","","","","","推荐品牌：\u007f中国上正阀门/精工阀门/五洲阀门/良工阀门/立信阀门/无锡美瑞克，使用地点：低温止回阀内件，直发长青能化，报价含卸车费，投标人需明确投标产品品牌及交货期，付款方式详见附件"]
["28","8289191716","外螺纹截止阀","J21W-160  PN160  Φ14","","个","5.00","","","","","","使用地点：现场压力表备用，直发长青能化，报价含卸车费，投标人需明确投标产品品牌及交货期，付款方式详见附件"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]