{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":17,"n_cols":13,"rows_kept":17,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["江苏徐矿能源股份有限公司物资供销分公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","1465020300","超高效三相异步电动机","YE3-200L1-2 30KW","","台","2.00","","","","","","P22201原水泵，电压：380V、电流：56A 接法：△ 转速：2950r/min 3C 安装：卧式，绝缘：F级，防护：IP55，防腐：WF2，带加油嘴，需供应商现场测绘或沟通确认安装尺寸。以下产品符合规格型号，直发长青能源化工有限公司，货到需包含卸车，物流快递需送货上门，交货期为订单下达后20天内送达；报价备注申请付款方式，不备注默认按集团月度排款；注意公告建议品牌厂家"]
["2","8260132203","超高效三相异步电动机","型号：YE3-100L-2，功率3KW， 电压：380V、电流：6.4A 接法：Y， 转速：2980r/min， 3C， 安装方式：卧式安装，绝缘等级：F级，防护等级：IP55，防腐等级：WF2，电机接线盒在电机尾端向前看左边，电机轴需要M10的内丝来固定风叶。","","台","1.00","","","","","","脱盐水K22201脱碳风机系列电机，需供应商测绘，沟通确认安装尺寸。"]
["3","8260139261","超高效三相异步电动机","型号：YE3-315L1-2，功率 160KW 电压：380V、电流：288.7A 接法：△， 转速：2980r/min，3C， 安装方式：卧式安装，绝缘等级：F级，防护等级：IP55，防腐等级：WF1，电机接线盒在电机尾端向前看左边，带加油嘴","脱盐水P22210除盐水泵系列电机？","台","1.00","","","","","","脱盐水P22210除盐水泵系列电机，需供应商测绘，确认安装尺寸。"]
["4","8260180475","三相异步电动机","型号：YBX3-80M2-4，功率0.75KW，电压：380V，电流：1.5A，接法：Y，转速：1400r/min，安装方式：立式安装，绝缘等级：F级，防护等级：IP55，防腐等级：WF2，防爆标志 ExdIICT6 Gb，EX 3C，","","台","1.00","","","","","","污水气浮池刮沫电机，特殊电机需供应商测绘，沟通确认安装尺寸"]
["5","8260184456","三相异步电动机","型号：YBX3-132S-4， 功率5.5KW 电压：380V、电流：14A， 接法：Y， 转速：1400r/min ，安装方式：立式安装，绝缘等级：F级，防爆标志 ExdIICT6 Gb，EX 3C，防护等级：IP66，防腐等级：WF2，","","台","1.00","","","","","","污水凉水塔风机电机，特殊电机需供应商测绘，沟通确认安装尺寸。按最新标准：GB/T 3836-2021，满足防爆ExdIICT6 Gb"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]