{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":21,"n_cols":13,"rows_kept":21,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["江苏省矿业工程集团有限公司安装分公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","TM202509291447006310683","加压泵","Q=7.5m3/h，H=23m 功率1.5KW，电流4.2A；电压380V（不锈钢）","Q=7.5m3/h，H=23m 功率1.5KW，电流4.2A；电压380V（不锈钢）","台","1.00","","","","","","按项目部规定时间送货"]
["2","TM20250929144700633e6c2","加压水泵控制箱","户内型，IP44，不锈钢304，F2防腐型","户内型，IP44，不锈钢304，F2防腐型","台","1.00","","","","","","由加压泵厂家配供，联系现场按项目部规定时间送货"]
["3","TM202509291447006342fd2","打印机","1.5kva/900w，待机60分钟 220V","1.5kva/900w，待机60分钟 220V","台","1.00","","","","","","按项目部规定时间送货"]
["4","TM2025092914470063564eb","循环水泵","1、型号：流量2.5m3/h,扬程15m组合件\n2、功率：150W 电压220V","1、型号：流量2.5m3/h,扬程15m组合件\n2、功率：150W 电压220V","台","1.00","","","","","","按项目部规定时间送货"]
["5","TM20250929144700636b8c0","手提式潜水泵","Q=12m3/h，H=8m 电压220V","Q=12m3/h，H=8m 电压220V","台","2.00","","","","","","按项目部规定时间送货"]
["6","TM20250929144700637afb2","空调器","8匹工业级空调\n制冷量22.4kw，功率6.5kw，风量≥6000m3/h  电压380V","8匹工业级空调\n制冷量22.4kw，功率6.5kw，风量≥6000m3/h  电压380V","台","2.00","","","","","","包含安装，按项目部规定时间送货"]
["7","TM20250929144700637f989","空调器","3匹智能空调\n制冷量7.5kw，功率2.2kw，风量≥700m3/h  电压220V","3匹智能空调\n制冷量7.5kw，功率2.2kw，风量≥700m3/h  电压220V","台","3.00","","","","","","包含安装，按项目部规定时间送货"]
["8","TM202509291447006382059","除湿机","15L/D移动式除湿器 电压220V","15L/D移动式除湿器 电压220","台","1.00","","","","","","按项目部规定时间送货"]
["9","TM202509291447006396439","轴流通风机","T40型风机，风量1130m3/h，风压100PA,W=0.18KW   电压220V（外设防虫网）","T40型风机，风量1130m3/h，风压100PA,W=0.18KW   电压220V（外设防虫网）","台","3.00","","","","","","按项目部规定时间送货"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]