{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":35,"n_cols":13,"rows_kept":35,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["陕西长青能源化工有限公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","TM20250514093013824d551","防爆按钮","BA8030 红色 一常开一常闭 ExdIIC IP65 AC220/380 10A 开孔安装尺寸：φ30mm","","个","2.00","","","","","","动力B锅炉点火系统就地控制柜检修"]
["2","TM20250514093013826b8e7","防爆按钮","BA8030 绿色 一常开一常闭 ExdIIC IP65 AC220/380 10A 开孔安装尺寸：φ30mm","","个","2.00","","","","","","动力B锅炉点火系统就地控制柜检修"]
["3","TM202505140930138272178","接触器模块","IEC/EN 60947？ 24VDC 0.5A","伊顿电气","只","12.00","","","","","","气化P1302A/B/C高压煤浆泵使用"]
["4","TM202505140930138284c2d","安全继电器","PILZ PNOZ X2.8P","施耐德","只","1.00","","","","","","关键备件补库，动力硫酸包装机就地控制柜检修"]
["5","TM202505140930138281954","防爆铠装电缆密封接头","Exd II CT4，IP65 NPT 1″  黄铜镀镍","","个","20.00","","","","","","净化现场格兰头整改"]
["6","TM202505140930138290cb3","防爆电缆密封接头","黄铜镀镍 M27*1.5（M） EXdII CT4","-长青","个","6.00","","","","","","动力3台锅炉一次风总门电动执行机构检修"]
["7","TM2025051409301383016f0","防爆电缆密封接头","黄铜镀镍 M50*1.5（M） EXdII CT4","-长青","个","10.00","","","","","","2#合成分析仪表预处理箱用"]
["8","TM202505140930138318781","电加热器","GY2-220/2 220V 2kW","","只","4.00","","","","","","气化P1302B/C高压煤浆泵使用？ 要求：需配垫子"]
["9","TM202505140930138317b9d","粘捕式挂墙灭蚊灯","椭圆形，长约38.5cm，宽26cm，厚约14cm，20W《加大荧光双管》旗舰版 珍珠白 ，含配件荧光双灯管，紫蓝光引诱，免打孔安装；附赠20张粘蝇纸。","","只","6.00","","","","","","食堂用"]
["10","TM202505140930138322ed9","防爆强光工作灯电池","MATRIX,NP12-12,12V ,12Ah,密封可充电电池","","块","6.00","","","","","","更换消防队备用防爆照明灯电池"]
["11","TM20250514093013833f61d","PZ30配电箱塑料面板","12回路","","个","1.00","","","","","","污水循环水泵房配电箱更换"]
["12","TM20250514093013834f008","金属电缆桥架垂直上弯道","宽200mm*高100mm* 厚2mm（ 附盖板及其连接件、螺丝） ，材质：铝合金","","件","3.00","","","","","","煤运火炬P3801使用，零星工程"]
["13","TM20250514093013834cd8d","金属电缆桥架垂直右弯道","宽200mm*高100mm* 厚2mm（ 附盖板及其连接件、螺丝） ，材质：铝合金","","件","1.00","","","","","","煤运火炬P3801使用，零星工程"]
["14","TM202505140930138353554","金属电缆桥架垂直左弯道","宽200mm*高100mm* 厚2mm（ 附盖板及其连接件、螺丝） ，材质：铝合金","","件","3.00","","","","","","煤运火炬P3801使用，零星工程"]
["15","TM20250514093013836246a","槽式直通电缆桥架","宽50mm×高25mm* 厚1.5mm（ 附盖板及其连接件、螺丝）长2米 ，材质：铝合金","","m","12.00","","","","","","脱硝取样电缆槽盒整改"]
["16","TM202505140930138370979","槽式直通电缆桥架","宽200mm*高100mm*厚2.0mm（附盖板及其连接件、螺丝），材质：铝合金，附件材质：304","","m","108.00","","","","","","煤运火炬P3801使用，零星工程"]
["17","TM20250514093013837c8fb","防水防尘防腐电源箱插座","16A-6h/220-250V IP66 2P+E/50+60HZ","浙江欧佩柯斯电器有限公司","个","2.00","","","","","","动力1442AQ动力箱使用，重要设备后续维修用零配件，必须保证与原有采购项目一致性的物资。附照片"]
["18","TM20250514093013838a193","黄油嘴（带防尘帽）","PT1/8 铜镀镍  1/8转10*1接头","","个","200.00","","","","","","煤储运计划：滚筒加油嘴更换"]
["19","TM2025051409301383904d0","黄油嘴（带防尘帽）","PT1/8 铜镀镍  1/8转8*1接头","","个","100.00","","","","","","煤储运计划：滚筒加油嘴更换"]
["20","TM202505140930138403965","防爆铠装电缆密封接头","Exd II CT4，IP65 M32*1.5（M) 黄铜镀镍","","个","2.00","","","","","","PV2227前手阀改电动阀（本安电缆）"]
["21","TM202505140930138413169","压延微晶板","300*200*14mm","","m2","15.00","","","","","","煤储运计划：汽车卸煤库受煤槽耐磨板修复"]
["22","TM20250514093013841598e","不锈钢电缆槽盒","材质：304  100*50*1.2mm 带配套槽盒盖","","m","12.00","","","","","","PV2227前手阀改电动阀（本安电缆）"]
["23","TM202505140930138425919","防爆接线箱","下进下出。进线电缆为ZR-YJV-8.7/10kV-3*95mm2，线缆外径62mm；出线电缆为ZR-YJV-0.6/1kV-3*35+1*25mm2，线缆外径30mm 。内置连接端子L1、L2、L3、N （L1L2L3镀锡铜排电流不小于200A），确保各接线端子绝缘良好，固定牢靠，端子两侧具有固定线缆的镀锡螺栓；","防爆等级为Exd IICT4 Gb，防腐等级为WF1；接线端子距箱体下边不小于700mm，距箱体上边不小于300mm，格兰头紧固线缆需密封良好。箱体：500*300*700mm,材质：304，带4个支撑高700mm。颜色：喷银灰漆。","个","1.00","","","","","","任小平计划 ：K2301B高压变更低压电机改造，厂家现场测绘。"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]