{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":24,"n_cols":13,"rows_kept":24,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["江苏徐矿能源股份有限公司物资供销分公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","TM20251027103535868ec7d","航空插头","WS16-4 4针4芯 （公头+六角螺母母座）","","个","4.00","","","","","","热控：#1吸收塔PH计连接线改造使用/"]
["2","TM202510271035358700955","BVR电线","10mm2 黄绿双色 100米/卷","","卷","1.00","","","","","","电气：现场接地整改/"]
["3","TM202510271035358705d6e","BVR电线","6mm2 黄绿双色 100米/卷","","卷","5030.00","","","","","","电气：现场接地整改/"]
["4","TM202510271035358711f50","PLC电源模块","IC693PWR321","","块","1.00","","","","","","（IC693PWR321 GE 90-30）工业废水PLC事故备件"]
["5","TM20251027103535872a142","控制器","IC693CPU372 GE","","块","1.00","","","","","","（IC693CPU372 GE 90-30）工业废水PLC事故备件"]
["6","TM20251027103535873d0b8","压力继电器","型号 D501/7DK 设定值： 0.03MPa 触点容量： AC 220V 6A（阻性）","","个","1.00","","","","","","东方汽轮机有限公司机修分厂顶轴装置D200X-601000A配套使用（热控材料：#1机顶轴油泵入口压力低报警使用1个/"]
["7","TM202510271035358746176","压力继电器","型号 D501/7DK 设定值： 0.35MPa 触点容量： AC 220V 6A（阻性）","","个","2.00","","","","","","东方汽轮机有限公司机修分厂顶轴装置D200X-601000A配套使用（热控材料：#1机顶轴油泵入口压力低报警使用1个/"]
["8","TM2025102710353587470b1","干簧管液位计","磁翻板捆绑式远传变送器 量程0-0.5m 输出4-20mA","","根","2.00","","","","","","尿素储罐、溶解罐使用"]
["9","TM20251027103535875d92c","温控器","台达 DTA4848R0 AC100-240V 50/60HZ 5VA","","块","2.00","","","","","","热控：#1机氢气干燥器使用1备1/"]
["10","TM20251027103535876872b","电极式液位计","PS-5S 电极材质：316 电极长度：1.5米（可裁剪）","","套","1.00","","","","","","热控：中水PAM加药箱事故备件/"]
["11","TM20251027103535877938f","消防水带接头","KN65","","只","2.00","","","","","","潜水泵使用"]
["12","TM202510271035358784d51","风向标杆","不锈钢管高2m 直径38mm，壁厚：7mm,法兰式底座，标杆头带360°轴承","","根","2.00","","","","","","合理化建议使用（风带，带杆及万向轮底座)"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]