{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":57,"n_cols":13,"rows_kept":57,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["陕西长青能源化工有限公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","TM2025040308495846533d5","不锈钢螺母","14mm","","十只","10.00","","","","","","M14,304 HG20634-1997，合成净化现场防静电跨接线、接地线螺母生锈更换（卢帅）"]
["2","TM20250403084958467e28b","不锈钢螺母","16mm","","十只","10.00","","","","","","M16,304 HG20634-1997，合成净化现场防静电跨接线、接地线螺母生锈更换（卢帅）"]
["3","TM20250403084958468eb44","不锈钢螺母","18mm   304","","十只","10.00","","","","","","M18,304 HG20634-1997，合成净化现场防静电跨接线、接地线螺母生锈更换（卢帅）"]
["4","TM20250403084958469b79f","弹性圆柱销","\"M12×￠18×95（一套含4个弹性套Φ35×Φ18×9、1个弹簧垫、1个钢圈、1个螺母和1个螺栓，总长度95mm）\"        \t35钢/聚氨酯     \tGB/T4323-2002","","套","16.00","","","","","","K23A01AB"]
["5","TM20250403084958470b326","锥形刻度量杯","10mL","","只","10.00","","","","","","岗位耗材"]
["6","TM20250403084958470155d","钢制柱型暖气片","钢二柱50*25型 600中心距*16柱 平顶","","组","1.00","","","","","","污水二楼暖气片更换"]
["7","TM202504030849584717f04","丝杆","14*1000","","根","2.00","","","","","","非标法兰螺栓加工 材质：35CrMoA HG/T20634-2009"]
["8","TM2025040308495847222ac","丝杆","16*1000","","根","2.00","","","","","","非标法兰螺栓加工 材质：35CrMoA HG/T20634-2009"]
["9","TM202504030849584731431","洁厕剂","3.8L/桶 4桶/件","","件","20.00","","","","","","保洁用"]
["10","TM20250403084958473d3d5","硅油","500ml进口二甲基硅油道康宁","","瓶","6.00","","","","","","仪修楼检修压力表用"]
["11","TM20250403084958474c3c5","水桶","不锈钢手提水桶16L","","个","3.00","","","","","","供水班组用"]
["12","TM202504030849584755012","可移动登高梯","平台离地面高度1.5米，四级登高，万向轮 铁质涂白漆","","架","5.00","","","","","","气化  开关阀门使用"]
["13","TM20250403084958476d280","不锈钢Ex防爆标识","30mm*20mm*0.5mm，带背胶","","个","10.00","","","","","","防爆行车整改用"]
["14","TM202504030849584774440","救生圈","外径：760MM     内径：460MM  外：聚乙烯塑料 内：聚氨酯泡沫  4.3KG成人型  （橙色）","","个","8.00","","","","","","供水  现场水池悬挂"]
["15","TM202504030849584776140","防爆丁字井盖勾","长度500mm,直径10mm,手柄宽度200mm,钩子头部宽度45mm","","个","2.00","","","","","","净化  现场使用  铜制"]
["16","TM20250403084958478f186","手持高音喇叭","MEGAPHONE    UM-2  8PCS  DC:12V  HL-POWER","","件","1.00","","","","","","渣场使用"]
["17","TM202504030849584785e68","AX-2100空气呼吸器面罩保护套","35cm*27cm，阻燃、防水、防尘面料","","个","50.00","","","","","","消防队应急救援"]
["18","TM20250403084958479a7c1","烟灰柱","120*25*25cm,不锈钢","","个","2.00","","","","","",""]
["19","TM2025040308495847985ac","苍蝇拍","长45cm 拍宽11.5cm","","件","10.00","","","","","","各装置现场灭虫用"]
["20","TM20250403084958480b422","实心橡胶轮胎三角垫","长300*宽280*高250mm   带塑料把手","","个","10.00","","","","","","动力  液氨卸车、灰库放灰以及高压清洗机使用"]
["21","TM202504030849584810786","消防救援三角架","多功能便携消防救援三角架  伸缩起重电动葫芦支架，全套1800磅，双向自锁手摇绞盘     材质：铝合金","","件","2.00","","","","","","供水班组下泵用"]
["22","TM202504030849584818652","水果包装盒","尺寸：175*135*76MM 颜色：透明 型号：500M 材质：PET","","个","1200.00","","","","","","食堂用"]
["23","TM202504030849584821361","塑料雨衣","","","套","310.00","","","","","","大检修使用"]
["24","TM20250403084958482ec38","合页","75MM","","件","50.00","","","","","","用于更换灭火器箱损坏合页，带螺丝"]
["25","TM202504030849584837672","O型密封圈","78*3.1 GB 1235-76 全氟醚 介质：脱盐水 压力：16MPa 适用温度≤250℃","","个","1.00","","","","","","给水泵最小流量阀用（西安泵阀）"]
["26","TM202504030849584834b27","O型密封圈","90*3.1 GB 1235-76 全氟醚 介质：脱盐水 压力：16MPa 适用温度≤250℃","","个","2.00","","","","","","给水泵最小流量阀用（西安泵阀）"]
["27","TM202504030849584846c61","O型密封圈","115*3.1 GB 1235-76 全氟醚 介质：脱盐水 压力：16MPa 适用温度≤250℃","","个","1.00","","","","","","给水泵最小流量阀用（西安泵阀）"]
["28","TM202504030849584844ce2","O型密封圈","200*5.7 GB 1235-76 全氟醚 介质：脱盐水 压力：16MPa 适用温度≤250℃","","个","1.00","","","","","","给水泵最小流量阀用（西安泵阀）"]
["29","TM20250403084958485ac37","弹性块","T85,橡胶","P409E","个","1.00","","","","","","脱硫氨水泵用"]
["30","TM202504030849584853e6f","密封胶条","材质：氟橡胶，宽52mm×厚9mm，耐受温度：250℃，耐腐蚀","","m","15.00","","","","","","动力3台锅炉布袋除尘器外置旁路阀检修"]
["31","TM2025040308495848606d9","吊环","M24，材质为合金钢","","个","6.00","","","","","","动力发电机本体使用"]
["32","TM2025040308495848666d5","六角头螺栓","M12*30 全螺纹带管法兰专用螺母,M12,,304 HG20634-1997","","套","15.00","","","","","","动力布袋除尘器外置旁路阀检修"]
["33","TM2025040308495848730d8","活节螺栓","M20，总长130mm， 材质：304，带螺母1个","","套","2.00","","","","","","P2204A 具体尺寸现场测绘 配带螺栓、螺母、销子"]
["34","TM20250403084958487d53f","防尘服","防粉尘，防静电、防岩棉  连帽分体","附图","套","4.00","","","","","","汽车卸煤库采样"]
["35","TM20250403084958488712e","开关保护贴（单个）","保护贴内径：86mm*86mm，上边宽56，其他边宽：30mm，白色不透明亚克力，定制附样品","-长青","个","230.00","","","","","","6S材料"]
["36","TM202504030849584880396","开关保护贴（二联）","保护贴内径：173mm*86mm，上边宽56，其他边宽：30mm， 白色不透明亚克力，定制附样品","-长青","个","15.00","","","","","","6S材料"]
["37","TM202504030849584895170","O型密封圈","300*5.7，材质：氟硅橡胶 标准：GB1235","","件","2.00","","","","","","K2201循环气压缩机"]
["38","TM20250403084958490f852","O型密封圈","20*2.4  橡胶II-2  GB/T3452.1-2005","","个","12.00","","","","","","K2201循环气压缩机"]
["39","TM2025040308495849003e3","密封胶条","材质：氟橡胶，宽52mm×厚9mm，耐受温度：250℃，耐腐蚀","","m","15.00","","","","","","仪表大修第2项，动力一台锅炉外置旁路阀检修"]
["40","TM202504030849584910c1a","玻璃视镜","Φ115*19，材质：玻璃  液流封视镜，耐高温  热电","","个","6.00","","","","","","液硫视镜处密封面检查、垫片更换（6处）"]
["41","TM2025040308495849189f1","F型扳手","铜制 250mm  开口：25mm 直径：14mm,","","只","8.00","","","","","","净化  现场使用"]
["42","TM202504030849584924434","移液枪枪头","5ml、短大口 口径12mm、长度98mm    300支/包","","包","2.00","","","","","","瑞宁移液枪替换枪头"]
["43","TM20250403084958492bf15","碳钢标准腐蚀挂片","I型 50mm*25mm*2mm","","片","70.00","","","","","","循环水腐蚀速率监测"]
["44","TM20250403084958492315a","镀锌六角内接头","32mm 1_1/4\"","","个","5.00","","","","","","季度计划"]
["45","TM202504030849584932e37","粘接式承口直通接头","dn140*10.3  S6.3  PN1.6MPa  PVC-U 灰色  GB/T 4219.2-2008","","个","1.00","","","","","","加药管线配管"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]