{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["询价单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价单","index":0,"n_rows":25,"n_cols":13,"rows_kept":25,"cut":false,"hidden":false,"merged":[[1,0,1,3],[1,6,1,11],[2,0,2,3],[2,6,2,11],[3,0,3,3],[3,6,3,11],[4,0,4,3],[4,6,4,11],[0,0,0,11]],"flags":["formulas_cached_only"]}
["江苏徐矿能源股份有限公司物资供销分公司物资采购询（报）价单"]
["报价单位（公章或合同章）:",{"$nulls":5},"询价部门："]
["联系人:",{"$nulls":5},"联系方式："]
["传真:",{"$nulls":5},"报价截止日期："]
["供应商编码:"]
["序号","物资编码","物资名称","规格","型号","计量单位","数量","交货期","主机","含税单价（元）","总价（元）","品牌","备注"]
["1","2499040267","骨架油封","115*140*12","","件","2.00","","","","","","直发阿克苏电厂，机务：斗提机减速机使用"]
["2","2499022054","O型圈","Ф54.5*3.0  氟橡胶","","个","12.00","","","","","","直发阿克苏电厂，机务：蓄能器底部与连接盘使用，φ54.5*3氟橡胶（温度：≥250℃，压力：10Mpa，介质：油）"]
["3","6012010054","蓄能器油管O型圈","40*4","","个","12.00","","","","","","直发阿克苏电厂，机务：蓄能器使用，φ40*4氟橡胶（温度：≥250°，压力：10Mpa，介质：油）"]
["4","6012010055","直径18油管O型圈","20*2.5","","个","12.00","","","","","","直发阿克苏电厂，机务：蓄能器油管使用，φ20*2.5氟橡胶（温度：≥250℃，压力：10Mpa，介质：油）"]
["5","6012010057","高压油管O型圈","37.5*3.55","","个","12.00","","","","","","直发阿克苏电厂，机务：磨煤机蓄能器使用，φ37.5*3.55氟橡胶（温度：≥250℃，压力：10Mpa，介质：油）"]
["6","TM202505161647287107742","O型圈","内φ38*2.5 氟橡胶（压力10Mpa，温度≥350，介质：水）","/阿克苏电厂","个","4.00","","","","","","定冷水泵，B修计划，需求日期：2025年7月份/"]
["7","TM20250516164728711ea6b","O型圈","内φ70*3.5 氟橡胶（压力10Mpa，温度≥350，介质：水）","/阿克苏电厂","个","4.00","","","","","","定冷水泵，B修计划，需求日期：2025年7月份/"]
["8","TM202505161647287124dda","O型圈","内φ39*3 氟橡胶（压力10Mpa，温度≥350，介质：水）","/阿克苏电厂","个","2.00","","","","","","定冷水泵，B修计划，需求日期：2025年7月份/"]
["9","TM2025051616472871301a6","机械密封","HM74D/60SGB-1101556 泵型号：40DT-B35(34)B、型式：离心式、流量：30m3/h、扬程：40m、壳体/叶轮材质：合金材料GLH-5、密封型式：机械密封、轴功率9.8千瓦、粒度≤1.6mm、转速1460R/MIN；效率40％；必须气蚀余量5.3M；原品牌：石家庄工业泵厂有限公司","/阿克苏电厂","套","2.00","","","","","","机务：1-1、1-2石膏排出泵使用/"]
["10","TM2025051616472871406e8","O型圈","φ460*10mm 材质：氟橡胶（温度：≥250°，压力：10Mpa，介质：水）","/阿克苏电厂","个","8.00","","","","","","给水泵工作油冷油器端面，B修计划，需求日期：2025年7月份/"]
["11","TM20250516164728715762f","堵阀自密封","φ610*554*56*45°","","个","2.00","","","","","","直发阿克苏电厂，机务：再热器使用/"]
["12","TM202505161647287169f6c","O型圈","φ68*3氟橡胶（温度：≥250℃，压力：10Mpa，介质：油）","","个","12.00","","","","","","直发阿克苏电厂，机务：磨煤机蓄能器使用/"]
["13","TM202505161647287175a37","O型圈","Φ20*2.5、氟橡胶（温度：≥250°，压力：10Mpa，介质：油）","","个","64.00","","","","","","直发阿克苏电厂，机务：挤渣门油管使用（1个油缸使用2个）/"]
["","合计","","","","","","","","","","",""]
["注：A、报价：无税单价（运费、装卸费出卖人承担）。"]
[" B、质量标准：国标、行业标准、企标，并注明标准号。非标产品以双方认可的图纸、协议等为准。"]
[" C、请务必填写完整、清晰，否则报价无效，修改处签章。"]
[" D、 “报价单”视为合同附件，具有法律效应。"]
[" E、付款方式：电子承兑。"]